| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
Architecture specific functions used with the LWIP examples
LightWeight IP TCP/IP Stack

## Detailed Description

## Functions
void | msDelay (uint32_t ms)
| Delay for the specified number of milliSeconds.

## Typedef Documentation

typedef uint8_t u8_t

Definition at line 43 of file cc.h.

## Function Documentation

void msDelay | ( | uint32_t | ms | ) |

Delay for the specified number of milliSeconds.

Parameters

  ms | : Time in milliSeconds to delay

Returns
  Nothing

Note
  For standalone systems. This function will block for the specified number of milliSconds. For RTOS based systems, this function will delay the task by the specified number of milliSeconds.

Delay for the specified number of milliSeconds.

Millisecond Delay function.

Parameters

  ms | : Delay period in milliseconds

Returns
  None Delay for the specified number of milliSeconds. This function is used by LWIP stack in stand-alone configuration

Delay for the specified number of milliSeconds.

Millisecond Delay function.

Delay function.

Parameters

  ms | : Number of milliSeconds to delay

Returns
  Nothing Needed for some functions, do not use prior to FreeRTOS running

Definition at line 300 of file lpc43xx_systick.c.