| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - r -

- R1_ADDRESS_ERROR : lpc_sdmmc.h
- R1_APP_CMD : lpc_sdmmc.h
- R1_BLOCK_LEN_ERROR : lpc_sdmmc.h
- R1_CARD_ECC_DISABLED : lpc_sdmmc.h
- R1_CARD_ECC_FAILED : lpc_sdmmc.h
- R1_CARD_IS_LOCKED : lpc_sdmmc.h
- R1_CC_ERROR : lpc_sdmmc.h
- R1_CID_CSD_OVERWRITE : lpc_sdmmc.h
- R1_COM_CRC_ERROR : lpc_sdmmc.h
- R1_CURRENT_STATE : lpc_sdmmc.h
- R1_ERASE_PARAM : lpc_sdmmc.h
- R1_ERASE_RESET : lpc_sdmmc.h
- R1_ERASE_SEQ_ERROR : lpc_sdmmc.h
- R1_ERROR : lpc_sdmmc.h
- R1_ILLEGAL_COMMAND : lpc_sdmmc.h
- R1_LOCK_UNLOCK_FAILED : lpc_sdmmc.h
- R1_OUT_OF_RANGE : lpc_sdmmc.h
- R1_OVERRUN : lpc_sdmmc.h
- R1_READY_FOR_DATA : lpc_sdmmc.h
- R1_STATUS : lpc_sdmmc.h
- R1_UNDERRUN : lpc_sdmmc.h
- R1_WP_ERASE_SKIP : lpc_sdmmc.h
- R1_WP_VIOLATION : lpc_sdmmc.h
- RAMDISK_LOCATION : lpc43xx_dualcore_config.h
- RAMDISK_SIZE : lpc43xx_dualcore_config.h
- RAND() : mrt.c
- RAND_LCG_PARAM_A : lib_math.h
- RAND_LCG_PARAM_B : lib_math.h
- RAND_LCG_PARAM_M : lib_math.h
- RAND_NBR : lib_math.h
- RAND_SEED_INIT_VAL : lib_math.h
- rb : uart_17xx_40xx.c , uart_18xx_43xx.c
- RB_INDH : ring_buffer.c
- RB_INDT : ring_buffer.c
- RB_SIGNATURE : ring_buffer.h
- RB_VHEAD : ring_buffer.h
- RB_VTAIL : ring_buffer.h
- RDES_AFM : enet_001.h
- RDES_CE : enet_001.h
- RDES_DE : enet_001.h
- RDES_DINT : enet_001.h
- RDES_DRE : enet_001.h
- RDES_ENH_BS1 : enet_001.h
- RDES_ENH_BS2 : enet_001.h
- RDES_ENH_IPCSB : enet_001.h
- RDES_ENH_IPHE : enet_001.h
- RDES_ENH_IPPL : enet_001.h
- RDES_ENH_IPPLE : enet_001.h
- RDES_ENH_IPV4 : enet_001.h
- RDES_ENH_IPV6 : enet_001.h
- RDES_ENH_MTMSK : enet_001.h
- RDES_ENH_RCH : enet_001.h
- RDES_ENH_RER : enet_001.h
- RDES_ES : enet_001.h
- RDES_ESA : enet_001.h
- RDES_FLMSK : enet_001.h
- RDES_FS : enet_001.h
- RDES_FT : enet_001.h
- RDES_LC : enet_001.h
- RDES_LE : enet_001.h
- RDES_LS : enet_001.h
- RDES_NORM_BS1 : enet_001.h
- RDES_NORM_BS2 : enet_001.h
- RDES_NORM_RCH : enet_001.h
- RDES_NORM_RER : enet_001.h
- RDES_OE : enet_001.h
- RDES_OWN : enet_001.h
- RDES_RE : enet_001.h
- RDES_RWT : enet_001.h
- RDES_SAF : enet_001.h
- RDES_TSA : enet_001.h
- RDES_VLAN : enet_001.h
- RDET_CLR : pinint_8xx.h
- readBlocks() : sdmmc_17xx_40xx.c
- readExtIDEntry() : can_001.c
- ReadFlash() : norflash.c
- readStdIDEntry() : can_001.c
- readTSCReg() : board_keil_mcb_18574357.c
- readWriteTSC2046() : board_ea_devkit_17884088.c , board_hitex_eva_18504350.c
- receiveCompleted : uart.c
- recv_buf : uart_rom.c
- RED : lpc_colors.h
- RED_COLORS : lpc_colors.h
- RED_LED_PORT_BIT : board_nxp_xpresso_812.c
- red_off_time : sct_user.h
- red_on_time : sct_user.h
- REDMASK : lpc_colors.h
- REDSHIFT : lpc_colors.h
- Refresh : AudioClassCommon.h
- RelAddr : MassStorageClassCommon.h
- ReleaseNumber : StdDescriptors.h
- reload_cross_timeout : sct_fsm.h
- reload_jumpTimeout : sct_fsm.h
- reload_maxcount : sct_fsm.h
- reload_pedestrian_stop : sct_fsm.h
- reload_pedestrian_walk : sct_fsm.h
- reload_toggleTimeout : sct_fsm.h
- reload_turn_red_off : sct_fsm.h
- reload_turn_red_on : sct_fsm.h
- reload_turn_yellow_off : sct_fsm.h
- reload_turn_yellow_on : sct_fsm.h
- reload_val : cpu_bsp_lpc43xx_m0.c
- REMAP_BOOT_LOADER_MODE : sysctl_11xx.h , sysctl_13xx.h , sysctl_17xx_40xx.h , syscon_8xx.h
- REMAP_USER_FLASH_MODE : sysctl_11xx.h , sysctl_13xx.h , sysctl_17xx_40xx.h , syscon_8xx.h
- REMAP_USER_RAM_MODE : sysctl_11xx.h , sysctl_13xx.h , syscon_8xx.h
- remote_ip_addr : dualcore_emwin.c
- REMOTE_NDIS_DF_CONNECTION_ORIENTED : RNDISClassCommon.h
- REMOTE_NDIS_DF_CONNECTIONLESS : RNDISClassCommon.h
- REMOTE_NDIS_HALT_MSG : RNDISClassCommon.h
- REMOTE_NDIS_INDICATE_STATUS_MSG : RNDISClassCommon.h
- REMOTE_NDIS_INITIALIZE_CMPLT : RNDISClassCommon.h
- REMOTE_NDIS_INITIALIZE_MSG : RNDISClassCommon.h
- REMOTE_NDIS_KEEPALIVE_CMPLT : RNDISClassCommon.h
- REMOTE_NDIS_KEEPALIVE_MSG : RNDISClassCommon.h
- REMOTE_NDIS_MEDIA_STATE_CONNECTED : RNDISClassCommon.h
- REMOTE_NDIS_MEDIA_STATE_DISCONNECTED : RNDISClassCommon.h
- REMOTE_NDIS_MEDIUM_802_3 : RNDISClassCommon.h
- REMOTE_NDIS_PACKET_ALL_FUNCTIONAL : RNDISClassCommon.h
- REMOTE_NDIS_PACKET_ALL_LOCAL : RNDISClassCommon.h
- REMOTE_NDIS_PACKET_ALL_MULTICAST : RNDISClassCommon.h
- REMOTE_NDIS_PACKET_BROADCAST : RNDISClassCommon.h
- REMOTE_NDIS_PACKET_DIRECTED : RNDISClassCommon.h
- REMOTE_NDIS_PACKET_FUNCTIONAL : RNDISClassCommon.h
- REMOTE_NDIS_PACKET_GROUP : RNDISClassCommon.h
- REMOTE_NDIS_PACKET_MAC_FRAME : RNDISClassCommon.h
- REMOTE_NDIS_PACKET_MSG : RNDISClassCommon.h
- REMOTE_NDIS_PACKET_MULTICAST : RNDISClassCommon.h
- REMOTE_NDIS_PACKET_PROMISCUOUS : RNDISClassCommon.h
- REMOTE_NDIS_PACKET_SMT : RNDISClassCommon.h
- REMOTE_NDIS_PACKET_SOURCE_ROUTING : RNDISClassCommon.h
- REMOTE_NDIS_QUERY_CMPLT : RNDISClassCommon.h
- REMOTE_NDIS_QUERY_MSG : RNDISClassCommon.h
- REMOTE_NDIS_RESET_CMPLT : RNDISClassCommon.h
- REMOTE_NDIS_RESET_MSG : RNDISClassCommon.h
- REMOTE_NDIS_SET_CMPLT : RNDISClassCommon.h
- REMOTE_NDIS_SET_MSG : RNDISClassCommon.h
- REMOTE_NDIS_STATUS_FAILURE : RNDISClassCommon.h
- REMOTE_NDIS_STATUS_INVALID_DATA : RNDISClassCommon.h
- REMOTE_NDIS_STATUS_MEDIA_CONNECT : RNDISClassCommon.h
- REMOTE_NDIS_STATUS_MEDIA_DISCONNECT : RNDISClassCommon.h
- REMOTE_NDIS_STATUS_NOT_SUPPORTED : RNDISClassCommon.h
- REMOTE_NDIS_STATUS_SUCCESS : RNDISClassCommon.h
- REMOTE_NDIS_VERSION_MAJOR : RNDISClassCommon.h
- REMOTE_NDIS_VERSION_MINOR : RNDISClassCommon.h
- REMOTE_WAKEUP_CONNECTED : OHCI.h
- REMOTE_WAKEUP_ENABLE : OHCI.h
- Removable : MassStorageClassCommon.h
- remove_chain() : ff.c
- RemoveEndpoint() : OHCI.h
- RemoveQueueHead() : EHCI.h
- ReplyNormalMessage() : can.c
- ReplyRemoteMessage() : can.c
- REQ_ClearFeature : StdRequestType.h
- REQ_GetConfiguration : StdRequestType.h
- REQ_GetDescriptor : StdRequestType.h
- REQ_GetInterface : StdRequestType.h
- REQ_GetStatus : StdRequestType.h
- REQ_SetAddress : StdRequestType.h
- REQ_SetConfiguration : StdRequestType.h
- REQ_SetDescriptor : StdRequestType.h
- REQ_SetFeature : StdRequestType.h
- REQ_SetInterface : StdRequestType.h
- REQ_SynchFrame : StdRequestType.h
- REQDIR_DEVICETOHOST : StdRequestType.h
- REQDIR_HOSTTODEVICE : StdRequestType.h
- REQREC_DEVICE : StdRequestType.h
- REQREC_ENDPOINT : StdRequestType.h
- REQREC_INTERFACE : StdRequestType.h
- REQREC_OTHER : StdRequestType.h
- REQTYPE_CLASS : StdRequestType.h
- REQTYPE_STANDARD : StdRequestType.h
- REQTYPE_VENDOR : StdRequestType.h
- REQUEST_CLASS : usbd.h
- REQUEST_DEVICE_TO_HOST : usbd.h
- REQUEST_HOST_TO_DEVICE : usbd.h
- REQUEST_RESERVED : usbd.h
- REQUEST_STANDARD : usbd.h
- REQUEST_TO_DEVICE : usbd.h
- REQUEST_TO_ENDPOINT : usbd.h
- REQUEST_TO_INTERFACE : usbd.h
- REQUEST_TO_OTHER : usbd.h
- REQUEST_VENDOR : usbd.h
- RequestId : RNDISClassCommon.h
- RES_ERROR : diskio.h
- RES_NOTRDY : diskio.h
- RES_OK : diskio.h
- RES_PARERR : diskio.h
- RES_WRPRT : diskio.h
- Reserved : HIDClassCommon.h , MassStorageClassCommon.h , RNDISClassCommon.h , StdDescriptors.h
- reserved : EHCI.h
- Reserved2 : MassStorageClassCommon.h
- reserved2 : EHCI.h , OHCI.h
- Reserved3 : MassStorageClassCommon.h
- reserved3 : OHCI.h
- Reserved4 : MassStorageClassCommon.h
- RESERVED_ALIGN : chip_clocks.h
- RESERVED_ALIGNB : chip_clocks.h
- RESERVED_ALIGNC : chip_clocks.h
- RESERVED_ALIGND : chip_clocks.h
- RESERVED_ALIGNE : chip_clocks.h
- RESERVED_ALIGNF : chip_clocks.h
- RESERVED_ALIGNG : chip_clocks.h
- RESERVED_ALIGNH : chip_clocks.h
- ReservedSectorCnt : fatutil.c
- RESERVEDSECTORCNT : fatutil.h
- RESET : lpc_types.h
- RESET_ACMP : sysctl_11xx.h , syscon_8xx.h
- RESET_ADC0 : sysctl_11xx.h
- RESET_CAN0 : sysctl_11xx.h
- RESET_DAC0 : sysctl_11xx.h
- RESET_FLASH : syscon_8xx.h
- RESET_GPIO : syscon_8xx.h
- RESET_I2C : syscon_8xx.h
- RESET_I2C0 : sysctl_11xx.h , sysctl_13xx.h
- RESET_MRT : syscon_8xx.h
- RESET_SCT : syscon_8xx.h
- RESET_SPI0 : syscon_8xx.h
- RESET_SPI1 : syscon_8xx.h
- RESET_SSP0 : sysctl_11xx.h , sysctl_13xx.h
- RESET_SSP1 : sysctl_11xx.h , sysctl_13xx.h
- RESET_TIMER0_16 : sysctl_11xx.h
- RESET_TIMER0_32 : sysctl_11xx.h
- RESET_TIMER1_16 : sysctl_11xx.h
- RESET_TIMER1_32 : sysctl_11xx.h
- RESET_UART0 : sysctl_11xx.h
- RESET_UARTFBRG : syscon_8xx.h
- RESET_USART0 : syscon_8xx.h
- RESET_USART1 : syscon_8xx.h
- RESET_USART2 : syscon_8xx.h
- RESET_WKT : syscon_8xx.h
- ResetISR() : cr_startup_8xx.c , cr_startup_lpc17xx40xx.c , cr_freertos_startup_lpc18xx43xx.c , cr_startup_lpc18xx43xx.c , cr_startup_lpc43xx_m0.c , cr_freertos_startup_lpc18xx43xx.c , cr_ucos_iii_startup_lpc18xx43xx.c , cr_startup_lpc18xx43xx.c , cr_startup_lpc43xx_m0.c , cr_freertos_startup_lpc17xx40xx.c , cr_ucos_iii_startup_lpc17xx40xx.c , cr_freertos_startup_lpc11xx.c , cr_startup_lpc11xx.c , cr_freertos_startup_lpc8xx.c , cr_freertos_startup_lpc13xx.c , cr_startup_lpc13xx.c
- ResponseCode : MassStorageClassCommon.h
- ResponseDataFormat : MassStorageClassCommon.h
- result : dfuutil_programming_iflash_algorithm.c , i2c.c
- RESUME_DETECT_INTERRUPT : OHCI.h
- RET_SLAVE_BUSY : i2c_001.h
- RET_SLAVE_IDLE : i2c_001.h
- RET_SLAVE_RX : i2c_001.h
- RET_SLAVE_TX : i2c_001.h
- RevisionID : MassStorageClassCommon.h
- RGU_ADC0_RST : rgu_18xx_43xx.h
- RGU_ADC1_RST : rgu_18xx_43xx.h
- RGU_BUS_RST : rgu_18xx_43xx.h
- RGU_CAN0_RST : rgu_18xx_43xx.h
- RGU_CAN1_RST : rgu_18xx_43xx.h
- RGU_CORE_RST : rgu_18xx_43xx.h
- RGU_CREG_RST : rgu_18xx_43xx.h
- RGU_DAC_RST : rgu_18xx_43xx.h
- RGU_DMA_RST : rgu_18xx_43xx.h
- RGU_EEPROM_RST : rgu_18xx_43xx.h
- RGU_EMC_RST : rgu_18xx_43xx.h
- RGU_ETHERNET_RST : rgu_18xx_43xx.h
- RGU_FLASHA_RST : rgu_18xx_43xx.h
- RGU_FLASHB_RST : rgu_18xx_43xx.h
- RGU_GPIO_RST : rgu_18xx_43xx.h
- RGU_I2C0_RST : rgu_18xx_43xx.h
- RGU_I2C1_RST : rgu_18xx_43xx.h
- RGU_I2S_RST : rgu_18xx_43xx.h
- RGU_LAST_RST : rgu_18xx_43xx.h
- RGU_LCD_RST : rgu_18xx_43xx.h
- RGU_M3_RST : rgu_18xx_43xx.h
- RGU_MASTER_RST : rgu_18xx_43xx.h
- RGU_MOTOCONPWM_RST : rgu_18xx_43xx.h
- RGU_PERIPH_RST : rgu_18xx_43xx.h
- RGU_QEI_RST : rgu_18xx_43xx.h
- RGU_RITIMER_RST : rgu_18xx_43xx.h
- RGU_SCT_RST : rgu_18xx_43xx.h
- RGU_SCU_RST : rgu_18xx_43xx.h
- RGU_SDIO_RST : rgu_18xx_43xx.h
- RGU_SPIFI_RST : rgu_18xx_43xx.h
- RGU_SSP0_RST : rgu_18xx_43xx.h
- RGU_SSP1_RST : rgu_18xx_43xx.h
- RGU_TIMER0_RST : rgu_18xx_43xx.h
- RGU_TIMER1_RST : rgu_18xx_43xx.h
- RGU_TIMER2_RST : rgu_18xx_43xx.h
- RGU_TIMER3_RST : rgu_18xx_43xx.h
- RGU_UART0_RST : rgu_18xx_43xx.h
- RGU_UART1_RST : rgu_18xx_43xx.h
- RGU_UART2_RST : rgu_18xx_43xx.h
- RGU_UART3_RST : rgu_18xx_43xx.h
- RGU_USB0_RST : rgu_18xx_43xx.h
- RGU_USB1_RST : rgu_18xx_43xx.h
- RGU_WWDT_RST : rgu_18xx_43xx.h
- RIGHT : lpc_swim_image.h
- ring_buff_get_status() : i2s.c
- ring_buffer : i2s.c
- RingBuffer_Flush() : ring_buffer.h
- RingBuffer_GetCount() : ring_buffer.h
- RingBuffer_GetFree() : ring_buffer.h
- RingBuffer_GetSize() : ring_buffer.h
- RingBuffer_Init() : ring_buffer.c , ring_buffer.h
- RingBuffer_Insert() : ring_buffer.c , ring_buffer.h
- RingBuffer_InsertMult() : ring_buffer.c , ring_buffer.h
- RingBuffer_IsEmpty() : ring_buffer.h
- RingBuffer_IsFull() : ring_buffer.h
- RingBuffer_IsValid : ring_buffer.h
- RingBuffer_Pop() : ring_buffer.c , ring_buffer.h
- RingBuffer_PopMult() : ring_buffer.h , ring_buffer.c
- RIT_CTRL_ENBR : ritimer_001.h
- RIT_CTRL_ENCLR : ritimer_001.h
- RIT_CTRL_INT : ritimer_001.h
- RIT_CTRL_TEN : ritimer_001.h
- RIT_IRQHandler() : ritimer.c , cpu_bsp_lpc43xx_m0.c
- RITENCLR : cpu_bsp_lpc43xx_m0.c
- RITINT : cpu_bsp_lpc43xx_m0.c
- RNDIS_ClassNotifications_t : RNDISClassCommon.h
- RNDIS_ClassRequests_t : RNDISClassCommon.h
- RNDIS_Data_Initialized : RNDISClassCommon.h
- RNDIS_Device_ConfigureEndpoints() : RNDISClassDevice.c , RNDISClassDevice.h
- RNDIS_Device_IsPacketReceived() : RNDISClassDevice.h , RNDISClassDevice.c
- RNDIS_Device_ProcessControlRequest() : RNDISClassDevice.c , RNDISClassDevice.h
- RNDIS_Device_ProcessNDISQuery() : RNDISClassDevice.c
- RNDIS_Device_ProcessNDISSet() : RNDISClassDevice.c
- RNDIS_Device_ProcessRNDISControlMessage() : RNDISClassDevice.c
- RNDIS_Device_ReadPacket() : RNDISClassDevice.h , RNDISClassDevice.c
- RNDIS_Device_SendPacket() : RNDISClassDevice.c , RNDISClassDevice.h
- RNDIS_Device_USBTask() : RNDISClassDevice.h , RNDISClassDevice.c
- RNDIS_ENUMERROR_InvalidConfigDescriptor : RNDISClassHost.h
- RNDIS_ENUMERROR_NoCompatibleInterfaceFound : RNDISClassHost.h
- RNDIS_ENUMERROR_NoError : RNDISClassHost.h
- RNDIS_ENUMERROR_PipeConfigurationFailed : RNDISClassHost.h
- RNDIS_ERROR_LOGICAL_CMD_FAILED : RNDISClassCommon.h
- RNDIS_GetEncapsulatedResponse() : RNDISClassHost.c
- RNDIS_Host_ConfigurePipes() : RNDISClassHost.c , RNDISClassHost.h
- RNDIS_Host_EnumerationFailure_ErrorCodes_t : RNDISClassHost.h
- RNDIS_Host_InitializeDevice() : RNDISClassHost.h , RNDISClassHost.c
- RNDIS_Host_IsPacketReceived() : RNDISClassHost.c , RNDISClassHost.h
- RNDIS_Host_QueryRNDISProperty() : RNDISClassHost.h , RNDISClassHost.c
- RNDIS_Host_ReadPacket() : RNDISClassHost.h , RNDISClassHost.c
- RNDIS_Host_SendKeepAlive() : RNDISClassHost.h , RNDISClassHost.c
- RNDIS_Host_SendPacket() : RNDISClassHost.h , RNDISClassHost.c
- RNDIS_Host_SetRNDISProperty() : RNDISClassHost.h , RNDISClassHost.c
- RNDIS_Host_USBTask() : RNDISClassHost.h
- RNDIS_Initialize_Complete_t : RNDISClassCommon.h
- RNDIS_Initialize_Message_t : RNDISClassCommon.h
- RNDIS_Initialized : RNDISClassCommon.h
- RNDIS_KeepAlive_Complete_t : RNDISClassCommon.h
- RNDIS_KeepAlive_Message_t : RNDISClassCommon.h
- RNDIS_MESSAGE_BUFFER_SIZE : RNDISClassCommon.h
- RNDIS_Message_Header_t : RNDISClassCommon.h
- RNDIS_NOTIF_ResponseAvailable : RNDISClassCommon.h
- RNDIS_Packet_Message_t : RNDISClassCommon.h
- RNDIS_Query_Complete_t : RNDISClassCommon.h
- RNDIS_Query_Message_t : RNDISClassCommon.h
- RNDIS_REQ_GetEncapsulatedResponse : RNDISClassCommon.h
- RNDIS_REQ_SendEncapsulatedCommand : RNDISClassCommon.h
- RNDIS_Reset_Complete_t : RNDISClassCommon.h
- RNDIS_SendEncapsulatedCommand() : RNDISClassHost.c
- RNDIS_Set_Complete_t : RNDISClassCommon.h
- RNDIS_Set_Message_t : RNDISClassCommon.h
- RNDIS_States_t : RNDISClassCommon.h
- RNDIS_Uninitialized : RNDISClassCommon.h
- rng : mrt.c
- RNG_MULTI : mrt.c
- rom8x16_bits : lpc_rom8x16.c
- rom8x16_width : lpc_rom8x16.c
- rom8x8_bits : lpc_rom8x8.c
- rom8x8_width : lpc_rom8x8.c
- ROM_DRIVER_BASE : ccand_11xx.h , romapi_8xx.h
- ROM_FUNCTION_TABLE_PTR_ADDR : usbd_rom_api.h
- ROM_USBD_PTR : usbd_rom_api.h
- ROOTENTRIES : fatutil.h
- RootEntries : fatutil.c , fatutil.h
- RST : swm_8xx.h
- RTC_ALARM_TIME : app_pmc_states.c
- RTC_AMR_CIIR_BITMASK : rtc_001.h
- RTC_AMR_CIIR_IMDOM : rtc_001.h
- RTC_AMR_CIIR_IMDOW : rtc_001.h
- RTC_AMR_CIIR_IMDOY : rtc_001.h
- RTC_AMR_CIIR_IMHOUR : rtc_001.h
- RTC_AMR_CIIR_IMMIN : rtc_001.h
- RTC_AMR_CIIR_IMMON : rtc_001.h
- RTC_AMR_CIIR_IMSEC : rtc_001.h
- RTC_AMR_CIIR_IMYEAR : rtc_001.h
- RTC_AUX_RTC_OSCF : rtc_001.h
- RTC_AUXEN_RTC_OSCFEN : rtc_001.h
- RTC_CALIB_DIR_BACKWARD : rtc_001.h
- RTC_CALIB_DIR_FORWARD : rtc_001.h
- RTC_CALIBRATION_CALVAL_MASK : rtc_001.h
- RTC_CALIBRATION_LIBDIR : rtc_001.h
- RTC_CALIBRATION_MAX : rtc_001.h
- RTC_CCR_BITMASK : rtc_001.h
- RTC_CCR_CCALEN : rtc_001.h
- RTC_CCR_CLKEN : rtc_001.h
- RTC_CCR_CTCRST : rtc_001.h
- RTC_CTIME0_DOW_MASK : rtc_001.h
- RTC_CTIME0_HOURS_MASK : rtc_001.h
- RTC_CTIME0_MINUTES_MASK : rtc_001.h
- RTC_CTIME0_SECONDS_MASK : rtc_001.h
- RTC_CTIME1_DOM_MASK : rtc_001.h
- RTC_CTIME1_MONTH_MASK : rtc_001.h
- RTC_CTIME1_YEAR_MASK : rtc_001.h
- RTC_CTIME2_DOY_MASK : rtc_001.h
- RTC_DAYOFMONTH_MAX : rtc_001.h
- RTC_DAYOFMONTH_MIN : rtc_001.h
- RTC_DAYOFWEEK_MAX : rtc_001.h
- RTC_DAYOFYEAR_MAX : rtc_001.h
- RTC_DAYOFYEAR_MIN : rtc_001.h
- RTC_DOM_MASK : rtc_001.h
- RTC_DOW_MASK : rtc_001.h
- RTC_DOY_MASK : rtc_001.h
- rtc_gettime() : rtc.c , rtc.h
- RTC_HOUR_MASK : rtc_001.h
- RTC_HOUR_MAX : rtc_001.h
- RTC_ILR_BITMASK : rtc_001.h
- rtc_initialize() : fsmci_cfg.h , rtc.c , rtc.h , fsmci_cfg.h , fsusb_cfg.h
- RTC_INT_ALARM : rtc_001.h
- RTC_INT_COUNTER_INCREASE : rtc_001.h
- RTC_IRL_RTCALF : rtc_001.h
- RTC_IRL_RTCCIF : rtc_001.h
- RTC_IRQHandler() : cr_startup_lpc43xx_m0.c , rtc.c , rtc_ev.c , cr_startup_lpc43xx_m0.c , rtc.c
- RTC_MIN_MASK : rtc_001.h
- RTC_MINUTE_MAX : rtc_001.h
- RTC_MONTH_MASK : rtc_001.h
- RTC_MONTH_MAX : rtc_001.h
- RTC_MONTH_MIN : rtc_001.h
- RTC_SEC_MASK : rtc_001.h
- RTC_SECOND_MAX : rtc_001.h
- rtc_settime() : rtc.h , rtc.c
- RTC_TIMETYPE_DAYOFMONTH : rtc_001.h
- RTC_TIMETYPE_DAYOFWEEK : rtc_001.h
- RTC_TIMETYPE_DAYOFYEAR : rtc_001.h
- RTC_TIMETYPE_HOUR : rtc_001.h
- RTC_TIMETYPE_LAST : rtc_001.h
- RTC_TIMETYPE_MINUTE : rtc_001.h
- RTC_TIMETYPE_MONTH : rtc_001.h
- RTC_TIMETYPE_SECOND : rtc_001.h
- RTC_TIMETYPE_YEAR : rtc_001.h
- RTC_YEAR_MASK : rtc_001.h
- RTC_YEAR_MAX : rtc_001.h
- RW_TEST : spi.c
- Rx_Buf : ssp.c
- rx_callback() : uart_rom.c
- RX_MODE_BUF_FULL : uartd_8xx.h
- RX_MODE_CRLF_RECVD : uartd_8xx.h
- RX_MODE_LF_RECVD : uartd_8xx.h
- rxAvail : enet.c
- RXBRK : usart_002.h
- RxBuf : spi.c
- RxBuf0 : uart.c
- RxBuf1 : uart.c
- RxBufCnt1 : uart.c
- rxbuff : uart.c
- RXBuffer : enet.c
- rxConsumeIdx : enet.c
- RXDescs : enet.c
- RxENDPKT_INT : HAL_LPC17xx.h
- rxFill : enet.c
- rxGet : enet.c
- RXIDLE : usart_002.h
- RXINTGROUP : lpc17xx_40xx_emac.c
- RXNOISE : usart_002.h
- RXNOISE_ERR_EN : uartd_8xx.h
- RXNOISE_INT : usart_002.h
- rxNumDescs : enet.c
- RXRDY : usart_002.h
- RXRDY_INT : usart_002.h
- rxring : uart.c