| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros
Main definitions
Audio Output Device | Audio Output Device

## Detailed Description

## Macros
#define | LEDMASK_USB_NOTREADY LEDS_LED1
| LED definitions.
#define | LEDMASK_USB_ENUMERATING (LEDS_LED2 | LEDS_LED3)
#define | LEDMASK_USB_READY (LEDS_LED2 | LEDS_LED4)
#define | LEDMASK_USB_ERROR (LEDS_LED1 | LEDS_LED3)
#define | LEDMASK_USB_NOTREADY LEDS_LED1
| LED definitions.
#define | LEDMASK_USB_ENUMERATING (LEDS_LED2 | LEDS_LED3)
#define | LEDMASK_USB_READY (LEDS_LED2 | LEDS_LED4)
#define | LEDMASK_USB_ERROR (LEDS_LED1 | LEDS_LED3)

## Macro Definition Documentation

#define LEDMASK_USB_ENUMERATING (LEDS_LED2 | LEDS_LED3)

LED mask for the library LED driver, to indicate that the USB interface is enumerating.

Definition at line 94 of file AudioOutput.h.

#define LEDMASK_USB_ENUMERATING (LEDS_LED2 | LEDS_LED3)

LED mask for the library LED driver, to indicate that the USB interface is enumerating.

Definition at line 97 of file AudioOutput.h.

#define LEDMASK_USB_ERROR (LEDS_LED1 | LEDS_LED3)

LED mask for the library LED driver, to indicate that an error has occurred in the USB interface.

Definition at line 100 of file AudioOutput.h.

#define LEDMASK_USB_ERROR (LEDS_LED1 | LEDS_LED3)

LED mask for the library LED driver, to indicate that an error has occurred in the USB interface.

Definition at line 103 of file AudioOutput.h.

#define LEDMASK_USB_NOTREADY LEDS_LED1

LED definitions.

LED mask for the library LED driver, to indicate that the USB interface is not ready.

Definition at line 91 of file AudioOutput.h.

#define LEDMASK_USB_NOTREADY LEDS_LED1

LED definitions.

LED mask for the library LED driver, to indicate that the USB interface is not ready.

Definition at line 94 of file AudioOutput.h.

#define LEDMASK_USB_READY (LEDS_LED2 | LEDS_LED4)

LED mask for the library LED driver, to indicate that the USB interface is ready.

Definition at line 97 of file AudioOutput.h.

#define LEDMASK_USB_READY (LEDS_LED2 | LEDS_LED4)

LED mask for the library LED driver, to indicate that the USB interface is ready.

Definition at line 100 of file AudioOutput.h.