| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Structures | Macros | Functions
scu_18xx_43xx.h File Reference

Go to the source code of this file.

## Data Structures
struct | LPC_SCU_T
| System Control Unit register block. More...

## Macros
#define | SCU_MODE_MODE_INACT (0x0 << 3)
#define | SCU_MODE_MODE_PULLDOWN (0x1 << 3)
#define | SCU_MODE_MODE_PULLUP (0x2 << 3)
#define | SCU_MODE_MODE_REPEATER (0x3 << 3)
#define | SCU_MODE_HIGHSPEEDSLEW_EN (0x1 << 5)
#define | SCU_MODE_INBUFF_EN (0x1 << 6)
#define | SCU_MODE_ZIF_DIS (0x1 << 7)
#define | SCU_MODE_4MA_DRIVESTR (0x0 << 8)
#define | SCU_MODE_8MA_DRIVESTR (0x1 << 8)
#define | SCU_MODE_14MA_DRIVESTR (0x2 << 8)
#define | SCU_MODE_20MA_DRIVESTR (0x3 << 8)
#define | SCU_MODE_FUNC0 0x0
#define | SCU_MODE_FUNC1 0x1
#define | SCU_MODE_FUNC2 0x2
#define | SCU_MODE_FUNC3 0x3
#define | SCU_MODE_FUNC4 0x4
#define | SCU_MODE_FUNC5 0x5
#define | SCU_MODE_FUNC6 0x6
#define | SCU_MODE_FUNC7 0x7
#define | SCU_PINIO_FAST (SCU_MODE_MODE_PULLUP | SCU_MODE_HIGHSPEEDSLEW_EN | SCU_MODE_INBUFF_EN | SCU_MODE_ZIF_DIS)
#define | MD_PUP (0x0 << 3) /** Disable pull-down and pull-up resistor at resistor at pad */
#define | MD_BUK (0x1 << 3) /** Enable pull-down resistor at pad */
#define | MD_PLN (0x2 << 3) /** Enable pull-up resistor at pad */
#define | MD_PDN (0x3 << 3) /** Enable pull-down and pull-up resistor at resistor at pad (repeater mode) */
#define | MD_EHS (0x1 << 5) /** Enable fast slew rate */
#define | MD_EZI (0x1 << 6) /** Input buffer enable */
#define | MD_ZI (0x1 << 7) /** Disable input glitch filter */
#define | MD_EHD0 (0x1 << 8) /** EHD driver strength low bit */
#define | MD_EHD1 (0x1 << 8) /** EHD driver strength high bit */
#define | MD_PLN_FAST (MD_PLN | MD_EZI | MD_ZI | MD_EHS)
#define | I2C0_STANDARD_FAST_MODE (1 << 3 | 1 << 11) /** Pin configuration for STANDARD/FAST mode I2C */
#define | I2C0_FAST_MODE_PLUS (2 << 1 | 1 << 3 | 1 << 7 | 1 << 10 | 1 << 11) /** Pin configuration for Fast-mode Plus I2C */
#define | FUNC0 0x0 /** Pin function 0 */
#define | FUNC1 0x1 /** Pin function 1 */
#define | FUNC2 0x2 /** Pin function 2 */
#define | FUNC3 0x3 /** Pin function 3 */
#define | FUNC4 0x4 /** Pin function 4 */
#define | FUNC5 0x5 /** Pin function 5 */
#define | FUNC6 0x6 /** Pin function 6 */
#define | FUNC7 0x7 /** Pin function 7 */
#define | PORT_OFFSET 0x80 /** Port offset definition */
#define | PIN_OFFSET 0x04 /** Pin offset definition */
#define | LPC_SCU_PIN(LPC_SCU_BASE, po, pi) (*(volatile int *) ((LPC_SCU_BASE) + ((po) * 0x80) + ((pi) * 0x4))
#define | LPC_SCU_CLK(LPC_SCU_BASE, c) (*(volatile int *) ((LPC_SCU_BASE) +0xC00 + ((c) * 0x4)))

## Functions
STATIC INLINE void | Chip_SCU_PinMuxSet (uint8_t port, uint8_t pin, uint16_t modefunc)
| Sets I/O Control pin mux.
STATIC INLINE void | Chip_SCU_PinMux (uint8_t port, uint8_t pin, uint16_t mode, uint8_t func)
| Configure pin function.
STATIC INLINE void | Chip_SCU_ClockPinMuxSet (uint8_t clknum, uint16_t modefunc)
| Configure clock pin function (pins SFSCLKx)
STATIC INLINE void | Chip_SCU_ClockPinMux (uint8_t clknum, uint16_t mode, uint8_t func)
| Configure clock pin function (pins SFSCLKx)
void | Chip_SCU_GPIOIntPinSel (uint8_t PortSel, uint8_t PortNum, uint8_t PinNum)
| GPIO Interrupt Pin Select.
STATIC INLINE void | Chip_SCU_I2C0PinConfig (uint32_t I2C0Mode)
| I2C Pin Configuration.
STATIC INLINE void | Chip_SCU_ADC_Channel_Config (uint32_t ADC_ID, uint8_t channel)
| ADC Pin Configuration.
STATIC INLINE void | Chip_SCU_DAC_Analog_Config (void)
| DAC Pin Configuration.