| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Hitex 4350 evaluation boards

Documentation links
Hitex LPC1850 and LPC4350 evaluation boards

Jumper configuration
The image below shows the default jumper configuration used for all Hitex 4350 examples. Use this configuration for the examples unless an example alters this default setting in it's description.
Hitex 1850 and 4350 boards use the same default jumper setting.

Board recovery using the ISP pin
If the board's FLASH can no longer be programmed, the image in FLASH may be corrupt. To recover the board, the board's boot source can be altered by changing the boot source on jumpers BOOT1 via BOOT4.