| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Enumerations | Functions
aes_18xx_43xx.h File Reference

Go to the source code of this file.

## Enumerations
enum | CHIP_AES_OP_MODE_T { CHIP_AES_API_CMD_ENCODE_ECB, CHIP_AES_API_CMD_DECODE_ECB, CHIP_AES_API_CMD_ENCODE_CBC, CHIP_AES_API_CMD_DECODE_CBC }
| AES Engine operation mode. More...

## Functions
void | Chip_AES_Init (void)
| Initialize the AES Engine function.
uint32_t | Chip_AES_SetMode (CHIP_AES_OP_MODE_T AesMode)
| Set operation mode in AES Engine.
void | Chip_AES_LoadKey (uint32_t keyNum)
| Load 128-bit AES user key in AES Engine.
void | Chip_AES_LoadKeyRNG (void)
| Load randomly generated key in AES engine.
void | Chip_AES_LoadKeySW (uint8_t *pKey)
| Load 128-bit AES software defined user key in AES Engine.
void | Chip_AES_LoadIV_SW (uint8_t *pVector)
| Load 128-bit AES initialization vector in AES Engine.
void | Chip_AES_LoadIV_IC (void)
| Load IC specific 128-bit AES initialization vector in AES Engine.
uint32_t | Chip_AES_Operate (uint8_t *pDatOut, uint8_t *pDatIn, uint32_t Size)
| Operate AES Engine.
uint32_t | Chip_AES_ProgramKey (uint32_t KeyNum, uint8_t *pKey)
| Program 128-bit AES Key in OTP.