| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
IP_CAN_STD_ID_Entry_T Struct Reference
IP: CAN register block and driver

## Detailed Description

Standard ID Entry structure.

Definition at line 686 of file can_001.h.

`#include "can_001.h"`

## Data Fields
uint8_t | CtrlNo
uint8_t | Disable
uint16_t | ID_11

## Field Documentation

uint8_t CtrlNo

Controller Number: 0 for CAN1 and 1 for CAN2

Definition at line 687 of file can_001.h.

uint8_t Disable

0(ENABLE)/1(DISABLE): Response On/Off dynamically

Definition at line 688 of file can_001.h.

uint16_t ID_11

Standard ID, should be 11-bit value

Definition at line 689 of file can_001.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/can_001.h