| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages

### - c -

- CalculateCountOfClusters() : fatutil.c , fatutil.h
- calibrateTSC2046() : board_hitex_eva_18504350.c , board_ea_devkit_17884088.c
- CALLBACK_Audio_Device_GetSetEndpointProperty() : AudioInput.c , AudioClassDevice.h , AudioOutput.c
- CALLBACK_Audio_Device_GetSetInterfaceProperty() : AudioInput.c
- CALLBACK_HAL_GetISOBufferAddress() : AudioOutput.c , AudioInput.c
- CALLBACK_HID_Device_CreateHIDReport() : Mouse.c , HIDClassDevice.h , GenericHID.c , Keyboard.c
- CALLBACK_HID_Device_ProcessHIDReport() : HIDClassDevice.h , GenericHID.c , Keyboard.c , Mouse.c
- CALLBACK_HIDParser_FilterHIDReportItem() : HIDParser.h , KeyboardHost.c
- CALLBACK_MS_Device_SCSICommandReceived() : MassStorageClassDevice.h , usbmsdev.c , usbmsdev.h , MassStorage_ucosiii.c , MassStorage.c
- CALLBACK_USB_GetDescriptor() : Descriptors.c , Device.h , Descriptors.c , Descriptors.h
- CALLBACK_UsbdCdc_Register_ControlInterfaceDescriptor() : usbd_cdc.h , UsbRom.h
- CALLBACK_UsbdCdc_Register_DataInEndpointNumber() : usbd_cdc.h , UsbRom.h
- CALLBACK_UsbdCdc_Register_DataInEndpointSize() : usbd_cdc.h , UsbRom.h
- CALLBACK_UsbdCdc_Register_DataInterfaceDescriptor() : usbd_cdc.h , UsbRom.h
- CALLBACK_UsbdCdc_Register_DataOutEndpointNumber() : usbd_cdc.h , UsbRom.h
- CALLBACK_UsbdCdc_Register_DataOutEndpointSize() : usbd_cdc.h , UsbRom.h
- CALLBACK_UsbdCdc_Register_LineCoding() : usbd_cdc.h , UsbRom.h
- CALLBACK_UsbdCdc_Register_NotificationEndpointNumber() : usbd_cdc.h , UsbRom.h
- CALLBACK_UsbdHid_IsReportChanged() : usbd_hid.h , UsbRom.h
- CALLBACK_UsbdHid_Register_InterfaceDescriptor() : usbd_hid.h , UsbRom.h
- CALLBACK_UsbdHid_Register_ReportDescriptor() : usbd_hid.h , UsbRom.h
- CALLBACK_UsbdHid_Register_ReportInBuffer() : usbd_hid.h , UsbRom.h
- CALLBACK_UsbdHid_SetReport() : usbd_hid.h , UsbRom.h
- CALLBACK_UsbdHid_SetReportChange() : usbd_hid.h , UsbRom.h
- CALLBACK_UsbdMsc_Register_BlockCount() : usbd_msc.h , UsbRom.h
- CALLBACK_UsbdMsc_Register_BlockSize() : usbd_msc.h , UsbRom.h
- CALLBACK_UsbdMsc_Register_InquiryData() : usbd_msc.h , UsbRom.h
- CALLBACK_UsbdMsc_Register_InterfaceDescriptor() : usbd_msc.h , UsbRom.h
- CALLBACK_UsbdMsc_Register_MemorySize() : usbd_msc.h , UsbRom.h
- CALLBACK_UsbdMsc_Register_MSCGetWriteBuf() : usbd_msc.h , UsbRom.h
- CALLBACK_UsbdMsc_Register_MSCRead() : usbd_msc.h , UsbRom.h
- CALLBACK_UsbdMsc_Register_MSCVerify() : usbd_msc.h , UsbRom.h
- CALLBACK_UsbdMsc_Register_MSCWrite() : usbd_msc.h , UsbRom.h
- CALLBACK_UsbdRom_Register_ConfigurationDescriptor() : usbd.h , UsbRom.h
- CALLBACK_UsbdRom_Register_ConfigureEndpoint() : usbd.h , UsbRom.h
- CALLBACK_UsbdRom_Register_DeviceDescriptor() : usbd.h , UsbRom.h
- CALLBACK_UsbdRom_Register_DeviceQualifierDescriptor() : UsbRom.h , usbd.h , UsbRom.h
- CALLBACK_UsbdRom_Register_StringDescriptor() : usbd.h , UsbRom.h
- CAN0_IRQHandler() : ccan.c
- CAN_error() : ccan_rom.c
- CAN_IRQHandler() : can.c , ccan_rom.c
- CAN_rx() : ccan_rom.c
- CAN_tx() : ccan_rom.c
- cardReset() : sdmmc_17xx_40xx.c
- CCAN_IF_Buf_transfer() : ccan_001.c
- CDC_Device_BytesReceived() : CDCClassDevice.c , CDCClassDevice.h
- CDC_Device_ConfigureEndpoints() : CDCClassDevice.c , CDCClassDevice.h
- CDC_Device_CreateBlockingStream() : CDCClassDevice.h
- CDC_Device_CreateStream() : CDCClassDevice.h
- CDC_Device_Event_Stub() : CDCClassDevice.c
- CDC_Device_Event_Stub2() : CDCClassDevice.c
- CDC_Device_Flush() : CDCClassDevice.c , CDCClassDevice.h
- CDC_Device_ProcessControlRequest() : CDCClassDevice.c , CDCClassDevice.h
- CDC_Device_ReceiveByte() : CDCClassDevice.c , CDCClassDevice.h
- CDC_Device_SendByte() : CDCClassDevice.c , CDCClassDevice.h
- CDC_Device_SendControlLineStateChange() : CDCClassDevice.c , CDCClassDevice.h
- CDC_Device_SendData() : CDCClassDevice.c , CDCClassDevice.h
- CDC_Device_SendString() : CDCClassDevice.c , CDCClassDevice.h
- CDC_Device_USBTask() : CDCClassDevice.c , CDCClassDevice.h
- CDC_Host_BytesReceived() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_ConfigurePipes() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_CreateBlockingStream() : CDCClassHost.h
- CDC_Host_CreateStream() : CDCClassHost.h
- CDC_Host_Event_Stub() : CDCClassHost.c
- CDC_Host_Flush() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_ReceiveByte() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_SendBreak() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_SendByte() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_SendControlLineStateChange() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_SendData() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_SendString() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_SetLineEncoding() : CDCClassHost.c , CDCClassHost.h
- CDC_Host_USBTask() : CDCClassHost.c , CDCClassHost.h
- ChangeAFLUT() : can.c
- check_fs() : ff.c
- checkBadBlock() : nandflash.c
- checkMagicHeader() : dfuutil_programming_dfu_ops.c
- checkR1Response() : sdmmc_17xx_40xx.c
- Chip_ACMP_Deinit() : acmp_8xx.c , acmp_8xx.h
- Chip_ACMP_DisableSyncCompOut() : acmp_8xx.h
- Chip_ACMP_DisableVoltLadder() : acmp_8xx.h
- Chip_ACMP_EdgeClear() : acmp_8xx.h
- Chip_ACMP_EnableSyncCompOut() : acmp_8xx.h
- Chip_ACMP_EnableVoltLadder() : acmp_8xx.h
- Chip_ACMP_GetCompStatus() : acmp_8xx.h
- Chip_ACMP_Init() : acmp_8xx.c , acmp_8xx.h
- Chip_ACMP_SetEdgeSelection() : acmp_8xx.h
- Chip_ACMP_SetHysteresis() : acmp_8xx.h
- Chip_ACMP_SetNegVoltRef() : acmp_8xx.h
- Chip_ACMP_SetPosVoltRef() : acmp_8xx.h
- Chip_ACMP_SetupAMCPRefs() : acmp_8xx.h
- Chip_ACMP_SetupVoltLadder() : acmp_8xx.h
- Chip_ADC_Burst_Cmd() : adc_11xx.c , adc_11xx.h , adc_13xx.c , adc_13xx.h , adc_17xx_40xx.c , adc_17xx_40xx.h , adc_18xx_43xx.c , adc_18xx_43xx.h
- Chip_ADC_Channel_Enable_Cmd() : adc_11xx.c , adc_11xx.h , adc_13xx.c , adc_13xx.h , adc_17xx_40xx.c , adc_17xx_40xx.h , adc_18xx_43xx.c , adc_18xx_43xx.h
- Chip_ADC_Channel_Int_Cmd() : adc_11xx.h , adc_13xx.h , adc_17xx_40xx.h , adc_18xx_43xx.h
- Chip_ADC_DeInit() : adc_11xx.c , adc_11xx.h , adc_13xx.c , adc_13xx.h , adc_17xx_40xx.c , adc_17xx_40xx.h , adc_18xx_43xx.c , adc_18xx_43xx.h
- Chip_ADC_GetClk() : adc_18xx_43xx.c
- Chip_ADC_Global_Int_Cmd() : adc_11xx.h , adc_13xx.h , adc_17xx_40xx.h , adc_18xx_43xx.h
- Chip_ADC_Init() : adc_18xx_43xx.h , adc_11xx.c , adc_11xx.h , adc_13xx.c , adc_13xx.h , adc_17xx_40xx.c , adc_17xx_40xx.h , adc_18xx_43xx.c
- Chip_ADC_Read_Byte() : adc_11xx.c , adc_11xx.h , adc_13xx.c , adc_13xx.h , adc_17xx_40xx.c , adc_17xx_40xx.h , adc_18xx_43xx.c , adc_18xx_43xx.h
- Chip_ADC_Read_Status() : adc_11xx.h , adc_13xx.h , adc_17xx_40xx.h , adc_18xx_43xx.h
- Chip_ADC_Read_Value() : adc_11xx.h , adc_13xx.h , adc_17xx_40xx.h , adc_18xx_43xx.h
- Chip_ADC_Set_Resolution() : adc_11xx.c , adc_11xx.h , adc_13xx.c , adc_13xx.h , adc_18xx_43xx.c , adc_18xx_43xx.h
- Chip_ADC_Set_SampleRate() : adc_11xx.c , adc_11xx.h , adc_13xx.c , adc_13xx.h , adc_17xx_40xx.c , adc_17xx_40xx.h , adc_18xx_43xx.c , adc_18xx_43xx.h
- Chip_ADC_Set_StartMode() : adc_11xx.c , adc_11xx.h , adc_13xx.c , adc_13xx.h , adc_17xx_40xx.c , adc_17xx_40xx.h , adc_18xx_43xx.c , adc_18xx_43xx.h
- Chip_AES_Init() : aes_18xx_43xx.c , aes_18xx_43xx.h
- Chip_AES_LoadIV_IC() : aes_18xx_43xx.c , aes_18xx_43xx.h
- Chip_AES_LoadIV_SW() : aes_18xx_43xx.c , aes_18xx_43xx.h
- Chip_AES_LoadKey() : aes_18xx_43xx.c , aes_18xx_43xx.h
- Chip_AES_LoadKeyRNG() : aes_18xx_43xx.c , aes_18xx_43xx.h
- Chip_AES_LoadKeySW() : aes_18xx_43xx.c , aes_18xx_43xx.h
- Chip_AES_Operate() : aes_18xx_43xx.c , aes_18xx_43xx.h
- Chip_AES_ProgramKey() : aes_18xx_43xx.c , aes_18xx_43xx.h
- Chip_AES_SetMode() : aes_18xx_43xx.c , aes_18xx_43xx.h
- Chip_ATIMER_ClearIntStatus() : atimer_18xx_43xx.h
- Chip_ATIMER_DeInit() : atimer_18xx_43xx.h
- Chip_ATIMER_GetPresetValue() : atimer_18xx_43xx.h
- Chip_ATIMER_Init() : atimer_18xx_43xx.c , atimer_18xx_43xx.h
- Chip_ATIMER_IntDisable() : atimer_18xx_43xx.h
- Chip_ATIMER_IntEnable() : atimer_18xx_43xx.h
- Chip_ATIMER_SetIntStatus() : atimer_18xx_43xx.h
- Chip_ATIMER_UpdatePresetValue() : atimer_18xx_43xx.h
- Chip_CAN_DeInit() : can_17xx_40xx.c , can_17xx_40xx.h
- Chip_CAN_DetermineClk() : can_17xx_40xx.c
- Chip_CAN_DetermineReset() : can_17xx_40xx.c
- Chip_CAN_FullCANIntConfig() : can_17xx_40xx.h
- Chip_CAN_FullCANReceive() : can_17xx_40xx.h
- Chip_CAN_GetClockRate() : can_17xx_40xx.c
- Chip_CAN_GetEntriesNum() : can_17xx_40xx.h
- Chip_CAN_GetFreeTxBuf() : can_17xx_40xx.c , can_17xx_40xx.h
- Chip_CAN_GetFullCANIntStatus() : can_17xx_40xx.h
- Chip_CAN_GetIntStatus() : can_17xx_40xx.h
- Chip_CAN_GetStatus() : can_17xx_40xx.h
- Chip_CAN_Init() : can_17xx_40xx.c , can_17xx_40xx.h
- Chip_CAN_InsertFullCANEntry() : can_17xx_40xx.h
- Chip_CAN_InsertGroupEXTEntry() : can_17xx_40xx.h
- Chip_CAN_InsertGroupSTDEntry() : can_17xx_40xx.h
- Chip_CAN_InsertIndividualEXTEntry() : can_17xx_40xx.h
- Chip_CAN_InsertIndividualSTDEntry() : can_17xx_40xx.h
- Chip_CAN_IntDisable() : can_17xx_40xx.h
- Chip_CAN_IntEnable() : can_17xx_40xx.h
- Chip_CAN_ReadFullCANEntry() : can_17xx_40xx.h
- Chip_CAN_ReadGroupEXTEntry() : can_17xx_40xx.h
- Chip_CAN_ReadGroupSTDEntry() : can_17xx_40xx.h
- Chip_CAN_ReadIndividualEXTEntry() : can_17xx_40xx.h
- Chip_CAN_ReadIndividualSTDEntry() : can_17xx_40xx.h
- Chip_CAN_Receive() : can_17xx_40xx.h
- Chip_CAN_RemoveFullCANEntry() : can_17xx_40xx.h
- Chip_CAN_RemoveGroupEXTEntry() : can_17xx_40xx.h
- Chip_CAN_RemoveGroupSTDEntry() : can_17xx_40xx.h
- Chip_CAN_RemoveIndividualEXTEntry() : can_17xx_40xx.h
- Chip_CAN_RemoveIndividualSTDEntry() : can_17xx_40xx.h
- Chip_CAN_Send() : can_17xx_40xx.h
- Chip_CAN_SetAFLUT() : can_17xx_40xx.h
- Chip_CAN_SetAFMode() : can_17xx_40xx.h
- Chip_CAN_SetBitRate() : can_17xx_40xx.c , can_17xx_40xx.h
- Chip_CAN_SetMode() : can_17xx_40xx.h
- Chip_CCAN_AddReceiveID() : ccan_18xx_43xx.c , ccan_18xx_43xx.h
- Chip_CCAN_ClearIntPend() : ccan_18xx_43xx.c , ccan_18xx_43xx.h
- Chip_CCAN_ClearStatus() : ccan_18xx_43xx.c , ccan_18xx_43xx.h
- Chip_CCAN_DeInit() : ccan_18xx_43xx.c , ccan_18xx_43xx.h
- Chip_CCAN_DeleteReceiveID() : ccan_18xx_43xx.c , ccan_18xx_43xx.h
- Chip_CCAN_GetIntID() : ccan_18xx_43xx.h
- Chip_CCAN_GetMsgObject() : ccan_18xx_43xx.h
- Chip_CCAN_GetStatus() : ccan_18xx_43xx.h
- Chip_CCAN_Init() : ccan_18xx_43xx.c , ccan_18xx_43xx.h
- Chip_CCAN_IntEnable() : ccan_18xx_43xx.h
- Chip_CCAN_Send() : ccan_18xx_43xx.c , ccan_18xx_43xx.h
- Chip_CCAN_SetBitRate() : ccan_18xx_43xx.c , ccan_18xx_43xx.h
- Chip_Clock_ClearPowerDown() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_Disable() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_DisableBaseClock() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_DisableCLKOUT() : clock_17xx_40xx.h
- Chip_Clock_DisableCrystal() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_DisableMainPLL() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_DisablePeriphClock() : clock_11xx.h , clock_13xx.h , clock_17xx_40xx.c , clock_17xx_40xx.h , clock_8xx.h
- Chip_Clock_DisablePLL() : clock_17xx_40xx.c , clock_17xx_40xx.h , clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_Enable() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_EnableBaseClock() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_EnableCLKOUT() : clock_17xx_40xx.h
- Chip_Clock_EnableCrystal() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_EnableMainPLL() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_EnableOpts() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_EnablePeriphClock() : clock_11xx.h , clock_13xx.h , clock_17xx_40xx.c , clock_17xx_40xx.h , clock_8xx.h
- Chip_Clock_EnablePLL() : clock_17xx_40xx.c , clock_17xx_40xx.h , clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_FeedPLL() : clock_17xx_40xx.h
- Chip_Clock_FindBaseClock() : clock_18xx_43xx.c
- Chip_Clock_GetBaseClock() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_GetBaseClockOpts() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_GetBaseClocktHz() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_GetClockInputHz() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_GetCPUClockDiv() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_GetCPUClockSource() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_GetDividerDivisor() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_GetDividerSource() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_GetDivRate() : clock_18xx_43xx.c
- Chip_Clock_GetEMCClockDiv() : clock_17xx_40xx.h
- Chip_Clock_GetEMCClockRate() : clock_17xx_40xx.h
- Chip_Clock_GetENETClockRate() : clock_17xx_40xx.h
- Chip_Clock_GetExtClockInRate() : clock_8xx.h
- Chip_Clock_GetGPDMAClockRate() : clock_17xx_40xx.h
- Chip_Clock_GetIntOscRate() : clock_11xx.h , clock_13xx.h , clock_17xx_40xx.h , clock_8xx.h
- Chip_Clock_GetLCDClockDiv() : clock_17xx_40xx.h
- Chip_Clock_GetMainClockRate() : clock_11xx.c , clock_11xx.h , clock_13xx.c , clock_13xx.h , clock_17xx_40xx.c , clock_17xx_40xx.h , clock_8xx.c , clock_8xx.h
- Chip_Clock_GetMainClockSource() : clock_11xx.h , clock_13xx.h , clock_8xx.h
- Chip_Clock_GetMainOscRate() : clock_11xx.h , clock_13xx.h , clock_17xx_40xx.h , clock_8xx.h
- Chip_Clock_GetMainPLLHz() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_GetMainPllInClockRate() : clock_17xx_40xx.h
- Chip_Clock_GetMainPllOutClockRate() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_GetMainPllSource() : clock_17xx_40xx.h
- Chip_Clock_GetPCLKDiv() : clock_17xx_40xx.h
- Chip_Clock_GetPeripheralClockRate() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_GetPllFreq() : clock_11xx.c , clock_13xx.c , clock_8xx.c
- Chip_Clock_GetPLLStatus() : clock_17xx_40xx.h , clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_GetRate() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_GetRTCClockRate() : clock_17xx_40xx.h
- Chip_Clock_GetRTCOscRate() : clock_17xx_40xx.h
- Chip_Clock_GetSPIFIClockDiv() : clock_17xx_40xx.h
- Chip_Clock_GetSPIFIClockRate() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_GetSPIFIClockSource() : clock_17xx_40xx.h
- Chip_Clock_GetSSP0ClockDiv() : clock_11xx.h , clock_13xx.h
- Chip_Clock_GetSSP1ClockDiv() : clock_13xx.h
- Chip_Clock_GetSYSCLKRate() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_GetSystemClockRate() : clock_11xx.c , clock_11xx.h , clock_13xx.c , clock_13xx.h , clock_17xx_40xx.c , clock_17xx_40xx.h , clock_8xx.c , clock_8xx.h
- Chip_Clock_GetSystemPllInClockRate() : clock_11xx.c , clock_11xx.h , clock_13xx.c , clock_13xx.h , clock_8xx.c , clock_8xx.h
- Chip_Clock_GetSystemPllOutClockRate() : clock_8xx.h , clock_11xx.c , clock_11xx.h , clock_13xx.c , clock_13xx.h , clock_8xx.c
- Chip_Clock_GetSystickClockDiv() : clock_13xx.h
- Chip_Clock_GetTraceClockDiv() : clock_13xx.h
- Chip_Clock_GetUARTClockDiv() : clock_11xx.h , clock_13xx.h , clock_8xx.h
- Chip_Clock_GetUSBClockDiv() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_GetUSBClockRate() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_GetUSBClockSource() : clock_17xx_40xx.h
- Chip_Clock_GetUSBPllInClockRate() : clock_13xx.c , clock_13xx.h , clock_17xx_40xx.h
- Chip_Clock_GetUSBPllOutClockRate() : clock_13xx.c , clock_13xx.h , clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_GetWDTLFORate() : clock_11xx.c , clock_13xx.c , clock_8xx.c
- Chip_Clock_GetWDTOSCRate() : clock_11xx.c , clock_11xx.h , clock_13xx.c , clock_13xx.h , clock_8xx.c , clock_8xx.h
- Chip_Clock_IsBaseClockEnabled() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_IsCLKOUTEnabled() : clock_17xx_40xx.h
- Chip_Clock_IsMainPLLEnabled() : clock_17xx_40xx.h
- Chip_Clock_IsMainPLLLocked() : clock_17xx_40xx.h
- Chip_Clock_IsPeripheralClockEnabled() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_IsSystemPLLLocked() : clock_11xx.h , clock_13xx.h , clock_8xx.h
- Chip_Clock_IsUSBPLLEnabled() : clock_17xx_40xx.h
- Chip_Clock_IsUSBPLLLocked() : clock_13xx.h , clock_17xx_40xx.h
- Chip_Clock_MainPLLLocked() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_SetBaseClock() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_SetCLKOUTSource() : clock_11xx.c , clock_11xx.h , clock_13xx.c , clock_13xx.h , clock_17xx_40xx.c , clock_17xx_40xx.h , clock_8xx.c , clock_8xx.h
- Chip_Clock_SetCPUClockDiv() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_SetCPUClockSource() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_SetDivider() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_SetEMCClockDiv() : clock_17xx_40xx.h
- Chip_Clock_SetLCDClockDiv() : clock_17xx_40xx.h
- Chip_Clock_SetMainClockSource() : clock_11xx.c , clock_11xx.h , clock_13xx.c , clock_13xx.h , clock_8xx.c , clock_8xx.h
- Chip_Clock_SetMainPllSource() : clock_17xx_40xx.h
- Chip_Clock_SetPCLKDiv() : clock_17xx_40xx.h
- Chip_Clock_SetPLLBypass() : clock_11xx.c , clock_11xx.h , clock_13xx.c , clock_13xx.h , clock_8xx.c , clock_8xx.h
- Chip_Clock_SetSPIFIClockDiv() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_SetSPIFIClockSource() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_SetSSP0ClockDiv() : clock_11xx.h , clock_13xx.h
- Chip_Clock_SetSSP1ClockDiv() : clock_13xx.h
- Chip_Clock_SetSysClockDiv() : clock_11xx.h , clock_13xx.h , clock_8xx.h
- Chip_Clock_SetSystemPllSource() : clock_11xx.c , clock_11xx.h , clock_13xx.c , clock_13xx.h , clock_8xx.c , clock_8xx.h
- Chip_Clock_SetSystickClockDiv() : clock_13xx.h
- Chip_Clock_SetTraceClockDiv() : clock_13xx.h
- Chip_Clock_SetUARTClockDiv() : clock_11xx.h , clock_13xx.h , clock_8xx.h
- Chip_Clock_SetupMainPLLHz() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_SetupMainPLLMult() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_SetupPLL() : clock_17xx_40xx.c , clock_17xx_40xx.h , clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_SetupSystemPLL() : clock_11xx.h , clock_13xx.h , clock_8xx.h
- Chip_Clock_SetupUSBPLL() : clock_13xx.h
- Chip_Clock_SetUSBClockDiv() : clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_SetUSBClockSource() : clock_13xx.c , clock_13xx.h , clock_17xx_40xx.c , clock_17xx_40xx.h
- Chip_Clock_SetUSBPllSource() : clock_13xx.c , clock_13xx.h
- Chip_Clock_SetWDTOSC() : clock_11xx.h , clock_13xx.h , clock_8xx.h
- Chip_Clock_StartPowerDown() : clock_18xx_43xx.c , clock_18xx_43xx.h
- Chip_Clock_TestMainPLLMultiplier() : clock_18xx_43xx.c
- Chip_CRC_CRC16() : crc_17xx_40xx.c , crc_17xx_40xx.h , crc_8xx.c , crc_8xx.h
- Chip_CRC_CRC32() : crc_17xx_40xx.c , crc_17xx_40xx.h , crc_8xx.c , crc_8xx.h
- Chip_CRC_CRC8() : crc_17xx_40xx.c , crc_17xx_40xx.h , crc_8xx.c , crc_8xx.h
- Chip_CRC_Deinit() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_GetMode() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_GetSeed() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_Init() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_SetMode() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_SetPoly() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_SetSeed() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_Sum() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_UseDefaultConfig() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_Write16() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_Write32() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CRC_Write8() : crc_17xx_40xx.h , crc_8xx.h
- Chip_CREG_ConfigureBODaR() : creg_18xx_43xx.h
- Chip_CREG_EnableUSB0Phy() : creg_18xx_43xx.h
- Chip_CREG_OnChipFlashIsPresent() : creg_18xx_43xx.h
- Chip_CREG_SetFlashAcceleration() : creg_18xx_43xx.h
- Chip_DAC_ConfigDAConverterControl() : dac_17xx_40xx.h , dac_18xx_43xx.h
- Chip_DAC_DeInit() : dac_17xx_40xx.h , dac_18xx_43xx.c , dac_18xx_43xx.h
- Chip_DAC_GetIntStatus() : dac_17xx_40xx.h , dac_18xx_43xx.h
- Chip_DAC_Init() : dac_17xx_40xx.c , dac_17xx_40xx.h , dac_18xx_43xx.c , dac_18xx_43xx.h
- Chip_DAC_SetBias() : dac_17xx_40xx.h , dac_18xx_43xx.h
- Chip_DAC_SetDMATimeOut() : dac_17xx_40xx.h , dac_18xx_43xx.h
- Chip_DAC_UpdateValue() : dac_17xx_40xx.h , dac_18xx_43xx.h
- Chip_DMA_GetFreeChannel() : gpdma_17xx_40xx.c , gpdma_17xx_40xx.h , gpdma_18xx_43xx.c , gpdma_18xx_43xx.h
- Chip_DMA_InitChannelCfg() : gpdma_17xx_40xx.c , gpdma_17xx_40xx.h , gpdma_18xx_43xx.c , gpdma_18xx_43xx.h
- Chip_DMA_Interrupt() : gpdma_17xx_40xx.c , gpdma_17xx_40xx.h , gpdma_18xx_43xx.c , gpdma_18xx_43xx.h
- Chip_DMA_PrepareDescriptor() : gpdma_17xx_40xx.c , gpdma_17xx_40xx.h , gpdma_18xx_43xx.c , gpdma_18xx_43xx.h
- Chip_DMA_SGTransfer() : gpdma_17xx_40xx.c , gpdma_17xx_40xx.h , gpdma_18xx_43xx.c , gpdma_18xx_43xx.h
- Chip_DMA_Stop() : gpdma_17xx_40xx.c , gpdma_17xx_40xx.h , gpdma_18xx_43xx.c , gpdma_18xx_43xx.h
- Chip_DMA_Transfer() : gpdma_17xx_40xx.c , gpdma_17xx_40xx.h , gpdma_18xx_43xx.c , gpdma_18xx_43xx.h
- Chip_EEPROM_ClearIntStatus() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_DeInit() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_DisableInt() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_DisablePowerDown() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_EnableInt() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_EnablePowerDown() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_Erase() : eeprom_17xx_40xx.h
- Chip_EEPROM_EraseProgramPage() : eeprom_18xx_43xx.h
- Chip_EEPROM_GetIntEnable() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_GetIntStatus() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_Init() : eeprom_17xx_40xx.c , eeprom_17xx_40xx.h , eeprom_18xx_43xx.c , eeprom_18xx_43xx.h
- Chip_EEPROM_Read() : eeprom_17xx_40xx.h
- Chip_EEPROM_SetAutoProg() : eeprom_18xx_43xx.h
- Chip_EEPROM_SetCmd() : eeprom_18xx_43xx.h
- Chip_EEPROM_SetIntStatus() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_SetReadWaitState() : eeprom_18xx_43xx.h
- Chip_EEPROM_SetWaitState() : eeprom_17xx_40xx.h , eeprom_18xx_43xx.h
- Chip_EEPROM_WaitForIntStatus() : eeprom_18xx_43xx.h
- Chip_EEPROM_Write() : eeprom_17xx_40xx.h
- Chip_EMC_Dynamic_Enable() : emc_17xx_40xx.h , emc_18xx_43xx.h
- Chip_EMC_Dynamic_Init() : emc_17xx_40xx.c , emc_17xx_40xx.h , emc_18xx_43xx.c , emc_18xx_43xx.h
- Chip_EMC_Enable() : emc_17xx_40xx.h , emc_18xx_43xx.h
- Chip_EMC_Init() : emc_17xx_40xx.h , emc_18xx_43xx.h
- Chip_EMC_LowPowerMode() : emc_17xx_40xx.h , emc_18xx_43xx.h
- Chip_EMC_Mirror() : emc_17xx_40xx.h , emc_18xx_43xx.h
- Chip_EMC_SetStaticExtendedWait() : emc_17xx_40xx.h , emc_18xx_43xx.h
- Chip_EMC_Static_Init() : emc_17xx_40xx.c , emc_17xx_40xx.h , emc_18xx_43xx.c , emc_18xx_43xx.h
- Chip_ENET_ClearIntStatus() : enet_17xx_40xx.h
- Chip_ENET_DeInit() : enet_17xx_40xx.c , enet_17xx_40xx.h , enet_18xx_43xx.c , enet_18xx_43xx.h
- Chip_ENET_DisableInt() : enet_17xx_40xx.h
- Chip_ENET_DisableRXFilter() : enet_17xx_40xx.h
- Chip_ENET_EnableInt() : enet_17xx_40xx.h
- Chip_ENET_EnableRXFilter() : enet_17xx_40xx.h
- Chip_ENET_FindMIIDiv() : enet_17xx_40xx.c , enet_17xx_40xx.h
- Chip_ENET_GetBufferStatus() : enet_17xx_40xx.h
- Chip_ENET_GetFillDescNum() : enet_17xx_40xx.h
- Chip_ENET_GetFreeDescNum() : enet_17xx_40xx.h
- Chip_ENET_GetIntStatus() : enet_17xx_40xx.h
- Chip_ENET_GetRXConsumeIndex() : enet_17xx_40xx.h
- Chip_ENET_GetRXProduceIndex() : enet_17xx_40xx.h
- Chip_ENET_GetTXConsumeIndex() : enet_17xx_40xx.h
- Chip_ENET_GetTXProduceIndex() : enet_17xx_40xx.h
- Chip_ENET_IncRXConsumeIndex() : enet_17xx_40xx.h
- Chip_ENET_IncTXProduceIndex() : enet_17xx_40xx.h
- Chip_ENET_Init() : enet_17xx_40xx.c , enet_17xx_40xx.h , enet_18xx_43xx.c , enet_18xx_43xx.h
- Chip_ENET_InitDescriptors() : enet_18xx_43xx.h
- Chip_ENET_InitRxDescriptors() : enet_17xx_40xx.h
- Chip_ENET_InitTxDescriptors() : enet_17xx_40xx.h
- Chip_ENET_IsMIIBusy() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_IsRxEmpty() : enet_17xx_40xx.h
- Chip_ENET_IsTxFull() : enet_17xx_40xx.h
- Chip_ENET_ReadMIIData() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_Reset() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_ResetRXLogic() : enet_17xx_40xx.h
- Chip_ENET_ResetTXLogic() : enet_17xx_40xx.h
- Chip_ENET_RXDisable() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_RXEnable() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_RXStart() : enet_18xx_43xx.h
- Chip_ENET_Set100Mbps() : enet_17xx_40xx.h
- Chip_ENET_Set10Mbps() : enet_17xx_40xx.h
- Chip_ENET_SetADDR() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_SetDuplex() : enet_18xx_43xx.h
- Chip_ENET_SetFullDuplex() : enet_17xx_40xx.h
- Chip_ENET_SetHalfDuplex() : enet_17xx_40xx.h
- Chip_ENET_SetSpeed() : enet_18xx_43xx.h
- Chip_ENET_SetupMII() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_StartMIIRead() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_StartMIIWrite() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_TXDisable() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_TXEnable() : enet_17xx_40xx.h , enet_18xx_43xx.h
- Chip_ENET_TXStart() : enet_18xx_43xx.h
- Chip_EVRT_ClrPendIntSrc() : evrt_18xx_43xx.h
- Chip_EVRT_ConfigIntSrcActiveType() : evrt_18xx_43xx.c , evrt_18xx_43xx.h
- Chip_EVRT_DeInit() : evrt_18xx_43xx.h
- Chip_EVRT_Init() : evrt_18xx_43xx.c , evrt_18xx_43xx.h
- Chip_EVRT_IsSourceInterrupting() : evrt_18xx_43xx.c , evrt_18xx_43xx.h
- Chip_EVRT_SetUpIntSrc() : evrt_18xx_43xx.c , evrt_18xx_43xx.h
- Chip_FIO_ClearValue() : gpio_18xx_43xx.h , gpio_8xx.h
- Chip_FIO_ReadValue() : gpio_18xx_43xx.h , gpio_8xx.h
- Chip_FIO_SetDir() : gpio_18xx_43xx.h
- Chip_FIO_SetValue() : gpio_18xx_43xx.h , gpio_8xx.h
- Chip_FMC_SetFLASHAccess() : fmc_11xx.h , fmc_13xx.h , fmc_17xx_40xx.h , fmc_8xx.h
- Chip_GPDMA_ChannelCmd() : gpdma_17xx_40xx.h , gpdma_18xx_43xx.h
- Chip_GPDMA_ClearIntPending() : gpdma_17xx_40xx.h , gpdma_18xx_43xx.h
- Chip_GPDMA_DeInit() : gpdma_17xx_40xx.c , gpdma_17xx_40xx.h , gpdma_18xx_43xx.c , gpdma_18xx_43xx.h
- Chip_GPDMA_Init() : gpdma_17xx_40xx.c , gpdma_17xx_40xx.h , gpdma_18xx_43xx.c , gpdma_18xx_43xx.h
- Chip_GPDMA_IntGetStatus() : gpdma_17xx_40xx.h , gpdma_18xx_43xx.h
- Chip_GPIO_ClearValue() : gpio_11xx.h , gpio_13xx.h , gpio_18xx_43xx.h
- Chip_GPIO_Init() : gpio_11xx.c , gpio_11xx.h , gpio_13xx.c , gpio_13xx.h , gpio_17xx_40xx.h , gpio_18xx_43xx.h , gpio_8xx.h
- Chip_GPIO_IntClear() : gpio_11xx.h , gpio_13xx.h , gpio_18xx_43xx.h
- Chip_GPIO_IntCmd() : gpio_11xx.h , gpio_13xx.h , gpio_18xx_43xx.h
- Chip_GPIO_IntGetStatus() : gpio_11xx.h , gpio_13xx.h , gpio_18xx_43xx.h
- Chip_GPIO_ReadDirBit() : gpio_11xx.h , gpio_13xx.h , gpio_17xx_40xx.h , gpio_18xx_43xx.h , gpio_8xx.h
- Chip_GPIO_ReadPortBit() : gpio_11xx.h , gpio_13xx.h , gpio_17xx_40xx.h , gpio_18xx_43xx.h , gpio_8xx.h
- Chip_GPIO_ReadValue() : gpio_11xx.h , gpio_13xx.h , gpio_18xx_43xx.h
- Chip_GPIO_SetDir() : gpio_11xx.c , gpio_11xx.h , gpio_13xx.c , gpio_13xx.h , gpio_18xx_43xx.c , gpio_18xx_43xx.h , gpio_8xx.c , gpio_8xx.h
- Chip_GPIO_SetValue() : gpio_11xx.h , gpio_13xx.h , gpio_18xx_43xx.h
- Chip_GPIO_WriteDirBit() : gpio_11xx.h , gpio_13xx.h , gpio_17xx_40xx.h , gpio_18xx_43xx.h , gpio_8xx.h
- Chip_GPIO_WritePortBit() : gpio_11xx.h , gpio_13xx.h , gpio_17xx_40xx.h , gpio_18xx_43xx.h , gpio_8xx.h
- Chip_GPIOGP_IntClear() : gpio_18xx_43xx.h
- Chip_GPIOGP_IntGetStatus() : gpio_18xx_43xx.h
- Chip_GPIOGP_IntInit() : gpio_18xx_43xx.h
- Chip_GPIOGP_IntPinAdd() : gpio_18xx_43xx.h
- Chip_GPIOGP_IntPinRemove() : gpio_18xx_43xx.h
- Chip_I2C_DeInit() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_Disable() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_EventHandler() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_EventHandlerPolling() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_GetClockRate() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_GetMasterEventHandler() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_Init() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h , i2c_8xx.c , i2c_8xx.h
- Chip_I2C_IsMasterActive() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_IsStateChanged() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_MasterCmdRead() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_MasterRead() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_MasterSend() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_MasterStateHandler() : i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h , i2c_11xx.c
- Chip_I2C_MasterTransfer() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_SetClockRate() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_SetMasterEventHandler() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_SlaveSetup() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2C_SlaveStateHandler() : i2c_11xx.c , i2c_11xx.h , i2c_13xx.c , i2c_13xx.h , i2c_17xx_40xx.c , i2c_17xx_40xx.h , i2c_18xx_43xx.c , i2c_18xx_43xx.h
- Chip_I2S_Config() : i2s_17xx_40xx.c , i2s_17xx_40xx.h , i2s_18xx_43xx.c , i2s_18xx_43xx.h
- Chip_I2S_DeInit() : i2s_17xx_40xx.c , i2s_17xx_40xx.h , i2s_18xx_43xx.c , i2s_18xx_43xx.h
- Chip_I2S_DisableMute() : i2s_17xx_40xx.h , i2s_18xx_43xx.h
- Chip_I2S_DMA_Cmd() : i2s_17xx_40xx.c , i2s_17xx_40xx.h , i2s_18xx_43xx.c , i2s_18xx_43xx.h
- Chip_I2S_EnableMute() : i2s_17xx_40xx.h , i2s_18xx_43xx.h
- Chip_I2S_GetLevel() : i2s_17xx_40xx.h , i2s_18xx_43xx.h
- Chip_I2S_Init() : i2s_17xx_40xx.c , i2s_17xx_40xx.h , i2s_18xx_43xx.c , i2s_18xx_43xx.h
- Chip_I2S_Int_Cmd() : i2s_17xx_40xx.c , i2s_17xx_40xx.h , i2s_18xx_43xx.c , i2s_18xx_43xx.h
- Chip_I2S_ModeConfig() : i2s_17xx_40xx.h , i2s_18xx_43xx.h
- Chip_I2S_Pause() : i2s_17xx_40xx.h , i2s_18xx_43xx.h
- Chip_I2S_Receive() : i2s_17xx_40xx.h , i2s_18xx_43xx.h
- Chip_I2S_Send() : i2s_17xx_40xx.h , i2s_18xx_43xx.h
- Chip_I2S_Start() : i2s_17xx_40xx.h , i2s_18xx_43xx.h
- Chip_I2S_Stop() : i2s_17xx_40xx.h , i2s_18xx_43xx.h
- Chip_IOCON_Init() : iocon_17xx_40xx.h
- Chip_IOCON_PinLocSel() : iocon_11xx.h , iocon_13xx.h
- Chip_IOCON_PinMux() : iocon_11xx.h , iocon_13xx.h , iocon_17xx_40xx.h
- Chip_IOCON_PinMuxSet() : iocon_11xx.h , iocon_13xx.h , iocon_17xx_40xx.h
- Chip_IOCON_PinSetClockDivisor() : iocon_8xx.c , iocon_8xx.h
- Chip_IOCON_PinSetHysteresis() : iocon_8xx.c , iocon_8xx.h
- Chip_IOCON_PinSetI2CMode() : iocon_8xx.c , iocon_8xx.h
- Chip_IOCON_PinSetInputInverted() : iocon_8xx.c , iocon_8xx.h
- Chip_IOCON_PinSetMode() : iocon_8xx.c , iocon_8xx.h
- Chip_IOCON_PinSetOpenDrainMode() : iocon_8xx.c , iocon_8xx.h
- Chip_IOCON_PinSetSampleMode() : iocon_8xx.c , iocon_8xx.h
- Chip_LCD_ClearInts() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_Cursor_Config() : lcd_17xx_40xx.c , lcd_17xx_40xx.h , lcd_18xx_43xx.c , lcd_18xx_43xx.h
- Chip_LCD_Cursor_Disable() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_Cursor_Enable() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_Cursor_LoadPalette0() : lcd_18xx_43xx.h , lcd_17xx_40xx.h
- Chip_LCD_Cursor_LoadPalette1() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_Cursor_SetClip() : lcd_18xx_43xx.h , lcd_17xx_40xx.h
- Chip_LCD_Cursor_SetPos() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_Cursor_WriteImage() : lcd_17xx_40xx.h , lcd_17xx_40xx.c , lcd_18xx_43xx.c , lcd_18xx_43xx.h
- Chip_LCD_DeInit() : lcd_17xx_40xx.c , lcd_17xx_40xx.h , lcd_18xx_43xx.c , lcd_18xx_43xx.h
- Chip_LCD_Disable() : lcd_18xx_43xx.h , lcd_17xx_40xx.h
- Chip_LCD_DisableInts() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_Enable() : lcd_18xx_43xx.h , lcd_17xx_40xx.h
- Chip_LCD_EnableInts() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_Init() : lcd_17xx_40xx.h , lcd_17xx_40xx.c , lcd_18xx_43xx.c , lcd_18xx_43xx.h
- Chip_LCD_LoadPalette() : lcd_17xx_40xx.c , lcd_17xx_40xx.h , lcd_18xx_43xx.c , lcd_18xx_43xx.h
- Chip_LCD_PowerOff() : lcd_18xx_43xx.h , lcd_17xx_40xx.h
- Chip_LCD_PowerOn() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_LCD_SetLPFrameBuffer() : lcd_18xx_43xx.h , lcd_17xx_40xx.h
- Chip_LCD_SetUPFrameBuffer() : lcd_17xx_40xx.h , lcd_18xx_43xx.h
- Chip_MRT_DeInit() : mrt_8xx.h
- Chip_MRT_GetEnabled() : mrt_8xx.h
- Chip_MRT_GetIdleChannel() : mrt_8xx.h
- Chip_MRT_GetInterval() : mrt_8xx.h
- Chip_MRT_GetIntPending() : mrt_8xx.h
- Chip_MRT_GetMode() : mrt_8xx.h
- Chip_MRT_GetTimer() : mrt_8xx.h
- Chip_MRT_Init() : mrt_8xx.h
- Chip_MRT_IntClear() : mrt_8xx.h
- Chip_MRT_IntPending() : mrt_8xx.h
- Chip_MRT_IsOneShotMode() : mrt_8xx.h
- Chip_MRT_IsRepeatMode() : mrt_8xx.h
- Chip_MRT_Running() : mrt_8xx.h
- Chip_MRT_SetEnabled() : mrt_8xx.h
- Chip_MRT_SetInterval() : mrt_8xx.h
- Chip_MRT_SetMode() : mrt_8xx.h
- Chip_OTP_GenRand() : otp_18xx_43xx.h , otp_18xx_43xx.c
- Chip_OTP_Init() : otp_18xx_43xx.c , otp_18xx_43xx.h
- Chip_OTP_ProgBootSrc() : otp_18xx_43xx.c , otp_18xx_43xx.h
- Chip_OTP_ProgGPWord() : otp_18xx_43xx.c , otp_18xx_43xx.h
- Chip_OTP_ProgJTAGDis() : otp_18xx_43xx.h , otp_18xx_43xx.c
- Chip_OTP_ProgKey() : otp_18xx_43xx.c , otp_18xx_43xx.h
- Chip_OTP_ProgUSBID() : otp_18xx_43xx.h , otp_18xx_43xx.c
- Chip_PININT_Config() : pinint_8xx.c , pinint_8xx.h
- Chip_PMC_Set_PwrState() : pmc_18xx_43xx.h , pmc_18xx_43xx.c
- Chip_PMC_Sleep() : pmc_18xx_43xx.c , pmc_18xx_43xx.h
- Chip_PMU_GetData() : pmu_11xx.h
- Chip_PMU_SetMode() : pmu_11xx.h
- Chip_PMU_Sleep() : pmu_8xx.c , pmu_8xx.h
- Chip_REGFILE_Read() : rtc_18xx_43xx.h , rtc_17xx_40xx.h
- Chip_REGFILE_Write() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RGU_ClearReset() : rgu_18xx_43xx.h , rgu_18xx_43xx.c
- Chip_RGU_InReset() : rgu_18xx_43xx.c , rgu_18xx_43xx.h
- Chip_RGU_TriggerReset() : rgu_18xx_43xx.h , rgu_18xx_43xx.c
- Chip_RIT_ClearInt() : ritimer_18xx_43xx.h
- Chip_RIT_DeInit() : ritimer_18xx_43xx.c , ritimer_18xx_43xx.h
- Chip_RIT_Disable() : ritimer_18xx_43xx.h
- Chip_RIT_Enable() : ritimer_18xx_43xx.h
- Chip_RIT_EnableCTRL() : ritimer_18xx_43xx.h
- Chip_RIT_GetCounter() : ritimer_18xx_43xx.h
- Chip_RIT_GetIntStatus() : ritimer_18xx_43xx.h
- Chip_RIT_Init() : ritimer_18xx_43xx.c , ritimer_18xx_43xx.h
- Chip_RIT_SetCOMPVAL() : ritimer_18xx_43xx.h
- Chip_RIT_SetTimerInterval() : ritimer_18xx_43xx.h , ritimer_18xx_43xx.c
- Chip_RIT_TimerDebugDisable() : ritimer_18xx_43xx.h
- Chip_RIT_TimerDebugEnable() : ritimer_18xx_43xx.h
- Chip_RTC_AlarmIntConfig() : rtc_18xx_43xx.h , rtc_17xx_40xx.h
- Chip_RTC_CalibConfig() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_CalibCounterCmd() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_ClearIntPending() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_CntIncrIntConfig() : rtc_18xx_43xx.h , rtc_17xx_40xx.h
- Chip_RTC_DeInit() : rtc_17xx_40xx.c , rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_Enable() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_GetAlarmTime() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_GetFullAlarmTime() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_GetFullTime() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_GetIntPending() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_GetTime() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_Init() : rtc_17xx_40xx.c , rtc_17xx_40xx.h , rtc_18xx_43xx.c , rtc_18xx_43xx.h
- Chip_RTC_ResetClockTickCounter() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_SetAlarmTime() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_SetFullAlarmTime() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_SetFullTime() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_RTC_SetTime() : rtc_17xx_40xx.h , rtc_18xx_43xx.h
- Chip_SCT_ClearEventFlag() : sct_8xx.h
- Chip_SCT_Config() : sct_18xx_43xx.h , sct_8xx.h
- Chip_SCT_ConflictResolutionSet() : sct_18xx_43xx.h
- Chip_SCT_ControlSetClr() : sct_18xx_43xx.h
- Chip_SCT_DeInit() : sct_18xx_43xx.h , sct_8xx.c , sct_8xx.h , sct_18xx_43xx.c
- Chip_SCT_EventFlagClear() : sct_18xx_43xx.h
- Chip_SCT_EventIntDisable() : sct_8xx.h
- Chip_SCT_EventIntEnable() : sct_8xx.h
- Chip_SCT_Init() : sct_18xx_43xx.c , sct_18xx_43xx.h , sct_8xx.c , sct_8xx.h
- Chip_SCT_SetCount() : sct_8xx.h
- Chip_SCT_SetCountH() : sct_8xx.h
- Chip_SCT_SetCountL() : sct_8xx.h
- Chip_SCT_SetMatchCount() : sct_8xx.h
- Chip_SCT_SetMatchReload() : sct_8xx.h
- Chip_SCU_ADC_Channel_Config() : scu_18xx_43xx.h
- Chip_SCU_ClockPinMux() : scu_18xx_43xx.h
- Chip_SCU_ClockPinMuxSet() : scu_18xx_43xx.h
- Chip_SCU_DAC_Analog_Config() : scu_18xx_43xx.h
- Chip_SCU_GPIOIntPinSel() : scu_18xx_43xx.h , scu_18xx_43xx.c
- Chip_SCU_I2C0PinConfig() : scu_18xx_43xx.h
- Chip_SCU_PinMux() : scu_18xx_43xx.h
- Chip_SCU_PinMuxSet() : scu_18xx_43xx.h
- Chip_SDC_DeInit() : sdc_17xx_40xx.c , sdc_17xx_40xx.h
- Chip_SDC_GetStatus() : sdc_17xx_40xx.h
- Chip_SDC_Init() : sdc_17xx_40xx.h , sdc_17xx_40xx.c
- Chip_SDC_SetClock() : sdc_17xx_40xx.c , sdc_17xx_40xx.h
- Chip_SDC_SetIntMask() : sdc_17xx_40xx.h
- Chip_SDIF_CardNDetect() : sdif_18xx_43xx.h
- Chip_SDIF_CardWpOn() : sdif_18xx_43xx.h
- Chip_SDIF_DeInit() : sdif_18xx_43xx.c , sdif_18xx_43xx.h
- Chip_SDIF_GetIntStatus() : sdif_18xx_43xx.c , sdif_18xx_43xx.h
- Chip_SDIF_Init() : sdif_18xx_43xx.c , sdif_18xx_43xx.h
- Chip_SDIF_PowerOff() : sdif_18xx_43xx.h
- Chip_SDIF_PowerOn() : sdif_18xx_43xx.h
- Chip_SDIF_SetIntMask() : sdif_18xx_43xx.h
- Chip_SDMMC_Acquire() : sdmmc_17xx_40xx.h , sdmmc_18xx_43xx.c , sdmmc_18xx_43xx.h , sdmmc_17xx_40xx.c
- Chip_SDMMC_FIFOIRQHandler() : sdmmc_17xx_40xx.c
- Chip_SDMMC_GetCardState() : sdmmc_17xx_40xx.c , sdmmc_17xx_40xx.h
- Chip_SDMMC_GetCardStatus() : sdmmc_17xx_40xx.c , sdmmc_17xx_40xx.h
- Chip_SDMMC_GetDeviceBlocks() : sdmmc_18xx_43xx.c , sdmmc_18xx_43xx.h
- Chip_SDMMC_GetDeviceSize() : sdmmc_18xx_43xx.c , sdmmc_18xx_43xx.h
- Chip_SDMMC_GetSDStatus() : sdmmc_17xx_40xx.c , sdmmc_17xx_40xx.h
- Chip_SDMMC_GetState() : sdmmc_18xx_43xx.c , sdmmc_18xx_43xx.h
- Chip_SDMMC_IRQHandler() : sdmmc_17xx_40xx.c , sdmmc_17xx_40xx.h
- Chip_SDMMC_ReadBlocks() : sdmmc_17xx_40xx.c , sdmmc_18xx_43xx.c , sdmmc_18xx_43xx.h , sdmmc_17xx_40xx.h
- Chip_SDMMC_WriteBlocks() : sdmmc_17xx_40xx.c , sdmmc_18xx_43xx.c , sdmmc_18xx_43xx.h , sdmmc_17xx_40xx.h
- Chip_SPI_CalClkRateDivider() : spi_8xx.c , spi_8xx.h
- Chip_SPI_DeInit() : spi_17xx_40xx.h , spi_8xx.c , spi_8xx.h
- Chip_SPI_DelayConfig() : spi_8xx.h
- Chip_SPI_Disable() : spi_8xx.h
- Chip_SPI_DisableLoopBack() : spi_8xx.h
- Chip_SPI_Enable() : spi_8xx.h
- Chip_SPI_EnableLoopBack() : spi_8xx.h
- Chip_SPI_GetStatus() : spi_17xx_40xx.h , spi_8xx.h
- Chip_SPI_Init() : spi_17xx_40xx.h , spi_8xx.h , spi_8xx.c
- Chip_SPI_Int_Cmd() : spi_8xx.c , spi_8xx.h
- Chip_SPI_Int_Disable() : spi_17xx_40xx.h
- Chip_SPI_Int_Enable() : spi_17xx_40xx.h
- Chip_SPI_Int_FlushData() : spi_17xx_40xx.h
- Chip_SPI_Int_RWFrames() : spi_8xx.c , spi_8xx.h
- Chip_SPI_Int_RWFrames16Bits() : spi_17xx_40xx.h
- Chip_SPI_Int_RWFrames8Bits() : spi_17xx_40xx.h
- Chip_SPI_ReadFrames_Blocking() : spi_17xx_40xx.h , spi_8xx.h , spi_8xx.c
- Chip_SPI_ReceiveFrame() : spi_8xx.h
- Chip_SPI_RWFrames_Blocking() : spi_17xx_40xx.h , spi_8xx.h , spi_8xx.c
- Chip_SPI_SendFirstFrame() : spi_8xx.h
- Chip_SPI_SendFirstFrame_RxIgnore() : spi_8xx.h
- Chip_SPI_SendLastFrame() : spi_8xx.h
- Chip_SPI_SendLastFrame_RxIgnore() : spi_8xx.h
- Chip_SPI_SendMidFrame() : spi_8xx.h
- Chip_SPI_SetBitRate() : spi_17xx_40xx.h
- Chip_SPI_SetFormat() : spi_17xx_40xx.h
- Chip_SPI_SetMode() : spi_17xx_40xx.h
- Chip_SPI_WriteFrames_Blocking() : spi_17xx_40xx.h , spi_8xx.c , spi_8xx.h
- Chip_SPIFI_DeInit() : spifi_17xx_40xx.h
- Chip_SPIFI_Init() : spifi_17xx_40xx.h
- Chip_SSP_DeInit() : ssp_11xx.c , ssp_13xx.c , ssp_13xx.h , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_18xx_43xx.h , ssp_11xx.h
- Chip_SSP_DetermineClk() : ssp_17xx_40xx.c
- Chip_SSP_Disable() : ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h , ssp_11xx.h
- Chip_SSP_DisableLoopBack() : ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h , ssp_11xx.h
- Chip_SSP_DMA_Disable() : ssp_18xx_43xx.h , ssp_17xx_40xx.h
- Chip_SSP_DMA_Enable() : ssp_17xx_40xx.h , ssp_18xx_43xx.h
- Chip_SSP_Enable() : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- Chip_SSP_EnableLoopBack() : ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h , ssp_11xx.h
- Chip_SSP_GetClockRate() : ssp_17xx_40xx.c
- Chip_SSP_GetStatus() : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- Chip_SSP_Init() : ssp_11xx.c , ssp_11xx.h , ssp_13xx.c , ssp_13xx.h , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_18xx_43xx.h
- Chip_SSP_Int_Disable() : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- Chip_SSP_Int_Enable() : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- Chip_SSP_Int_FlushData() : ssp_11xx.c , ssp_11xx.h , ssp_13xx.c , ssp_13xx.h , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_18xx_43xx.h
- Chip_SSP_Int_RWFrames16Bits() : ssp_11xx.c , ssp_11xx.h , ssp_13xx.c , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_18xx_43xx.h , ssp_13xx.h
- Chip_SSP_Int_RWFrames8Bits() : ssp_11xx.c , ssp_11xx.h , ssp_13xx.c , ssp_13xx.h , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_18xx_43xx.h
- Chip_SSP_ReadFrames_Blocking() : ssp_11xx.c , ssp_11xx.h , ssp_13xx.c , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_18xx_43xx.h , ssp_13xx.h
- Chip_SSP_RWFrames_Blocking() : ssp_11xx.c , ssp_11xx.h , ssp_13xx.c , ssp_13xx.h , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_18xx_43xx.h
- Chip_SSP_SetBitRate() : ssp_13xx.h , ssp_11xx.c , ssp_11xx.h , ssp_13xx.c , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_18xx_43xx.h
- Chip_SSP_SetFormat() : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- Chip_SSP_SetMaster() : ssp_18xx_43xx.c , ssp_18xx_43xx.h , ssp_11xx.c , ssp_11xx.h , ssp_13xx.c , ssp_13xx.h , ssp_17xx_40xx.c , ssp_17xx_40xx.h
- Chip_SSP_WriteFrames_Blocking() : ssp_11xx.h , ssp_18xx_43xx.h , ssp_13xx.h , ssp_11xx.c , ssp_17xx_40xx.c , ssp_17xx_40xx.h , ssp_18xx_43xx.c , ssp_13xx.c
- Chip_SWM_Deinit() : swm_8xx.h
- Chip_SWM_FixedPinEnable() : swm_8xx.h , swm_8xx.c
- Chip_SWM_Init() : swm_8xx.h
- Chip_SWM_IsEnabled() : swm_8xx.c , swm_8xx.h
- Chip_SWM_MovablePinAssign() : swm_8xx.h , swm_8xx.c
- Chip_SYSCTL_AssertPeriphReset() : sysctl_13xx.h , sysctl_11xx.h , syscon_8xx.h
- Chip_SYSCTL_ClearSystemRSTStatus() : sysctl_11xx.h , sysctl_13xx.h , sysctl_17xx_40xx.h , syscon_8xx.h
- Chip_SYSCTL_DeassertPeriphReset() : sysctl_11xx.h , syscon_8xx.h , sysctl_13xx.h
- Chip_SYSCTL_DisableBOD() : sysctl_17xx_40xx.h
- Chip_SYSCTL_DisableBODReset() : sysctl_11xx.h , syscon_8xx.h , sysctl_13xx.h , sysctl_17xx_40xx.h
- Chip_SYSCTL_DisableBODRPM() : sysctl_17xx_40xx.h
- Chip_SYSCTL_DisableBoost() : sysctl_17xx_40xx.h
- Chip_SYSCTL_DisableNMISource() : syscon_8xx.h
- Chip_SYSCTL_DisablePeriphWakeup() : syscon_8xx.h
- Chip_SYSCTL_DisablePINTWakeup() : syscon_8xx.h
- Chip_SYSCTL_DisableStartPin() : sysctl_13xx.h
- Chip_SYSCTL_EnableBOD() : sysctl_17xx_40xx.h
- Chip_SYSCTL_EnableBODReset() : sysctl_13xx.h , sysctl_11xx.h , sysctl_17xx_40xx.h , syscon_8xx.h
- Chip_SYSCTL_EnableBODRPM() : sysctl_17xx_40xx.h
- Chip_SYSCTL_EnableBoost() : sysctl_17xx_40xx.h
- Chip_SYSCTL_EnableNMISource() : syscon_8xx.h
- Chip_SYSCTL_EnablePeriphWakeup() : syscon_8xx.h
- Chip_SYSCTL_EnablePINTWakeuup() : syscon_8xx.h
- Chip_SYSCTL_EnableStartPin() : sysctl_13xx.h
- Chip_SYSCTL_GetClrSleepFlags() : sysctl_17xx_40xx.h , sysctl_17xx_40xx.c
- Chip_SYSCTL_GetDeepSleepPD() : sysctl_13xx.h , syscon_8xx.h , sysctl_11xx.h
- Chip_SYSCTL_GetDeviceID() : syscon_8xx.h , sysctl_11xx.h , sysctl_13xx.h
- Chip_SYSCTL_GetIRQLatency() : syscon_8xx.h
- Chip_SYSCTL_GetPORPIOStatus() : syscon_8xx.h , sysctl_13xx.h , sysctl_11xx.h
- Chip_SYSCTL_GetPowerStates() : sysctl_11xx.h , syscon_8xx.h , sysctl_13xx.h
- Chip_SYSCTL_GetStartPinStatus() : sysctl_13xx.h
- Chip_SYSCTL_GetSystemRSTStatus() : sysctl_13xx.h , syscon_8xx.h , sysctl_11xx.h , sysctl_17xx_40xx.h
- Chip_SYSCTL_GetUSARTFRGDivider() : syscon_8xx.h
- Chip_SYSCTL_GetUSARTFRGMultiplier() : syscon_8xx.h
- Chip_SYSCTL_GetWakeup() : sysctl_13xx.h , sysctl_11xx.h , syscon_8xx.h
- Chip_SYSCTL_Map() : sysctl_13xx.h , sysctl_17xx_40xx.h , syscon_8xx.h , sysctl_11xx.h
- Chip_SYSCTL_PeriphReset() : syscon_8xx.h , sysctl_17xx_40xx.c , sysctl_13xx.h , sysctl_17xx_40xx.h , sysctl_11xx.h
- Chip_SYSCTL_PowerDown() : syscon_8xx.h , sysctl_11xx.h , sysctl_13xx.c , sysctl_13xx.h , syscon_8xx.c , sysctl_11xx.c
- Chip_SYSCTL_PowerUp() : sysctl_13xx.h , sysctl_11xx.h , sysctl_13xx.c , sysctl_11xx.c , syscon_8xx.c , syscon_8xx.h
- Chip_SYSCTL_ResetStartPin() : sysctl_13xx.h
- Chip_SYSCTL_SetBODLevels() : syscon_8xx.h , sysctl_11xx.h , sysctl_13xx.h
- Chip_SYSCTL_SetDeepSleepPD() : syscon_8xx.h , sysctl_11xx.h , sysctl_13xx.c , sysctl_13xx.h , syscon_8xx.c , sysctl_11xx.c
- Chip_SYSCTL_SetIRQLatency() : syscon_8xx.h
- Chip_SYSCTL_SetNMISource() : syscon_8xx.h
- Chip_SYSCTL_SetPinInterrupt() : syscon_8xx.h
- Chip_SYSCTL_SetStartPinFalling() : sysctl_13xx.h
- Chip_SYSCTL_SetStartPinRising() : sysctl_13xx.h
- Chip_SYSCTL_SetSYSTCKCAL() : syscon_8xx.h , sysctl_13xx.h , sysctl_11xx.h
- Chip_SYSCTL_SetUSARTFRGDivider() : syscon_8xx.h
- Chip_SYSCTL_SetUSARTFRGMultiplier() : syscon_8xx.h
- Chip_SYSCTL_SetWakeup() : syscon_8xx.h , sysctl_11xx.h , sysctl_13xx.c , sysctl_13xx.h , syscon_8xx.c , sysctl_11xx.c
- Chip_TIMER_CaptureDisableInt() : timer_18xx_43xx.h , timer_17xx_40xx.h , timer_11xx.h , timer_13xx.h
- Chip_TIMER_CaptureEnableInt() : timer_18xx_43xx.h , timer_11xx.h , timer_17xx_40xx.h , timer_13xx.h
- Chip_TIMER_CaptureFallingEdgeDisable() : timer_17xx_40xx.h , timer_13xx.h , timer_18xx_43xx.h , timer_11xx.h
- Chip_TIMER_CaptureFallingEdgeEnable() : timer_18xx_43xx.h , timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h
- Chip_TIMER_CapturePending() : timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h , timer_11xx.h
- Chip_TIMER_CaptureRisingEdgeDisable() : timer_13xx.h , timer_18xx_43xx.h , timer_11xx.h , timer_17xx_40xx.h
- Chip_TIMER_CaptureRisingEdgeEnable() : timer_17xx_40xx.h , timer_13xx.h , timer_18xx_43xx.h , timer_11xx.h
- Chip_TIMER_ClearCapture() : timer_18xx_43xx.h , timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h
- Chip_TIMER_ClearMatch() : timer_18xx_43xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_11xx.h
- Chip_TIMER_DeInit() : timer_11xx.h , timer_18xx_43xx.c , timer_17xx_40xx.h , timer_18xx_43xx.h , timer_13xx.h , timer_11xx.c , timer_13xx.c , timer_17xx_40xx.c
- Chip_TIMER_Disable() : timer_18xx_43xx.h , timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h
- Chip_TIMER_Enable() : timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h , timer_11xx.h
- Chip_TIMER_ExtMatchControlSet() : timer_18xx_43xx.h , timer_13xx.h , timer_11xx.h , timer_17xx_40xx.h
- Chip_Timer_GetClock() : timer_13xx.c , timer_17xx_40xx.c , timer_18xx_43xx.c , timer_11xx.c
- Chip_TIMER_Init() : timer_18xx_43xx.h , timer_17xx_40xx.h , timer_13xx.h , timer_18xx_43xx.c , timer_11xx.c , timer_11xx.h , timer_13xx.c , timer_17xx_40xx.c
- Chip_TIMER_MatchDisableInt() : timer_18xx_43xx.h , timer_13xx.h , timer_11xx.h , timer_17xx_40xx.h
- Chip_TIMER_MatchEnableInt() : timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h , timer_11xx.h
- Chip_TIMER_MatchPending() : timer_18xx_43xx.h , timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h
- Chip_TIMER_PrescaleSet() : timer_17xx_40xx.h , timer_18xx_43xx.h , timer_13xx.h , timer_11xx.h
- Chip_TIMER_ReadCapture() : timer_18xx_43xx.h , timer_13xx.h , timer_11xx.h , timer_17xx_40xx.h
- Chip_TIMER_ReadCount() : timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h , timer_11xx.h
- Chip_TIMER_ReadPrescale() : timer_18xx_43xx.h , timer_11xx.h , timer_13xx.h , timer_17xx_40xx.h
- Chip_TIMER_Reset() : timer_18xx_43xx.h , timer_13xx.h , timer_17xx_40xx.h , timer_11xx.h
- Chip_TIMER_ResetOnMatchDisable() : timer_18xx_43xx.h , timer_13xx.h , timer_11xx.h , timer_17xx_40xx.h
- Chip_TIMER_ResetOnMatchEnable() : timer_13xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h , timer_11xx.h
- Chip_TIMER_SetMatch() : timer_18xx_43xx.h , timer_17xx_40xx.h , timer_11xx.h , timer_13xx.h
- Chip_TIMER_StopOnMatchDisable() : timer_17xx_40xx.h , timer_18xx_43xx.h , timer_13xx.h , timer_11xx.h
- Chip_TIMER_StopOnMatchEnable() : timer_11xx.h , timer_17xx_40xx.h , timer_13xx.h , timer_18xx_43xx.h
- Chip_TIMER_TIMER_SetCountClockSrc() : timer_13xx.h , timer_11xx.h , timer_17xx_40xx.h , timer_18xx_43xx.h
- Chip_UART_ABClearIntPending() : uart_17xx_40xx.h , uart_18xx_43xx.h
- Chip_UART_ABCmd() : uart_17xx_40xx.h , uart_18xx_43xx.h
- Chip_UART_CheckBusy() : uart_17xx_40xx.h , uart_18xx_43xx.h
- Chip_UART_ClearAutoBaudReg() : uart_11xx.h , uart_13xx.h
- Chip_UART_ClearModemControl() : uart_11xx.h , uart_13xx.h
- Chip_UART_ClearRS485Flags() : uart_11xx.h , uart_13xx.h
- Chip_UART_ConfigData() : uart_11xx.h , uart_8xx.h , uart_13xx.h , uart_17xx_40xx.h , uart_18xx_43xx.h
- Chip_UART_DeInit() : uart_11xx.c , uart_11xx.h , uart_13xx.h , uart_18xx_43xx.h , uart_17xx_40xx.c , uart_17xx_40xx.h , uart_18xx_43xx.c , uart_13xx.c
- Chip_UART_DetermineClk() : uart_18xx_43xx.c , uart_17xx_40xx.c
- Chip_UART_DisableDivisorAccess() : uart_13xx.h , uart_11xx.h
- Chip_UART_EnableDivisorAccess() : uart_11xx.h , uart_13xx.h
- Chip_UART_FIFOConfig() : uart_18xx_43xx.h , uart_17xx_40xx.h
- Chip_UART_FIFOConfigStructInit() : uart_18xx_43xx.h , uart_17xx_40xx.h
- Chip_UART_ForceBreak() : uart_18xx_43xx.h , uart_17xx_40xx.h
- Chip_UART_Get_UARTNum() : uart_17xx_40xx.c , uart_18xx_43xx.c
- Chip_UART_GetABEOStatus() : uart_17xx_40xx.h , uart_18xx_43xx.h , uart_18xx_43xx.c , uart_17xx_40xx.c
- Chip_UART_GetClockRate() : uart_17xx_40xx.c
- Chip_UART_GetIntStatus() : uart_17xx_40xx.c , uart_8xx.h , uart_17xx_40xx.h , uart_18xx_43xx.c , uart_18xx_43xx.h
- Chip_UART_GetLineStatus() : uart_17xx_40xx.h , uart_18xx_43xx.h
- Chip_UART_GetRS485Addr() : uart_13xx.h , uart_11xx.h
- Chip_UART_GetRS485Delay() : uart_13xx.h , uart_11xx.h
- Chip_UART_Init() : uart_17xx_40xx.h , uart_17xx_40xx.c , uart_13xx.h , uart_11xx.h , uart_11xx.c , uart_13xx.c , uart_8xx.h , uart_8xx.c , uart_18xx_43xx.h , uart_18xx_43xx.c
- Chip_UART_InitRingBuffer() : uart_17xx_40xx.h , uart_18xx_43xx.h , uart_17xx_40xx.c , uart_18xx_43xx.c
- Chip_UART_IntConfig() : uart_18xx_43xx.h , uart_17xx_40xx.h
- Chip_UART_IntDisable() : uart_13xx.h , uart_11xx.h
- Chip_UART_IntEnable() : uart_11xx.h , uart_8xx.h , uart_13xx.h
- Chip_UART_Interrupt_Handler() : uart_17xx_40xx.c , uart_18xx_43xx.h , uart_18xx_43xx.c , uart_17xx_40xx.h
- Chip_UART_Interrupt_Receive() : uart_17xx_40xx.h , uart_18xx_43xx.c , uart_18xx_43xx.h , uart_17xx_40xx.c
- Chip_UART_Interrupt_Transmit() : uart_18xx_43xx.c , uart_17xx_40xx.h , uart_18xx_43xx.h , uart_17xx_40xx.c
- Chip_UART_IntGetStatus() : uart_18xx_43xx.h , uart_17xx_40xx.h
- Chip_UART_IRQRBHandler() : uart_11xx.c , uart_11xx.h , uart_13xx.c , uart_13xx.h
- Chip_UART_Read() : uart_13xx.h , uart_11xx.h , uart_13xx.c , uart_11xx.c
- Chip_UART_ReadBlocking() : uart_11xx.c , uart_13xx.c , uart_13xx.h , uart_11xx.h
- Chip_UART_ReadByte() : uart_13xx.h , uart_11xx.h
- Chip_UART_ReadIntIDReg() : uart_11xx.h , uart_13xx.h
- Chip_UART_ReadLineStatus() : uart_11xx.h , uart_13xx.h
- Chip_UART_ReadModemControl() : uart_13xx.h , uart_11xx.h
- Chip_UART_ReadModemStatus() : uart_11xx.h , uart_13xx.h
- Chip_UART_ReadRB() : uart_11xx.h , uart_13xx.h , uart_13xx.c , uart_11xx.c
- Chip_UART_ReadScratch() : uart_13xx.h , uart_11xx.h
- Chip_UART_Receive() : uart_18xx_43xx.h , uart_17xx_40xx.h
- Chip_UART_ReceiveByte() : uart_18xx_43xx.h , uart_8xx.h , uart_17xx_40xx.h , uart_8xx.c
- Chip_UART_RXIntHandlerRB() : uart_11xx.c , uart_13xx.h , uart_13xx.c , uart_11xx.h
- Chip_UART_Send() : uart_11xx.h , uart_18xx_43xx.h , uart_13xx.h , uart_13xx.c , uart_17xx_40xx.h , uart_11xx.c
- Chip_UART_SendBlocking() : uart_11xx.c , uart_13xx.h , uart_13xx.c , uart_11xx.h
- Chip_UART_SendByte() : uart_17xx_40xx.h , uart_11xx.h , uart_18xx_43xx.h , uart_8xx.c , uart_8xx.h , uart_13xx.h
- Chip_UART_SendRB() : uart_13xx.c , uart_11xx.h , uart_13xx.h , uart_11xx.c
- Chip_UART_SetAutoBaudReg() : uart_13xx.h , uart_11xx.h
- Chip_UART_SetBaud() : uart_17xx_40xx.h , uart_13xx.c , uart_18xx_43xx.c , uart_17xx_40xx.c , uart_11xx.c , uart_13xx.h , uart_11xx.h , uart_18xx_43xx.h
- Chip_UART_SetBaudFDR() : uart_11xx.h , uart_13xx.h
- Chip_UART_SetBaudRate() : uart_8xx.h , uart_8xx.c
- Chip_UART_SetDivisorLatches() : uart_13xx.h , uart_11xx.h
- Chip_UART_SetModemControl() : uart_11xx.h , uart_13xx.h
- Chip_UART_SetRS485Addr() : uart_13xx.h , uart_11xx.h
- Chip_UART_SetRS485Delay() : uart_13xx.h , uart_11xx.h
- Chip_UART_SetRS485Flags() : uart_11xx.h , uart_13xx.h
- Chip_UART_SetScratch() : uart_13xx.h , uart_11xx.h
- Chip_UART_SetupFIFOS() : uart_11xx.h , uart_13xx.h
- Chip_UART_TxCmd() : uart_18xx_43xx.h , uart_17xx_40xx.h , uart_18xx_43xx.c , uart_17xx_40xx.c
- Chip_UART_TXDisable() : uart_11xx.h , uart_13xx.h
- Chip_UART_TXEnable() : uart_13xx.h , uart_11xx.h
- Chip_UART_TXIntHandlerRB() : uart_13xx.c , uart_13xx.h , uart_11xx.h , uart_11xx.c
- Chip_WKT_ClearIntStatus() : wkt_8xx.h
- Chip_WKT_Start() : wkt_8xx.h , wkt_8xx.c
- Chip_WKT_Stop() : wkt_8xx.h
- Chip_WWDT_ClearStatusFlag() : wwdt_18xx_43xx.h , wwdt_17xx_40xx.h , wwdt_8xx.h , wwdt_11xx.h , wwdt_13xx.h
- Chip_WWDT_DeInit() : wwdt_18xx_43xx.h , wwdt_11xx.h , wwdt_11xx.c , wwdt_8xx.h , wwdt_13xx.h , wwdt_13xx.c , wwdt_17xx_40xx.h
- Chip_WWDT_Feed() : wwdt_18xx_43xx.h , wwdt_17xx_40xx.h , wwdt_11xx.h , wwdt_13xx.h , wwdt_8xx.h
- Chip_WWDT_GetCurrentCount() : wwdt_13xx.h , wwdt_17xx_40xx.h , wwdt_8xx.h , wwdt_11xx.h , wwdt_18xx_43xx.h
- Chip_WWDT_GetStatus() : wwdt_8xx.h , wwdt_18xx_43xx.h , wwdt_11xx.h , wwdt_13xx.h , wwdt_17xx_40xx.h
- Chip_WWDT_Init() : wwdt_11xx.c , wwdt_11xx.h , wwdt_17xx_40xx.c , wwdt_13xx.h , wwdt_18xx_43xx.c , wwdt_8xx.c , wwdt_17xx_40xx.h , wwdt_18xx_43xx.h , wwdt_13xx.c , wwdt_8xx.h
- Chip_WWDT_SetOption() : wwdt_13xx.h , wwdt_17xx_40xx.h , wwdt_11xx.h , wwdt_18xx_43xx.h , wwdt_8xx.h
- Chip_WWDT_SetTimeOut() : wwdt_18xx_43xx.h , wwdt_8xx.h , wwdt_13xx.h , wwdt_11xx.h , wwdt_17xx_40xx.h
- Chip_WWDT_SetWarning() : wwdt_18xx_43xx.h , wwdt_8xx.h
- Chip_WWDT_SetWindow() : wwdt_8xx.h , wwdt_18xx_43xx.h
- Chip_WWDT_Start() : wwdt_18xx_43xx.h , wwdt_11xx.h , wwdt_8xx.h , wwdt_17xx_40xx.h , wwdt_13xx.h
- Chip_WWDT_UnsetOption() : wwdt_18xx_43xx.h , wwdt_13xx.h , wwdt_11xx.h , wwdt_17xx_40xx.h , wwdt_8xx.h
- chk_chr() : ff.c
- chk_mounted() : ff.c
- clust2sect() : ff.c
- CMP_IRQHandler() : acmp.c
- con_get_input() : i2c.c
- Con_GetInput() : i2s.c
- con_print_data() : i2c.c
- configTSC2046Pins() : board_ea_devkit_17884088.c
- CPU_BitBandClr() : cpu_c.c , cpu.h , cpu_c.c , cpu_c_m0.c , cpu.h , cpu_c.c , cpu_c_m0.c , cpu_c.c , cpu.h , cpu_c_m0.c , cpu_c.c , cpu.h , cpu_c.c , cpu.h
- CPU_BitBandSet() : cpu.h , cpu_c.c , cpu.h , cpu_c_m0.c , cpu.h , cpu_c.c , cpu.h , cpu_c_m0.c , cpu.h , cpu_c.c , cpu_c_m0.c
- CPU_CntLeadZeros() : cpu.h , os_cpu_c_m0.c , cpu.h , cpu_core.c , cpu.h , cpu_core.h
- CPU_Init() : cpu_core.c , cpu_core.h
- CPU_IntDis() : cpu.h
- CPU_IntEn() : cpu.h
- CPU_IntSrcDis() : cpu_c.c , cpu.h , cpu_c_m0.c , cpu.h , cpu_c_m0.c , cpu.h , cpu_c.c , cpu.h , cpu_c_m0.c , cpu_c.c , cpu.h , cpu_c.c
- CPU_IntSrcEn() : cpu_c_m0.c , cpu.h , cpu_c.c , cpu_c_m0.c , cpu.h , cpu_c.c , cpu.h , cpu_c.c , cpu.h , cpu_c.c , cpu.h , cpu_c.c , cpu.h , cpu_c_m0.c
- CPU_IntSrcPendClr() : cpu_c_m0.c , cpu_c.c , cpu.h , cpu_c_m0.c , cpu_c.c , cpu.h , cpu_c.c , cpu_c_m0.c , cpu_c.c , cpu.h , cpu_c.c , cpu.h , cpu_c.c
- CPU_IntSrcPrioGet() : cpu_c.c , cpu.h , cpu_c.c , cpu.h , cpu_c.c , cpu_c_m0.c , cpu.h , cpu_c.c , cpu.h , cpu_c.c , cpu.h
- CPU_IntSrcPrioSet() : cpu.h , cpu_c_m0.c , cpu.h , cpu_c.c , cpu.h , cpu_c.c , cpu_c_m0.c , cpu_c.c
- CPU_NameClr() : cpu_core.h , cpu_core.c
- CPU_NameGet() : cpu_core.h , cpu_core.c
- CPU_NameInit() : cpu_core.c
- CPU_NameSet() : cpu_core.c , cpu_core.h
- CPU_RevBits() : cpu.h
- CPU_SR_Restore() : cpu.h
- CPU_SR_Save() : cpu.h
- CPU_SW_Exception() : cpu_core.h , cpu_core.c
- CPU_TS32_to_uSec() : cpu_core.h
- CPU_TS64_to_uSec() : cpu_core.h
- CPU_TS_Get32() : cpu_core.h , cpu_core.c
- CPU_TS_Get64() : cpu_core.h , cpu_core.c
- CPU_TS_Init() : cpu_core.c
- CPU_TS_TmrFreqGet() : cpu_core.h , cpu_core.c
- CPU_TS_TmrFreqSet() : cpu_core.c , cpu_core.h
- CPU_TS_TmrInit() : cpu_bsp_lpc43xx_m0.c , cpu_bsp.c , cpu_core.h , cpu_bsp.c
- CPU_TS_TmrRd() : cpu_core.h , cpu_bsp.c , cpu_bsp_lpc43xx_m0.c , cpu_bsp.c
- CPU_TS_Update() : cpu_core.h , cpu_core.c
- CPU_WaitForExcept() : cpu.h
- CPU_WaitForInt() : cpu.h
- create_chain() : ff.c
- create_name() : ff.c
- CreateDiskImage() : fatutil.c , fatutil.h
- createExtIDEntry() : can_001.c
- createStdIDEntry() : can_001.c
- createUnUsedSTDEntry() : can_001.c