| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
rtc_18xx_43xx.h
Go to the documentation of this file.
1 /*
2 * @brief LPC18xx/43xx RTC driver
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __RTC_18XX_43XX_H_
33 #define __RTC_18XX_43XX_H_
34
35 #ifdef __cplusplus
36 extern "C" {
37 #endif
38
49 void Chip_RTC_Init(LPC_RTC_T *pRTC);
50
56 STATIC INLINE void Chip_RTC_DeInit(LPC_RTC_T *pRTC)
57 {
58 IP_RTC_DeInit(LPC_RTC);
59 }
60
66 STATIC INLINE void Chip_RTC_ResetClockTickCounter(LPC_RTC_T *pRTC)
67 {
68 IP_RTC_ResetClockTickCounter(LPC_RTC);
69 }
70
79 STATIC INLINE void Chip_RTC_Enable(LPC_RTC_T *pRTC, FunctionalState NewState)
80 {
81 IP_RTC_Enable(LPC_RTC, NewState);
82 }
83
92 STATIC INLINE void Chip_RTC_CntIncrIntConfig(LPC_RTC_T *pRTC, uint32_t cntrMask, FunctionalState NewState)
93 {
94 IP_RTC_CntIncrIntConfig(LPC_RTC, cntrMask, NewState);
95 }
96
105 STATIC INLINE void Chip_RTC_AlarmIntConfig(LPC_RTC_T *pRTC, uint32_t alarmMask, FunctionalState NewState)
106 {
107 IP_RTC_AlarmIntConfig(LPC_RTC, alarmMask, NewState);
108 }
109
117 STATIC INLINE void Chip_RTC_SetTime(LPC_RTC_T *pRTC, IP_RTC_TIMEINDEX_T Timetype, uint32_t TimeValue)
118 {
119 IP_RTC_SetTime(LPC_RTC, Timetype, TimeValue);
120 }
121
128 STATIC INLINE uint32_t Chip_RTC_GetTime(LPC_RTC_T *pRTC, IP_RTC_TIMEINDEX_T Timetype)
129 {
130 return IP_RTC_GetTime(LPC_RTC, Timetype);
131 }
132
139 STATIC INLINE void Chip_RTC_SetFullTime(LPC_RTC_T *pRTC, IP_RTC_TIME_T *pFullTime)
140 {
141 IP_RTC_SetFullTime(LPC_RTC, pFullTime);
142 }
143
150 STATIC INLINE void Chip_RTC_GetFullTime(LPC_RTC_T *pRTC, IP_RTC_TIME_T *pFullTime)
151 {
152 IP_RTC_GetFullTime(LPC_RTC, pFullTime);
153 }
154
162 STATIC INLINE void Chip_RTC_SetAlarmTime(LPC_RTC_T *pRTC, IP_RTC_TIMEINDEX_T Timetype, uint32_t ALValue)
163 {
164 IP_RTC_SetAlarmTime(LPC_RTC, Timetype, ALValue);
165 }
166
173 STATIC INLINE uint32_t Chip_RTC_GetAlarmTime(LPC_RTC_T *pRTC, IP_RTC_TIMEINDEX_T Timetype)
174 {
175 return IP_RTC_GetAlarmTime(LPC_RTC, Timetype);
176 }
177
184 STATIC INLINE void Chip_RTC_SetFullAlarmTime(LPC_RTC_T *pRTC, IP_RTC_TIME_T *pFullTime)
185 {
186 IP_RTC_SetFullAlarmTime(LPC_RTC, pFullTime);
187 }
188
195 STATIC INLINE void Chip_RTC_GetFullAlarmTime(LPC_RTC_T *pRTC, IP_RTC_TIME_T *pFullTime)
196 {
197 IP_RTC_GetFullAlarmTime(LPC_RTC, pFullTime);
198 }
199
211 STATIC INLINE void Chip_REGFILE_Write(LPC_REGFILE_T *pRegFile, uint8_t index, uint32_t Value)
212 {
213 IP_REGFILE_Write(pRegFile, index, Value);
214 }
215
226 STATIC INLINE uint32_t Chip_REGFILE_Read(LPC_REGFILE_T *pRegFile, uint8_t index)
227 {
228 return IP_REGFILE_Read(pRegFile, index);
229 }
230
239 STATIC INLINE void Chip_RTC_CalibCounterCmd(LPC_RTC_T *pRTC, FunctionalState NewState)
240 {
241 IP_RTC_CalibCounterCmd(LPC_RTC, NewState);
242 }
243
253 STATIC INLINE void Chip_RTC_CalibConfig(LPC_RTC_T *pRTC, uint32_t CalibValue, uint8_t CalibDir)
254 {
255 IP_RTC_CalibConfig(LPC_RTC, CalibValue, CalibDir);
256 }
257
266 STATIC INLINE void Chip_RTC_ClearIntPending(LPC_RTC_T *pRTC, uint32_t IntType)
267 {
268 IP_RTC_ClearIntPending(LPC_RTC, IntType);
269 }
270
279 STATIC INLINE IntStatus Chip_RTC_GetIntPending(LPC_RTC_T *pRTC, uint32_t IntType)
280 {
281 return IP_RTC_GetIntPending(LPC_RTC, IntType);
282 }
283
288 #ifdef __cplusplus
289 }
290 #endif
291
292 #endif /* __RTC_18XX_43XX_H_ */