| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - s -

- S16_F : cc.h
- s16_t : cc.h
- S29GL64N90_config : sysinit_keil_mcb_18574357.c
- S32_F : cc.h
- s32_t : cc.h
- s8_t : cc.h
- SAMPLE_MAX_RANGE : AudioOutputHost.h , AudioInput.h
- saved_period : lpc43xx_systick.c
- SCHEDULING_OVRERRUN_INTERRUPT : OHCI.h
- SCSI_ASENSE_FORMAT_ERROR : MassStorageClassCommon.h
- SCSI_ASENSE_INVALID_COMMAND : MassStorageClassCommon.h
- SCSI_ASENSE_INVALID_FIELD_IN_CDB : MassStorageClassCommon.h
- SCSI_ASENSE_LOGICAL_BLOCK_ADDRESS_OUT_OF_RANGE : MassStorageClassCommon.h
- SCSI_ASENSE_LOGICAL_UNIT_NOT_READY : MassStorageClassCommon.h
- SCSI_ASENSE_MEDIUM_NOT_PRESENT : MassStorageClassCommon.h
- SCSI_ASENSE_NO_ADDITIONAL_INFORMATION : MassStorageClassCommon.h
- SCSI_ASENSE_NOT_READY_TO_READY_CHANGE : MassStorageClassCommon.h
- SCSI_ASENSE_WRITE_PROTECTED : MassStorageClassCommon.h
- SCSI_ASENSEQ_FORMAT_COMMAND_FAILED : MassStorageClassCommon.h
- SCSI_ASENSEQ_INITIALIZING_COMMAND_REQUIRED : MassStorageClassCommon.h
- SCSI_ASENSEQ_NO_QUALIFIER : MassStorageClassCommon.h
- SCSI_ASENSEQ_OPERATION_IN_PROGRESS : MassStorageClassCommon.h
- SCSI_CMD_INQUIRY : MassStorageClassCommon.h
- SCSI_CMD_MODE_SENSE_10 : MassStorageClassCommon.h
- SCSI_CMD_MODE_SENSE_6 : MassStorageClassCommon.h
- SCSI_CMD_PREVENT_ALLOW_MEDIUM_REMOVAL : MassStorageClassCommon.h
- SCSI_CMD_READ_10 : MassStorageClassCommon.h
- SCSI_CMD_READ_6 : MassStorageClassCommon.h
- SCSI_CMD_READ_CAPACITY_10 : MassStorageClassCommon.h
- SCSI_CMD_REQUEST_SENSE : MassStorageClassCommon.h
- SCSI_CMD_SEND_DIAGNOSTIC : MassStorageClassCommon.h
- SCSI_CMD_TEST_UNIT_READY : MassStorageClassCommon.h
- SCSI_CMD_VERIFY_10 : MassStorageClassCommon.h
- SCSI_CMD_WRITE_10 : MassStorageClassCommon.h
- SCSI_CMD_WRITE_6 : MassStorageClassCommon.h
- SCSI_Command_Inquiry() : SCSI.c
- SCSI_Command_ModeSense_6() : SCSI.c
- SCSI_Command_Read_Capacity_10() : SCSI.c
- SCSI_Command_ReadWrite_10() : SCSI.c
- SCSI_Command_Request_Sense() : SCSI.c
- SCSI_Command_Send_Diagnostic() : SCSI.c
- SCSI_DecodeSCSICommand() : SCSI.c , SCSI.h
- SCSI_FORMAT_UNIT : usbd_msc.h
- SCSI_INQUIRY : usbd_msc.h
- SCSI_Inquiry_Response_t : MassStorageClassCommon.h
- SCSI_MEDIA_REMOVAL : usbd_msc.h
- SCSI_MODE_SELECT10 : usbd_msc.h
- SCSI_MODE_SELECT6 : usbd_msc.h
- SCSI_MODE_SENSE10 : usbd_msc.h
- SCSI_MODE_SENSE6 : usbd_msc.h
- SCSI_READ10 : usbd_msc.h
- SCSI_READ12 : usbd_msc.h
- SCSI_READ_CAPACITY : usbd_msc.h
- SCSI_READ_FORMAT_CAPACITIES : usbd_msc.h
- SCSI_REQUEST_SENSE : usbd_msc.h
- SCSI_Request_Sense_Response_t : MassStorageClassCommon.h
- SCSI_SENSE_KEY_ABORTED_COMMAND : MassStorageClassCommon.h
- SCSI_SENSE_KEY_BLANK_CHECK : MassStorageClassCommon.h
- SCSI_SENSE_KEY_COPY_ABORTED : MassStorageClassCommon.h
- SCSI_SENSE_KEY_DATA_PROTECT : MassStorageClassCommon.h
- SCSI_SENSE_KEY_GOOD : MassStorageClassCommon.h
- SCSI_SENSE_KEY_HARDWARE_ERROR : MassStorageClassCommon.h
- SCSI_SENSE_KEY_ILLEGAL_REQUEST : MassStorageClassCommon.h
- SCSI_SENSE_KEY_MEDIUM_ERROR : MassStorageClassCommon.h
- SCSI_SENSE_KEY_MISCOMPARE : MassStorageClassCommon.h
- SCSI_SENSE_KEY_NOT_READY : MassStorageClassCommon.h
- SCSI_SENSE_KEY_RECOVERED_ERROR : MassStorageClassCommon.h
- SCSI_SENSE_KEY_UNIT_ATTENTION : MassStorageClassCommon.h
- SCSI_SENSE_KEY_VENDOR_SPECIFIC : MassStorageClassCommon.h
- SCSI_SENSE_KEY_VOLUME_OVERFLOW : MassStorageClassCommon.h
- SCSI_SET_SENSE : SCSI.h
- SCSI_START_STOP_UNIT : usbd_msc.h
- SCSI_TEST_UNIT_READY : usbd_msc.h
- SCSI_VERIFY10 : usbd_msc.h
- SCSI_WRITE10 : usbd_msc.h
- SCSI_WRITE12 : usbd_msc.h
- SCSICommandData : MassStorageClassCommon.h
- SCSICommandLength : MassStorageClassCommon.h
- SCT_CONFIG_16BIT_COUNTER : sct_001.h
- SCT_CONFIG_32BIT_COUNTER : sct_001.h
- SCT_CONFIG_CLKMODE_BUSCLK : sct_001.h
- SCT_CONFIG_CLKMODE_INCLK : sct_001.h
- SCT_CONFIG_CLKMODE_INEDGECLK : sct_001.h
- SCT_CONFIG_CLKMODE_SCTCLK : sct_001.h
- SCT_CONFIG_NORELOADH : sct_001.h
- SCT_CONFIG_NORELOADL_U : sct_001.h
- SCT_CTRL_BIDIR_H : sct_001.h
- SCT_CTRL_BIDIR_L : sct_001.h
- SCT_CTRL_CLRCTR_H : sct_001.h
- SCT_CTRL_CLRCTR_L : sct_001.h
- SCT_CTRL_HALT_H : sct_001.h
- SCT_CTRL_HALT_L : sct_001.h
- SCT_CTRL_PRE_H : sct_001.h
- SCT_CTRL_PRE_L : sct_001.h
- SCT_CTRL_STOP_H : sct_001.h
- SCT_CTRL_STOP_L : sct_001.h
- SCT_EVT_0 : sct_8xx.h
- SCT_EVT_1 : sct_8xx.h
- SCT_EVT_2 : sct_8xx.h
- SCT_EVT_3 : sct_8xx.h
- SCT_EVT_4 : sct_8xx.h
- sct_fsm_init() : sct_fsm_keil_mcb_18574357.c , sct_fsm.h , sct_fsm_ngx_xplorer_18304330.c , sct_fsm.h , sct_fsm_hitex_eva_18504350.c , sct_fsm.h , sct_fsm_keil_mcb_18574357.c , sct_fsm.h , sct_fsm_hitex_eva_18504350.c , sct_fsm.h , sct_fsm_keil_mcb_18574357.c , sct_fsm.h , sct_fsm_hitex_eva_18504350.c , sct_fsm.h
- SCT_INPUT_CROSS_REQUEST : sct_fsm.h
- SCT_INPUT_DOWN : sct_fsm.h
- SCT_INPUT_RESET : sct_fsm.h
- SCT_IRQ_EVENT_crossingTimeout : sct_fsm.h
- SCT_IRQHandler() : sct_blinky.c , sct_trafficlight.c , sct.c
- SCT_MATCH_0 : sct_8xx.h
- SCT_MATCH_1 : sct_8xx.h
- SCT_MATCH_2 : sct_8xx.h
- SCT_MATCH_3 : sct_8xx.h
- SCT_MATCH_4 : sct_8xx.h
- SCT_OUTPUT_AUTO_CROSS : sct_fsm.h
- SCT_OUTPUT_BLUE_N : sct_fsm.h
- SCT_OUTPUT_CTOUT0 : sct_fsm.h
- SCT_OUTPUT_CTOUT1 : sct_fsm.h
- SCT_OUTPUT_CTOUT2 : sct_fsm.h
- SCT_OUTPUT_CTOUT3 : sct_fsm.h
- SCT_OUTPUT_GREEN_N : sct_fsm.h
- SCT_OUTPUT_JUMP_SIGNAL : sct_fsm.h
- SCT_OUTPUT_LED1 : sct_fsm.h
- SCT_OUTPUT_LED2 : sct_fsm.h
- SCT_OUTPUT_LED3 : sct_fsm.h
- SCT_OUTPUT_LED4 : sct_fsm.h
- SCT_OUTPUT_RED_N : sct_fsm.h
- SCT_OUTPUT_REQUEST : sct_fsm.h
- SCT_OUTPUTPRELOAD_AUTO_CROSS : sct_fsm.h
- SCT_OUTPUTPRELOAD_BLUE_N : sct_fsm.h
- SCT_OUTPUTPRELOAD_CTOUT0 : sct_fsm.h
- SCT_OUTPUTPRELOAD_CTOUT1 : sct_fsm.h
- SCT_OUTPUTPRELOAD_CTOUT2 : sct_fsm.h
- SCT_OUTPUTPRELOAD_CTOUT3 : sct_fsm.h
- SCT_OUTPUTPRELOAD_GREEN_N : sct_fsm.h
- SCT_OUTPUTPRELOAD_JUMP_SIGNAL : sct_fsm.h
- SCT_OUTPUTPRELOAD_LED1 : sct_fsm.h
- SCT_OUTPUTPRELOAD_LED2 : sct_fsm.h
- SCT_OUTPUTPRELOAD_LED3 : sct_fsm.h
- SCT_OUTPUTPRELOAD_LED4 : sct_fsm.h
- SCT_OUTPUTPRELOAD_RED_N : sct_fsm.h
- SCT_OUTPUTPRELOAD_REQUEST : sct_fsm.h
- SCT_PinsConfigure() : sct_blinky.c , sct_simple_match.c , sct_trafficlight.c
- SCT_RES_CLEAR_OUTPUT : sct_001.h
- SCT_RES_NOCHANGE : sct_001.h
- SCT_RES_SET_OUTPUT : sct_001.h
- SCT_RES_TOGGLE_OUTPUT : sct_001.h
- SCU_MODE_14MA_DRIVESTR : scu_18xx_43xx.h
- SCU_MODE_20MA_DRIVESTR : scu_18xx_43xx.h
- SCU_MODE_4MA_DRIVESTR : scu_18xx_43xx.h
- SCU_MODE_8MA_DRIVESTR : scu_18xx_43xx.h
- SCU_MODE_FUNC0 : scu_18xx_43xx.h
- SCU_MODE_FUNC1 : scu_18xx_43xx.h
- SCU_MODE_FUNC2 : scu_18xx_43xx.h
- SCU_MODE_FUNC3 : scu_18xx_43xx.h
- SCU_MODE_FUNC4 : scu_18xx_43xx.h
- SCU_MODE_FUNC5 : scu_18xx_43xx.h
- SCU_MODE_FUNC6 : scu_18xx_43xx.h
- SCU_MODE_FUNC7 : scu_18xx_43xx.h
- SCU_MODE_HIGHSPEEDSLEW_EN : scu_18xx_43xx.h
- SCU_MODE_INBUFF_EN : scu_18xx_43xx.h
- SCU_MODE_MODE_INACT : scu_18xx_43xx.h
- SCU_MODE_MODE_PULLDOWN : scu_18xx_43xx.h
- SCU_MODE_MODE_PULLUP : scu_18xx_43xx.h
- SCU_MODE_MODE_REPEATER : scu_18xx_43xx.h
- SCU_MODE_ZIF_DIS : scu_18xx_43xx.h
- SCU_PINIO_FAST : scu_18xx_43xx.h
- SD_ACMD13_SEND_SD_STATUS : sdmmc_17xx_40xx.h
- SD_ACMD41_SD_SEND_OP_COND : sdmmc_17xx_40xx.h
- SD_ACMD6_SET_BUS_WIDTH : sdmmc_17xx_40xx.h
- SD_APP_CMD_T : lpc_sdmmc.h
- SD_APP_OP_COND : lpc_sdmmc.h
- SD_APP_SEND_SCR : lpc_sdmmc.h
- SD_APP_SET_BUS_WIDTH : lpc_sdmmc.h
- SD_CLEAR_CARD_DET : lpc_sdmmc.h
- SD_CMD12_STOP_TRANSMISSION : sdmmc_17xx_40xx.h
- SD_CMD13_SEND_STATUS : sdmmc_17xx_40xx.h
- SD_CMD16_SET_BLOCKLEN : sdmmc_17xx_40xx.h
- SD_CMD17_READ_SINGLE_BLOCK : sdmmc_17xx_40xx.h
- SD_CMD18_READ_MULTIPLE_BLOCK : sdmmc_17xx_40xx.h
- SD_CMD1_SEND_OP_COND : sdmmc_17xx_40xx.h
- SD_CMD24_WRITE_BLOCK : sdmmc_17xx_40xx.h
- SD_CMD25_WRITE_MULTIPLE_BLOCK : sdmmc_17xx_40xx.h
- SD_CMD2_ALL_SEND_CID : sdmmc_17xx_40xx.h
- SD_CMD32_ERASE_WR_BLK_START : sdmmc_17xx_40xx.h
- SD_CMD33_ERASE_WR_BLK_END : sdmmc_17xx_40xx.h
- SD_CMD38_ERASE : sdmmc_17xx_40xx.h
- SD_CMD3_SEND_RELATIVE_ADDR : sdmmc_17xx_40xx.h
- SD_CMD3_SET_RELATIVE_ADDR : sdmmc_17xx_40xx.h
- SD_CMD55_APP_CMD : sdmmc_17xx_40xx.h
- SD_CMD7_SELECT_CARD : sdmmc_17xx_40xx.h
- SD_CMD8 : lpc_sdmmc.h
- SD_CMD8_SEND_IF_COND : sdmmc_17xx_40xx.h
- SD_CMD9_SEND_CSD : sdmmc_17xx_40xx.h
- SD_ERASE : lpc_sdmmc.h
- SD_ERASE_WR_BLK_END : lpc_sdmmc.h
- SD_ERASE_WR_BLK_START : lpc_sdmmc.h
- SD_FIFO_SZ : sdmmc_001.h
- SD_GO_IDLE_STATE : sdmmc_17xx_40xx.h
- SD_INT_ERROR : sdmmc_18xx_43xx.c
- SD_INVALID_APP_CMD : lpc_sdmmc.h
- SD_MAX_CLOCK : sdif_18xx_43xx.h
- SD_MMC_ENUM_CLOCK : sdif_18xx_43xx.h
- SD_SEND_IF_ARG : lpc_sdmmc.h
- SD_SEND_IF_ECHO_MSK : lpc_sdmmc.h
- SD_SEND_IF_RESP : lpc_sdmmc.h
- SD_SEND_RELATIVE_ADDR : lpc_sdmmc.h
- SD_SEND_SCR : lpc_sdmmc.h
- SD_SEND_STATUS : lpc_sdmmc.h
- SD_SEND_WR_BLOCKS : lpc_sdmmc.h
- SD_SENDOP_COND : lpc_sdmmc.h
- SD_SET_BUS_WIDTH : lpc_sdmmc.h
- SD_SET_ERASE_COUNT : lpc_sdmmc.h
- SDC_BLOCK_SIZE_1 : sdc_001.h
- SDC_BLOCK_SIZE_1024 : sdc_001.h
- SDC_BLOCK_SIZE_128 : sdc_001.h
- SDC_BLOCK_SIZE_16 : sdc_001.h
- SDC_BLOCK_SIZE_2 : sdc_001.h
- SDC_BLOCK_SIZE_2048 : sdc_001.h
- SDC_BLOCK_SIZE_256 : sdc_001.h
- SDC_BLOCK_SIZE_32 : sdc_001.h
- SDC_BLOCK_SIZE_4 : sdc_001.h
- SDC_BLOCK_SIZE_512 : sdc_001.h
- SDC_BLOCK_SIZE_64 : sdc_001.h
- SDC_BLOCK_SIZE_8 : sdc_001.h
- SDC_CARDSTATUS_BYTENUM : sdc_001.h
- SDC_CLEAR_ALL : sdc_001.h
- SDC_CLEAR_CMDCRCFAIL : sdc_001.h
- SDC_CLEAR_CMDRESPEND : sdc_001.h
- SDC_CLEAR_CMDSENT : sdc_001.h
- SDC_CLEAR_CMDTIMEOUT : sdc_001.h
- SDC_CLEAR_DATABLOCKEND : sdc_001.h
- SDC_CLEAR_DATACRCFAIL : sdc_001.h
- SDC_CLEAR_DATAEND : sdc_001.h
- SDC_CLEAR_DATATIMEOUT : sdc_001.h
- SDC_CLEAR_RXOVERRUN : sdc_001.h
- SDC_CLEAR_STARTBITERR : sdc_001.h
- SDC_CLEAR_TXUNDERRUN : sdc_001.h
- SDC_CLOCK_BITMASK : sdc_001.h
- SDC_CLOCK_CLKDIV : sdc_001.h
- SDC_CLOCK_CLKDIV_BITMASK : sdc_001.h
- SDC_CLOCK_DIVIDER_BYPASS : sdc_001.h
- SDC_CLOCK_ENABLE : sdc_001.h
- SDC_CLOCK_POWER_SAVE : sdc_001.h
- SDC_CLOCK_WIDEBUS_MODE : sdc_001.h
- SDC_COMMAND_BITMASK : sdc_001.h
- SDC_COMMAND_ENABLE : sdc_001.h
- SDC_COMMAND_INDEX : sdc_001.h
- SDC_COMMAND_INDEX_BITMASK : sdc_001.h
- SDC_COMMAND_INTERRUPT : sdc_001.h
- SDC_COMMAND_LONG_RSP : sdc_001.h
- SDC_COMMAND_NO_RSP : sdc_001.h
- SDC_COMMAND_PENDING : sdc_001.h
- SDC_COMMAND_RSP_BITMASK : sdc_001.h
- SDC_COMMAND_SHORT_RSP : sdc_001.h
- SDC_DATACNT_VAL : sdc_001.h
- SDC_DATACTRL_BITMASK : sdc_001.h
- SDC_DATACTRL_BLOCKSIZE : sdc_001.h
- SDC_DATACTRL_BLOCKSIZE_VAL : sdc_001.h
- SDC_DATACTRL_DIR_FROMCARD : sdc_001.h
- SDC_DATACTRL_DIR_TOCARD : sdc_001.h
- SDC_DATACTRL_DMA_ENABLE : sdc_001.h
- SDC_DATACTRL_ENABLE : sdc_001.h
- SDC_DATACTRL_XFER_MODE_BLOCK : sdc_001.h
- SDC_DATACTRL_XFER_MODE_STREAM : sdc_001.h
- SDC_DATALENGTH_LEN : sdc_001.h
- SDC_DMA_ENABLE : sys_config.h
- SDC_FIFOCNT_VAL : sdc_001.h
- SDC_IDENT_CLOCK_RATE : sdmmc_17xx_40xx.h
- SDC_LONG_RESPONSE : sdc_001.h
- SDC_MASK0_CMDACTIVE : sdc_001.h
- SDC_MASK0_CMDCRCFAIL : sdc_001.h
- SDC_MASK0_CMDERR : sdc_001.h
- SDC_MASK0_CMDRESPEND : sdc_001.h
- SDC_MASK0_CMDSENT : sdc_001.h
- SDC_MASK0_CMDTIMEOUT : sdc_001.h
- SDC_MASK0_DATA : sdc_001.h
- SDC_MASK0_DATABLOCKEND : sdc_001.h
- SDC_MASK0_DATACRCFAIL : sdc_001.h
- SDC_MASK0_DATAEND : sdc_001.h
- SDC_MASK0_DATATIMEOUT : sdc_001.h
- SDC_MASK0_RXACTIVE : sdc_001.h
- SDC_MASK0_RXDATAAVLBL : sdc_001.h
- SDC_MASK0_RXDATAERR : sdc_001.h
- SDC_MASK0_RXFIFO : sdc_001.h
- SDC_MASK0_RXFIFOEMPTY : sdc_001.h
- SDC_MASK0_RXFIFOFULL : sdc_001.h
- SDC_MASK0_RXFIFOHALFFULL : sdc_001.h
- SDC_MASK0_RXOVERRUN : sdc_001.h
- SDC_MASK0_STARTBITERR : sdc_001.h
- SDC_MASK0_TXACTIVE : sdc_001.h
- SDC_MASK0_TXDATAAVLBL : sdc_001.h
- SDC_MASK0_TXDATAERR : sdc_001.h
- SDC_MASK0_TXFIFO : sdc_001.h
- SDC_MASK0_TXFIFOEMPTY : sdc_001.h
- SDC_MASK0_TXFIFOFULL : sdc_001.h
- SDC_MASK0_TXFIFOHALFEMPTY : sdc_001.h
- SDC_MASK0_TXUNDERRUN : sdc_001.h
- SDC_NO_RESPONSE : sdc_001.h
- SDC_OCR_20_21 : lpc_sdmmc.h
- SDC_OCR_21_22 : lpc_sdmmc.h
- SDC_OCR_22_23 : lpc_sdmmc.h
- SDC_OCR_23_24 : lpc_sdmmc.h
- SDC_OCR_24_25 : lpc_sdmmc.h
- SDC_OCR_25_26 : lpc_sdmmc.h
- SDC_OCR_26_27 : lpc_sdmmc.h
- SDC_OCR_27_28 : lpc_sdmmc.h
- SDC_OCR_27_36 : lpc_sdmmc.h
- SDC_OCR_28_29 : lpc_sdmmc.h
- SDC_OCR_29_30 : lpc_sdmmc.h
- SDC_OCR_30_31 : lpc_sdmmc.h
- SDC_OCR_31_32 : lpc_sdmmc.h
- SDC_OCR_32_33 : lpc_sdmmc.h
- SDC_OCR_33_34 : lpc_sdmmc.h
- SDC_OCR_34_35 : lpc_sdmmc.h
- SDC_OCR_35_36 : lpc_sdmmc.h
- SDC_OCR_BUSY : lpc_sdmmc.h
- SDC_OCR_HC_CCS : lpc_sdmmc.h
- SDC_OCR_IDLE : lpc_sdmmc.h
- SDC_POWER_OFF : sdc_001.h
- SDC_POWER_ON : sdc_001.h
- SDC_POWER_UP : sdc_001.h
- SDC_PWR_BITMASK : sdc_001.h
- SDC_PWR_CTRL : sdc_001.h
- SDC_PWR_CTRL_BITMASK : sdc_001.h
- SDC_PWR_OPENDRAIN : sdc_001.h
- SDC_PWR_ROD : sdc_001.h
- SDC_RESPCOMMAND_VAL : sdc_001.h
- SDC_RET_BAD_PARAMETERS : sdc_17xx_40xx.h
- SDC_RET_BUS_NOT_IDLE : sdc_17xx_40xx.h
- SDC_RET_CMD_FAILED : sdc_17xx_40xx.h
- SDC_RET_ERR_STATE : sdc_17xx_40xx.h
- SDC_RET_FAILED : sdc_17xx_40xx.h
- SDC_RET_NOT_READY : sdc_17xx_40xx.h
- SDC_RET_OK : sdc_17xx_40xx.h
- SDC_RET_TIMEOUT : sdc_17xx_40xx.h
- SDC_SHORT_RESPONSE : sdc_001.h
- SDC_STATUS_CMDACTIVE : sdc_001.h
- SDC_STATUS_CMDCRCFAIL : sdc_001.h
- SDC_STATUS_CMDERR : sdc_001.h
- SDC_STATUS_CMDRESPEND : sdc_001.h
- SDC_STATUS_CMDSENT : sdc_001.h
- SDC_STATUS_CMDTIMEOUT : sdc_001.h
- SDC_STATUS_DATA : sdc_001.h
- SDC_STATUS_DATABLOCKEND : sdc_001.h
- SDC_STATUS_DATACRCFAIL : sdc_001.h
- SDC_STATUS_DATAEND : sdc_001.h
- SDC_STATUS_DATAERR : sdc_001.h
- SDC_STATUS_DATATIMEOUT : sdc_001.h
- SDC_STATUS_FIFO : sdc_001.h
- SDC_STATUS_RXACTIVE : sdc_001.h
- SDC_STATUS_RXDATAAVLBL : sdc_001.h
- SDC_STATUS_RXFIFOEMPTY : sdc_001.h
- SDC_STATUS_RXFIFOFULL : sdc_001.h
- SDC_STATUS_RXFIFOHALFFULL : sdc_001.h
- SDC_STATUS_RXOVERRUN : sdc_001.h
- SDC_STATUS_STARTBITERR : sdc_001.h
- SDC_STATUS_TXACTIVE : sdc_001.h
- SDC_STATUS_TXDATAAVLBL : sdc_001.h
- SDC_STATUS_TXFIFOEMPTY : sdc_001.h
- SDC_STATUS_TXFIFOFULL : sdc_001.h
- SDC_STATUS_TXFIFOHALFEMPTY : sdc_001.h
- SDC_STATUS_TXUNDERRUN : sdc_001.h
- SDC_TRAN_CLOCK_RATE : sdmmc_17xx_40xx.h
- SDC_TRANSFER_DIR_FROMCARD : sdc_001.h
- SDC_TRANSFER_DIR_TOCARD : sdc_001.h
- SDC_TRANSFER_MODE_BLOCK : sdc_001.h
- SDC_TRANSFER_MODE_STREAM : sdc_001.h
- sdCardInfo : fsmci_cfg.h , sdmmc.c
- sdcardinfo : fsmci_cfg.h , lwip_fs.c , fsmci_cfg.h , sdmmc.c
- sdcWaitExit : sdmmc.c
- SDIO_BUS_WIDTH : sdif_18xx_43xx.h
- SDIO_IRQHandler() : lwip_fs.c , app_sdmmc_meas.c , sdmmc.c
- sdio_wait_exit : lwip_fs.c , sdmmc.c
- SDMMC_DATA_ST : lpc_sdmmc.h
- SDMMC_DIS_ST : lpc_sdmmc.h
- SDMMC_EVSETUP_FUNC_T : lpc_sdmmc.h
- SDMMC_EVWAIT_FUNC_T : lpc_sdmmc.h
- sdmmc_execute_command() : sdmmc_18xx_43xx.c
- SDMMC_IDENT_ST : lpc_sdmmc.h
- SDMMC_IDLE_ST : lpc_sdmmc.h
- sdmmc_irq_driven_wait() : lwip_fs.c , app_sdmmc_meas.c , sdmmc.c
- SDMMC_MSDELAY_FUNC_T : lpc_sdmmc.h
- SDMMC_PRG_ST : lpc_sdmmc.h
- SDMMC_RCV_ST : lpc_sdmmc.h
- SDMMC_READY_ST : lpc_sdmmc.h
- SDMMC_RESPONSE_NONE : lpc_sdmmc.h
- SDMMC_RESPONSE_R1 : lpc_sdmmc.h
- SDMMC_RESPONSE_R1B : lpc_sdmmc.h
- SDMMC_RESPONSE_R2 : lpc_sdmmc.h
- SDMMC_RESPONSE_R3 : lpc_sdmmc.h
- SDMMC_RESPONSE_R4 : lpc_sdmmc.h
- SDMMC_RESPONSE_R5 : lpc_sdmmc.h
- SDMMC_RESPONSE_R6 : lpc_sdmmc.h
- SDMMC_RESPONSE_T : lpc_sdmmc.h
- sdmmc_setup_wakeup() : lwip_fs.c , app_sdmmc_meas.c , sdmmc.c
- SDMMC_STATE_T : lpc_sdmmc.h
- SDMMC_STBY_ST : lpc_sdmmc.h
- SDMMC_TRAN_ST : lpc_sdmmc.h
- sdmmc_waitms() : lwip_fs.c , sdmmc.c
- SDO_ABORT_ACCINCOMP : ccand_11xx.h
- SDO_ABORT_DEVSTAT : ccand_11xx.h
- SDO_ABORT_LOCAL : ccand_11xx.h
- SDO_ABORT_NOT_EXISTS : ccand_11xx.h
- SDO_ABORT_PARAINCOMP : ccand_11xx.h
- SDO_ABORT_READONLY : ccand_11xx.h
- SDO_ABORT_SDOTIMEOUT : ccand_11xx.h
- SDO_ABORT_TOGGLE : ccand_11xx.h
- SDO_ABORT_TRANSFER : ccand_11xx.h
- SDO_ABORT_TYPEMISMATCH : ccand_11xx.h
- SDO_ABORT_UNKNOWN_COMMAND : ccand_11xx.h
- SDO_ABORT_UNKNOWNSUB : ccand_11xx.h
- SDO_ABORT_UNSUPPORTED : ccand_11xx.h
- SDO_ABORT_VALUE_RANGE : ccand_11xx.h
- SDO_ABORT_WRITEONLY : ccand_11xx.h
- searchInsertIndex() : can_001.c
- SECTOR_NOT_BLANK : flash_001.h
- SECTOR_NOT_PREPARED_FOR_WRITE_OPERATION : flash_001.h
- SECTOR_SIZE : lpc_norflash_sst39vf320.c
- SECTOR_SZ : fs_mem.h
- sectorinfo : dfuutil_programming_iflash_algorithm.c
- SECTORSPERCLUSTER : fatutil.h
- SectorsPerFat : fatutil.c , fatutil.h
- SECTORSPERFAT : fatutil.h
- seep_data : i2c.c
- seep_xfer : i2c.c
- SegmentNumber : MassStorageClassCommon.h
- selectCard() : sdmmc_17xx_40xx.c
- SelectMenu : adc.c , dac.c , adc.c , dac.c
- send_flag : i2s.c
- sendAppCmd() : sdmmc_17xx_40xx.c
- sendAppOpCond() : sdmmc_17xx_40xx.c
- sendCmd() : sdmmc_17xx_40xx.c
- sendCompleted : uart.c
- sendIfCond() : sdmmc_17xx_40xx.c
- sendOpCond() : sdmmc_17xx_40xx.c
- SenseData : SCSI.c
- SenseKey : MassStorageClassCommon.h
- SenseKeySpecific : MassStorageClassCommon.h
- SERIAL_CFG_ARG_CHK_EXT_EN : serial_cfg.h
- SERIAL_CFG_MAX_NBR_IF : serial_cfg.h
- SERIAL_CFG_RD_BUF_EN : serial_cfg.h
- SERIAL_CFG_TX_DESC_NBR : serial_cfg.h
- SERIAL_CFG_WR_BUF_EN : serial_cfg.h
- Serial_CreateStream() : board_ea_devkit_17884088.c , board_ea_devkit_17884088.h , board_nxp_xpresso_1769.c , board_nxp_xpresso_1769.h , board_hitex_eva_18504350.c , board_hitex_eva_18504350.h , board_keil_mcb_18574357.c , board_keil_mcb_18574357.h , board_ngx_xplorer_18304330.c , board_ngx_xplorer_18304330.h
- SerialNumStrIndex : StdDescriptors.h
- SET : lpc_types.h
- SET_OP_RETRIES : sdif_18xx_43xx.h
- setAddr() : sdmmc_17xx_40xx.c
- setblock_length() : sdmmc_17xx_40xx.c
- setBusWidth() : sdmmc_17xx_40xx.c
- setCardParams() : sdmmc_17xx_40xx.c
- SetDiskMetricsFromDiskImage() : fatutil.c , fatutil.h
- SETENAF : pinint_8xx.h
- SETENRL : pinint_8xx.h
- SetFAT12Entry() : fatutil.c , fatutil.h
- SetGlobalInterruptMask() : Common.h
- setSectionEndAddress() : can_001.c
- setSendFrameInfo() : can_001.c
- SetState : lpc_types.h
- setTranState() : sdmmc_17xx_40xx.c
- SETUP_TRANSFER : HCD.h
- SetupAFLUT() : can.c
- setupEvWakeup() : sdmmc.c
- setupEXTRangeSection() : can_001.c
- setupEXTSection() : can_001.c
- SetupHardware() : AudioOutput.c , AudioOutput.h , AudioOutput.c , AudioOutputHost.c , GenericHID.c , Keyboard.c , KeyboardHost.c , MassStorage.c , MassStorageHost.c , Mouse.c , VirtualSerial.c
- setupSTDRangeSection() : can_001.c
- setupSTDSection() : can_001.c
- SffGrpSection : can.c
- SFFSection : can.c
- SHARED_MEM_M0 : lpc43xx_dualcore_config.h
- SHARED_MEM_M4 : lpc43xx_dualcore_config.h
- shiftSTDEntryDown() : can_001.c
- shiftSTDEntryUp() : can_001.c
- SHMEMM0 : ipc_msg.c
- SHMEMM4 : ipc_msg.c
- SHORT : integer.h
- ShowString() : eeprom.c , nandflash.c , norflash.c , eeprom.c
- showTime() : rtc.c , rtc_ev.c
- showTimeStamp() : rtc_ev.c
- SI_CSCP_BulkOnlyProtocol : StillImageClassCommon.h
- SI_CSCP_StillImageClass : StillImageClassCommon.h
- SI_CSCP_StillImageSubclass : StillImageClassCommon.h
- SI_Descriptor_ClassSubclassProtocol_t : StillImageClassCommon.h
- SI_ENUMERROR_InvalidConfigDescriptor : StillImageClassHost.h
- SI_ENUMERROR_NoCompatibleInterfaceFound : StillImageClassHost.h
- SI_ENUMERROR_NoError : StillImageClassHost.h
- SI_ENUMERROR_PipeConfigurationFailed : StillImageClassHost.h
- SI_ERROR_LOGICAL_CMD_FAILED : StillImageClassHost.h
- SI_Host_CloseSession() : StillImageClassHost.c , StillImageClassHost.h
- SI_Host_ConfigurePipes() : StillImageClassHost.c , StillImageClassHost.h
- SI_Host_EnumerationFailure_ErrorCodes_t : StillImageClassHost.h
- SI_Host_IsEventReceived() : StillImageClassHost.c , StillImageClassHost.h
- SI_Host_OpenSession() : StillImageClassHost.c , StillImageClassHost.h
- SI_Host_ReadData() : StillImageClassHost.c , StillImageClassHost.h
- SI_Host_ReceiveBlockHeader() : StillImageClassHost.c , StillImageClassHost.h
- SI_Host_ReceiveEventHeader() : StillImageClassHost.c , StillImageClassHost.h
- SI_Host_ReceiveResponse() : StillImageClassHost.c , StillImageClassHost.h
- SI_Host_SendBlockHeader() : StillImageClassHost.c , StillImageClassHost.h
- SI_Host_SendCommand() : StillImageClassHost.c , StillImageClassHost.h
- SI_Host_SendData() : StillImageClassHost.c , StillImageClassHost.h
- SI_Host_USBTask() : StillImageClassHost.h
- SIE_ReadCommandData() : HAL_LPC17xx.h
- Signature : MassStorageClassCommon.h
- SIGNATURE_M0_MAGIC : m0_ImageLoader.c
- SIGNATURE_M4_MAGIC : m0_ImageLoader.c
- SITD_TYPE : EHCI.h
- Size : StdDescriptors.h
- Skip : OHCI.h
- SLAVE_ACTIVE : i2c_11xx.c , i2c_13xx.c , i2c_17xx_40xx.c , i2c_18xx_43xx.c
- SLAVE_RECEIVE : i2cd_8xx.h
- SLAVE_SEND : i2cd_8xx.h
- SlaveInterfaceNumber : CDCClassCommon.h
- smsc_update_phy_sts() : lpc_phy_smsc87x0.c
- SOF_INTERRUPT : OHCI.h
- SoftReset : MassStorageClassCommon.h
- SourceID : AudioClassCommon.h
- SourceJackID : MIDIClassCommon.h
- SourcePinID : MIDIClassCommon.h
- Speaker_Audio_Interface : AudioOutput.c , AudioOutputHost.c
- speed : sct_user.h
- Speed : OHCI.h
- SPEED_100KHZ : i2c.c
- SPEED_400KHZ : i2c.c
- SPI0_IRQHandler() : cr_freertos_startup_lpc8xx.c , cr_startup_8xx.c
- SPI_BITS_10 : spi_001.h
- SPI_BITS_11 : spi_001.h
- SPI_BITS_12 : spi_001.h
- SPI_BITS_13 : spi_001.h
- SPI_BITS_14 : spi_001.h
- SPI_BITS_15 : spi_001.h
- SPI_BITS_16 : spi_001.h
- SPI_BITS_8 : spi_001.h
- SPI_BITS_9 : spi_001.h
- SPI_CFG_BITMASK : spi_002.h
- SPI_CFG_CPHA_FIRST : spi_002.h
- SPI_CFG_CPHA_SECOND : spi_002.h
- SPI_CFG_CPOL_HI : spi_002.h
- SPI_CFG_CPOL_LO : spi_002.h
- SPI_CFG_LBM_EN : spi_002.h
- SPI_CFG_LSB_FIRST_EN : spi_002.h
- SPI_CFG_MASTER_EN : spi_002.h
- SPI_CFG_MSB_FIRST_EN : spi_002.h
- SPI_CFG_SLAVE_EN : spi_002.h
- SPI_CFG_SPI_EN : spi_002.h
- SPI_CFG_SPOL_HI : spi_002.h
- SPI_CFG_SPOL_LO : spi_002.h
- SPI_CLOCK_CPHA0_CPOL0 : spi_001.h , spi_002.h
- SPI_CLOCK_CPHA0_CPOL1 : spi_001.h , spi_002.h
- SPI_CLOCK_CPHA1_CPOL0 : spi_001.h , spi_002.h
- SPI_CLOCK_CPHA1_CPOL1 : spi_001.h , spi_002.h
- SPI_CLOCK_MODE0 : spi_001.h , spi_002.h
- SPI_CLOCK_MODE1 : spi_001.h , spi_002.h
- SPI_CLOCK_MODE2 : spi_001.h , spi_002.h
- SPI_CLOCK_MODE3 : spi_001.h , spi_002.h
- SPI_CONFIG_T : spi_8xx.h
- SPI_CR_BIT_EN : spi_001.h
- SPI_CR_BITMASK : spi_001.h
- SPI_CR_BITS : spi_001.h
- SPI_CR_BITS_MASK : spi_001.h
- SPI_CR_CPHA_FIRST : spi_001.h
- SPI_CR_CPHA_SECOND : spi_001.h
- SPI_CR_CPOL_HI : spi_001.h
- SPI_CR_CPOL_LO : spi_001.h
- SPI_CR_INT_EN : spi_001.h
- SPI_CR_LSB_FIRST_EN : spi_001.h
- SPI_CR_MASTER_EN : spi_001.h
- SPI_CR_MSB_FIRST_EN : spi_001.h
- SPI_CR_SLAVE_EN : spi_001.h
- SPI_DATA_LSB_FIRST : spi_001.h , spi_002.h
- SPI_DATA_MSB_FIRST : spi_001.h , spi_002.h
- SPI_DELAY_CONFIG_T : spi_8xx.h
- SPI_DIV_VAL : spi_002.h
- SPI_DLY_BITMASK : spi_002.h
- SPI_DLY_FRAME_DELAY : spi_002.h
- SPI_DLY_POST_DELAY : spi_002.h
- SPI_DLY_PRE_DELAY : spi_002.h
- SPI_DLY_TRANSFER_DELAY : spi_002.h
- SPI_DR_DATA : spi_001.h
- spi_format : spi.c
- SPI_INT_SPIF : spi_001.h
- SPI_INTENCLR_BITMASK : spi_002.h
- SPI_INTENCLR_RXDYEN : spi_002.h
- SPI_INTENCLR_RXOVEN : spi_002.h
- SPI_INTENCLR_SSAEN : spi_002.h
- SPI_INTENCLR_SSDEN : spi_002.h
- SPI_INTENCLR_TXDYEN : spi_002.h
- SPI_INTENCLR_TXUREN : spi_002.h
- SPI_INTENSET_BITMASK : spi_002.h
- SPI_INTENSET_RXDYEN : spi_002.h
- SPI_INTENSET_RXOVEN : spi_002.h
- SPI_INTENSET_SSAEN : spi_002.h
- SPI_INTENSET_SSDEN : spi_002.h
- SPI_INTENSET_TXDYEN : spi_002.h
- SPI_INTENSET_TXUREN : spi_002.h
- SPI_INTERRUPT_SEL : spi.c
- SPI_INTSTAT_BITMASK : spi_002.h
- SPI_INTSTAT_RXOV : spi_002.h
- SPI_INTSTAT_RXRDY : spi_002.h
- SPI_INTSTAT_SSA : spi_002.h
- SPI_INTSTAT_SSD : spi_002.h
- SPI_INTSTAT_TXRDY : spi_002.h
- SPI_INTSTAT_TXUR : spi_002.h
- SPI_IRQ : spi.c
- SPI_MASTER_MODE_SEL : spi.c
- SPI_MODE_MASTER : spi_001.h , spi_002.h
- SPI_MODE_SEL : spi.c
- SPI_MODE_SLAVE : spi_001.h , spi_002.h
- SPI_MODE_TEST : spi.c
- SPI_POLLING_SEL : spi.c
- SPI_Receive_Data() : spi_8xx.c
- spi_rx_buf : spi.c
- SPI_RXDAT_BITMASK : spi_002.h
- SPI_RXDAT_DATA : spi_002.h
- SPI_RXDAT_RXSSELN_ACTIVE : spi_002.h
- SPI_RXDAT_RXSSELN_INACTIVE : spi_002.h
- SPI_RXDAT_SOT : spi_002.h
- SPI_Send_Data() : spi_8xx.c
- SPI_Send_Data_RxIgnore() : spi_8xx.c
- SPI_Send_Dummy() : spi_8xx.c
- SPI_SLAVE_MODE_SEL : spi.c
- SPI_SR_ABRT : spi_001.h
- SPI_SR_BITMASK : spi_001.h
- SPI_SR_ERROR : spi_001.h
- SPI_SR_MODF : spi_001.h
- SPI_SR_ROVR : spi_001.h
- SPI_SR_SPIF : spi_001.h
- SPI_SR_WCOL : spi_001.h
- SPI_SSEL_ACTIVE_HI : spi_002.h
- SPI_SSEL_ACTIVE_LO : spi_002.h
- SPI_STAT_BITMASK : spi_002.h
- SPI_STAT_CLR_RXOV : spi_002.h
- SPI_STAT_CLR_SSA : spi_002.h
- SPI_STAT_CLR_SSD : spi_002.h
- SPI_STAT_CLR_TXUR : spi_002.h
- SPI_STAT_EOT : spi_002.h
- SPI_STAT_FORCE_EOT : spi_002.h
- SPI_STAT_LE : spi_002.h
- SPI_STAT_RXOV : spi_002.h
- SPI_STAT_RXRDY : spi_002.h
- SPI_STAT_SSA : spi_002.h
- SPI_STAT_SSD : spi_002.h
- SPI_STAT_STALLED : spi_002.h
- SPI_STAT_TXRDY : spi_002.h
- SPI_STAT_TXUR : spi_002.h
- SPI_TCR_TEST : spi_001.h
- SPI_TRANSFER_MODE_SEL : spi.c
- spi_tx_buf : spi.c
- SPI_TXCTL_ASSERT_SSEL : spi_002.h
- SPI_TXCTL_BITMASK : spi_002.h
- SPI_TXCTL_DEASSERT_SSEL : spi_002.h
- SPI_TXCTL_EOF : spi_002.h
- SPI_TXCTL_EOT : spi_002.h
- SPI_TXCTL_FLEN : spi_002.h
- SPI_TXCTL_RXIGNORE : spi_002.h
- SPI_TXDAT_DATA : spi_002.h
- SPI_TXDATCTL_ASSERT_SSEL : spi_002.h
- SPI_TXDATCTL_BITMASK : spi_002.h
- SPI_TXDATCTL_DATA : spi_002.h
- SPI_TXDATCTL_DEASSERT_SSEL : spi_002.h
- SPI_TXDATCTL_EOF : spi_002.h
- SPI_TXDATCTL_EOT : spi_002.h
- SPI_TXDATCTL_FLEN : spi_002.h
- SPI_TXDATCTL_RXIGNORE : spi_002.h
- spi_xf : spi.c
- spi_xfer_completed : spi.c
- SPIFI_BASE_ADDR : lpc43xx_dualcore_config.h
- spifi_obj : main.c
- spifi_rom_init : flash_config.h
- SPIFI_ROM_PTR : spifi_17xx_40xx.h
- SPIFI_WRITE_SECTOR_ADDRESS : flash_config.h
- SPIFI_WRITE_SECTOR_OFFSET : flash_config.h
- spifipinmuxing : sysinit_hitex_eva_18504350.c , sysinit_keil_mcb_18574357.c , sysinit_ngx_xplorer_18304330.c , dfuutil_programming_spiiflash_systeminit.c
- SPIFLASH_BASE_ADDRESS : spifi_17xx_40xx.h
- SpiGood : dfuutil_programming_spiflash_algorithm.c
- SPIIRQHANDLER : spi.c
- spin_on_error() : i2c.c
- spiobj : dfuutil_programming_spiflash_algorithm.c
- spiopers : dfuutil_programming_spiflash_algorithm.c
- SPLIT_MAX_LEN_UFRAME : EHCI.h
- SplitXstate : EHCI.h
- SRC_ADDR_ERROR : flash_001.h
- SRC_ADDR_NOT_MAPPED : flash_001.h
- SRC_PER_CONTROLLER : gpdma_17xx_40xx.h , gpdma_18xx_43xx.h
- SS : ff.c
- SSP_BITS_10 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_BITS_11 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_BITS_12 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_BITS_13 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_BITS_14 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_BITS_15 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_BITS_16 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_BITS_4 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_BITS_5 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_BITS_6 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_BITS_7 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_BITS_8 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_BITS_9 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_CLOCK_CPHA0_CPOL0 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_CLOCK_CPHA0_CPOL1 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_CLOCK_CPHA1_CPOL0 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_CLOCK_CPHA1_CPOL1 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_CLOCK_MODE0 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_CLOCK_MODE1 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_CLOCK_MODE2 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_CLOCK_MODE3 : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_CPHA_FIRST : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_CPHA_SECOND : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_CPOL_HI : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_CPOL_LO : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_CPSR_BITMASK : ssp_001.h
- SSP_CR0_BITMASK : ssp_001.h
- SSP_CR0_CPHA_FIRST : ssp_001.h
- SSP_CR0_CPHA_SECOND : ssp_001.h
- SSP_CR0_CPOL_HI : ssp_001.h
- SSP_CR0_CPOL_LO : ssp_001.h
- SSP_CR0_DSS : ssp_001.h
- SSP_CR0_FRF_MICROWIRE : ssp_001.h
- SSP_CR0_FRF_SPI : ssp_001.h
- SSP_CR0_FRF_TI : ssp_001.h
- SSP_CR0_SCR : ssp_001.h
- SSP_CR1_BITMASK : ssp_001.h
- SSP_CR1_LBM_EN : ssp_001.h
- SSP_CR1_MASTER_EN : ssp_001.h
- SSP_CR1_SLAVE_EN : ssp_001.h
- SSP_CR1_SO_DISABLE : ssp_001.h
- SSP_CR1_SSP_EN : ssp_001.h
- SSP_DATA_BIT_NUM : ssp.c
- SSP_DATA_BITS : ssp.c
- SSP_DATA_BYTES : ssp.c
- SSP_DMA_BITMASK : ssp_001.h
- SSP_DMA_RX : ssp_001.h
- ssp_dma_rx_ch : spi.c
- ssp_dma_rxf_completed : spi.c
- SSP_DMA_SEL : ssp.c
- SSP_DMA_TX : ssp_001.h
- ssp_dma_tx_ch : spi.c
- ssp_dma_txf_completed : spi.c
- SSP_DR_BITMASK : ssp_001.h
- ssp_format : ssp.c , spi.c , ssp.c
- SSP_FRAMEFORMAT_MICROWIRE : ssp_11xx.h , ssp_13xx.h , ssp_18xx_43xx.h , ssp_17xx_40xx.h
- SSP_FRAMEFORMAT_SPI : ssp_11xx.h , ssp_13xx.h , ssp_18xx_43xx.h , ssp_17xx_40xx.h
- SSP_HI_BYTE_MSK : ssp.c
- SSP_ICR_BITMASK : ssp_001.h
- SSP_ID : board_keil_mcb_18574357.h
- SSP_INT_CLEAR_BITMASK : ssp_001.h
- SSP_INT_MASK_BITMASK : ssp_001.h
- SSP_INTERRUPT_SEL : ssp.c
- SSP_IRQ : ssp.c
- SSP_LO_BYTE_MSK : ssp.c
- SSP_MASK_INT_STAT_BITMASK : ssp_001.h
- SSP_MASTER_MODE : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- SSP_MASTER_MODE_SEL : ssp.c
- SSP_MODE_MASTER : ssp_11xx.h , ssp_13xx.h , ssp_18xx_43xx.h , ssp_17xx_40xx.h
- SSP_MODE_SEL : ssp.c
- SSP_MODE_SLAVE : ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h , ssp_11xx.h
- SSP_MODE_TEST : ssp.c
- SSP_POLLING_SEL : ssp.c
- SSP_RAW_INT_STAT_BITMASK : ssp_001.h
- SSP_Read1BFifo : ssp_11xx.c , ssp_18xx_43xx.c , ssp_13xx.c
- SSP_Read2BFifo : ssp_18xx_43xx.c , ssp_13xx.c , ssp_11xx.c
- SSP_ReadFromFifo() : ssp_17xx_40xx.c
- SSP_RORIC : ssp_001.h
- SSP_RORIM : ssp_001.h
- SSP_RORMIS : ssp_001.h
- SSP_RORRIS : ssp_001.h
- SSP_RTIC : ssp_001.h
- SSP_RTIM : ssp_001.h
- SSP_RTMIS : ssp_001.h
- SSP_RTRIS : ssp_001.h
- ssp_rx_buf : spi.c
- SSP_RXIM : ssp_001.h
- SSP_RXMIS : ssp_001.h
- SSP_RXRIS : ssp_001.h
- SSP_SLAVE_MODE : ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h , ssp_11xx.h
- SSP_SLAVE_MODE_SEL : ssp.c
- SSP_SR_BITMASK : ssp_001.h
- SSP_STAT_BSY : ssp_001.h
- SSP_STAT_RFF : ssp_001.h
- SSP_STAT_RNE : ssp_001.h
- SSP_STAT_TFE : ssp_001.h
- SSP_STAT_TNF : ssp_001.h
- SSP_TRANSFER_MODE_SEL : ssp.c
- ssp_tx_buf : spi.c
- SSP_TXIM : ssp_001.h
- SSP_TXMIS : ssp_001.h
- SSP_TXRIS : ssp_001.h
- SSP_Write1BFifo : ssp_11xx.c , ssp_18xx_43xx.c , ssp_13xx.c
- SSP_Write2BFifo : ssp_11xx.c , ssp_18xx_43xx.c , ssp_13xx.c
- SSP_Write2Fifo() : ssp_17xx_40xx.c
- SSPIRQHANDLER : ssp.c
- SST39VF320_config : sysinit_ea_devkit_17884088.c , sysinit_hitex_eva_18504350.c
- st_clust() : ff.c
- ST_DWORD : ff.h
- ST_WORD : ff.h
- STA_NODISK : diskio.h
- STA_NOINIT : diskio.h
- STA_PROTECT : diskio.h
- STACK_SIZE : lpc43xx_dualcore_config.h , cr_startup_lpc18xx43xx.c , cr_startup_lpc43xx_m0.c , lpc43xx_dualcore_config.h , cr_freertos_startup_lpc17xx40xx.c , lpc43xx_dualcore_config.h
- start : dualcore_emwin.c
- START_DETECT : usart_002.h
- START_DETECT_INT : usart_002.h
- START_SECTOR : app_sdmmc_meas.c
- STARTDATAREGION : fatutil.h
- StartDataRegion : fatutil.h , fatutil.c
- StartingFrame : OHCI.h
- Stat : fs_mci.c , fs_usb.c , fs_mem.c
- STATIC : lpc_types.h
- status : EHCI.h
- Status : lpc_types.h , MassStorageClassCommon.h , RNDISClassCommon.h
- stopTranmission() : sdmmc_17xx_40xx.c
- Str_Cat() : lib_str.h , lib_str.c
- Str_Cat_N() : lib_str.c , lib_str.h
- Str_Char() : lib_str.h , lib_str.c
- Str_Char_Last() : lib_str.c , lib_str.h
- Str_Char_Last_N() : lib_str.h , lib_str.c
- Str_Char_N() : lib_str.c , lib_str.h
- Str_Cmp() : lib_str.c , lib_str.h
- Str_Cmp_N() : lib_str.c , lib_str.h
- Str_CmpIgnoreCase() : lib_str.h , lib_str.c
- Str_CmpIgnoreCase_N() : lib_str.c , lib_str.h
- Str_Copy() : lib_str.h , lib_str.c
- Str_Copy_N() : lib_str.c , lib_str.h
- Str_FmtNbr_32() : lib_str.c
- Str_FmtNbr_Int32() : lib_str.c
- Str_FmtNbr_Int32S() : lib_str.c , lib_str.h
- Str_FmtNbr_Int32U() : lib_str.c , lib_str.h
- Str_FmtPrint : lib_str.h
- Str_FmtScan : lib_str.h
- Str_Len() : lib_str.h , lib_str.c
- Str_Len_N() : lib_str.c , lib_str.h
- Str_MultOvfThTbl_Int32U : lib_str.c
- Str_ParseNbr_Int32() : lib_str.c
- Str_ParseNbr_Int32S() : lib_str.c , lib_str.h
- Str_ParseNbr_Int32U() : lib_str.h , lib_str.c
- Str_Str() : lib_str.c , lib_str.h
- Str_Str_N() : lib_str.c , lib_str.h
- STRINGIFY : Common.h
- STRINGIFY_EXPANDED : Common.h
- SubClass : StdDescriptors.h
- SubFrameSize : AudioClassCommon.h
- Subtype : AudioClassCommon.h , CDCClassCommon.h , MIDIClassCommon.h
- SUCCESS : lpc_types.h
- SVC_Handler() : cr_startup_lpc11xx.c , cr_freertos_startup_lpc8xx.c , cr_ucos_iii_startup_lpc18xx43xx.c , cr_startup_lpc17xx40xx.c , cr_startup_lpc18xx43xx.c , cr_startup_lpc43xx_m0.c , cr_startup_lpc18xx43xx.c , cr_startup_lpc43xx_m0.c , cr_ucos_iii_startup_lpc17xx40xx.c , cr_freertos_startup_lpc11xx.c , cr_freertos_startup_lpc13xx.c , cr_startup_lpc13xx.c , cr_startup_8xx.c
- SwapEndian_16() : Endianness.h
- SWAPENDIAN_16 : Endianness.h
- SWAPENDIAN_32 : Endianness.h
- SwapEndian_32() : Endianness.h
- SwapEndian_n() : Endianness.h
- SWCLK : swm_8xx.h
- SWDIO : swm_8xx.h
- swim_abs() : lpc_swim.c
- swim_clear_screen() : lpc_swim.h , lpc_swim.c
- swim_get_font_height() : lpc_swim_font.c , lpc_swim_font.h
- swim_get_horizontal_size() : lpc_swim.c , lpc_swim.h
- swim_get_vertical_size() : lpc_swim.c , lpc_swim.h
- swim_get_word_len() : lpc_swim_font.c
- swim_get_xy() : lpc_swim_font.c , lpc_swim_font.h
- swim_plot4points() : lpc_swim.c
- swim_plot8points() : lpc_swim.c
- swim_put_box() : lpc_swim.c , lpc_swim.h
- swim_put_char() : lpc_swim_font.c , lpc_swim_font.h
- swim_put_circle() : lpc_swim.c , lpc_swim.h
- swim_put_diamond() : lpc_swim.h , lpc_swim.c
- swim_put_image() : lpc_swim_image.h , lpc_swim_image.c
- swim_put_invert_image() : lpc_swim_image.h , lpc_swim_image.c
- swim_put_left_image() : lpc_swim_image.c , lpc_swim_image.h
- swim_put_line() : lpc_swim.h , lpc_swim.c
- swim_put_line_raw() : lpc_swim.c
- swim_put_ltext() : lpc_swim_font.c , lpc_swim_font.h
- swim_put_newline() : lpc_swim_font.h , lpc_swim_font.c
- swim_put_pixel() : lpc_swim.h , lpc_swim.c
- swim_put_right_image() : lpc_swim_image.c , lpc_swim_image.h
- swim_put_scale_image() : lpc_swim_image.c , lpc_swim_image.h
- swim_put_scale_invert_image() : lpc_swim_image.h , lpc_swim_image.c
- swim_put_scale_left_image() : lpc_swim_image.c , lpc_swim_image.h
- swim_put_scale_right_image() : lpc_swim_image.h , lpc_swim_image.c
- swim_put_text() : lpc_swim_font.c , lpc_swim_font.h
- swim_put_text_xy() : lpc_swim_font.h , lpc_swim_font.c
- swim_put_win_image() : lpc_swim_image.c , lpc_swim_image.h
- swim_put_word() : lpc_swim_font.c
- SWIM_ROTATION_T : lpc_swim_image.h
- swim_set_bkg_color() : lpc_swim.c , lpc_swim.h
- swim_set_fill_color() : lpc_swim.h , lpc_swim.c
- swim_set_font() : lpc_swim_font.c , lpc_swim_font.h
- swim_set_font_trasparency() : lpc_swim_font.c , lpc_swim_font.h
- swim_set_pen_color() : lpc_swim.c , lpc_swim.h
- swim_set_title() : lpc_swim_font.h , lpc_swim_font.c
- swim_set_xy() : lpc_swim_font.h , lpc_swim_font.c
- swim_window_close() : lpc_swim.c , lpc_swim.h
- swim_window_open() : lpc_swim.c , lpc_swim.h
- swim_window_open_noclear() : lpc_swim.h , lpc_swim.c
- swim_window_open_p() : lpc_swim.c
- swim_window_scroll() : lpc_swim_font.h , lpc_swim_font.c
- SWM_ACMP_O_O : swm_8xx.h
- SWM_CLKOUT_O : swm_8xx.h
- SWM_CTIN_0_I : swm_8xx.h
- SWM_CTIN_1_I : swm_8xx.h
- SWM_CTIN_2_I : swm_8xx.h
- SWM_CTIN_3_I : swm_8xx.h
- SWM_CTOUT_0_O : swm_8xx.h
- SWM_CTOUT_1_O : swm_8xx.h
- SWM_CTOUT_2_O : swm_8xx.h
- SWM_CTOUT_3_O : swm_8xx.h
- SWM_GPIO_INT_BMAT_O : swm_8xx.h
- SWM_I2C_SCL_IO : swm_8xx.h
- SWM_I2C_SDA_IO : swm_8xx.h
- SWM_SPI0_MISO_IO : swm_8xx.h
- SWM_SPI0_MOSI_IO : swm_8xx.h
- SWM_SPI0_SCK_IO : swm_8xx.h
- SWM_SPI0_SSEL_IO : swm_8xx.h
- SWM_SPI1_MISO_IO : swm_8xx.h
- SWM_SPI1_MOSI_IO : swm_8xx.h
- SWM_SPI1_SCK_IO : swm_8xx.h
- SWM_SPI1_SSEL_IO : swm_8xx.h
- SWM_U0_CTS_I : swm_8xx.h
- SWM_U0_RTS_O : swm_8xx.h
- SWM_U0_RXD_I : swm_8xx.h
- SWM_U0_SCLK_IO : swm_8xx.h
- SWM_U0_TXD_O : swm_8xx.h
- SWM_U1_CTS_I : swm_8xx.h
- SWM_U1_RTS_O : swm_8xx.h
- SWM_U1_RXD_I : swm_8xx.h
- SWM_U1_SCLK_IO : swm_8xx.h
- SWM_U1_TXD_O : swm_8xx.h
- SWM_U2_CTS_I : swm_8xx.h
- SWM_U2_RTS_O : swm_8xx.h
- SWM_U2_RXD_I : swm_8xx.h
- SWM_U2_SCLK_IO : swm_8xx.h
- SWM_U2_TXD_O : swm_8xx.h
- sync() : ff.c
- Sync : MassStorageClassCommon.h
- SyncEndpointNumber : AudioClassCommon.h
- sys_arch_mbox_fetch() : sys_arch_freertos.c
- sys_arch_mbox_tryfetch() : sys_arch_freertos.c
- sys_arch_protect() : sys_arch_freertos.c
- sys_arch_sem_wait() : sys_arch_freertos.c
- sys_arch_unprotect() : sys_arch_freertos.c
- sys_assert() : sys_arch_freertos.c
- SYS_CTRL1 : board_keil_mcb_18574357.h
- SYS_CTRL2 : board_keil_mcb_18574357.h
- SYS_DEFAULT_THREAD_STACK_DEPTH : sys_arch.h
- SYS_ERR_INT : HAL_LPC17xx.h
- sys_init() : sys_arch_freertos.c
- SYS_LIGHTWEIGHT_PROT : lwipopts.h
- sys_mbox_free() : sys_arch_freertos.c
- sys_mbox_new() : sys_arch_freertos.c
- SYS_MBOX_NULL : sys_arch.h
- sys_mbox_post() : sys_arch_freertos.c
- sys_mbox_set_invalid : sys_arch.h
- sys_mbox_t : sys_arch.h
- sys_mbox_trypost() : sys_arch_freertos.c
- sys_mbox_valid : sys_arch.h
- sys_mutex_free() : sys_arch_freertos.c
- sys_mutex_lock() : sys_arch_freertos.c
- sys_mutex_new() : sys_arch_freertos.c
- sys_mutex_t : sys_arch.h
- sys_mutex_unlock() : sys_arch_freertos.c
- sys_now() : lpc43xx_systick.c , sys_arch_freertos.c
- sys_prot_t : sys_arch.h
- sys_sem_free() : sys_arch_freertos.c
- sys_sem_new() : sys_arch_freertos.c
- SYS_SEM_NULL : sys_arch.h
- sys_sem_set_invalid : sys_arch.h
- sys_sem_signal() : sys_arch_freertos.c
- sys_sem_t : sys_arch.h
- sys_sem_valid : sys_arch.h
- sys_thread_new() : sys_arch_freertos.c
- sys_thread_t : sys_arch.h
- SYSCTL_BODINTVAL_2_22V : sysctl_13xx.h
- SYSCTL_BODINTVAL_2_52V : sysctl_13xx.h
- SYSCTL_BODINTVAL_2_80V : sysctl_13xx.h
- SYSCTL_BODINTVAL_LVL0 : syscon_8xx.h
- SYSCTL_BODINTVAL_LVL1 : syscon_8xx.h
- SYSCTL_BODINTVAL_LVL2 : syscon_8xx.h
- SYSCTL_BODINTVAL_LVL3 : syscon_8xx.h
- SYSCTL_BODINTVAL_RESERVED1 : sysctl_11xx.h , sysctl_13xx.h
- SYSCTL_BODRSTLVL_0 : syscon_8xx.h
- SYSCTL_BODRSTLVL_1 : syscon_8xx.h
- SYSCTL_BODRSTLVL_1_46V : sysctl_13xx.h
- SYSCTL_BODRSTLVL_2 : syscon_8xx.h
- SYSCTL_BODRSTLVL_2_06V : sysctl_11xx.h , sysctl_13xx.h
- SYSCTL_BODRSTLVL_2_35V : sysctl_11xx.h , sysctl_13xx.h
- SYSCTL_BODRSTLVL_2_63V : sysctl_11xx.h , sysctl_13xx.h
- SYSCTL_BODRSTLVL_3 : syscon_8xx.h
- SYSCTL_BODRSTLVL_RESERVED1 : sysctl_11xx.h
- SYSCTL_CCLKSRC_MAINPLL : clock_17xx_40xx.h
- SYSCTL_CCLKSRC_SYSCLK : clock_17xx_40xx.h
- SYSCTL_CLKOUTSRC_CPU : clock_17xx_40xx.h
- SYSCTL_CLKOUTSRC_IRC : clock_11xx.h , clock_13xx.h , clock_8xx.h , clock_17xx_40xx.h
- SYSCTL_CLKOUTSRC_LFOSC : clock_11xx.h
- SYSCTL_CLKOUTSRC_MAINOSC : clock_11xx.h , clock_17xx_40xx.h
- SYSCTL_CLKOUTSRC_MAINSYSCLK : clock_11xx.h , clock_8xx.h , clock_13xx.h
- SYSCTL_CLKOUTSRC_RESERVED3 : clock_17xx_40xx.h
- SYSCTL_CLKOUTSRC_RTC : clock_17xx_40xx.h
- SYSCTL_CLKOUTSRC_SPIFI : clock_17xx_40xx.h
- SYSCTL_CLKOUTSRC_SYSOSC : clock_13xx.h , clock_8xx.h
- SYSCTL_CLKOUTSRC_USB : clock_17xx_40xx.h
- SYSCTL_CLKOUTSRC_WATCHDOGOSC : clock_17xx_40xx.h
- SYSCTL_CLKOUTSRC_WDTOSC : clock_11xx.h , clock_8xx.h , clock_13xx.h
- SYSCTL_CLOCK_ACOMP : clock_8xx.h
- SYSCTL_CLOCK_ADC : clock_17xx_40xx.h , clock_11xx.h , clock_13xx.h
- SYSCTL_CLOCK_CAN1 : clock_17xx_40xx.h
- SYSCTL_CLOCK_CAN2 : clock_17xx_40xx.h
- SYSCTL_CLOCK_CRC : clock_8xx.h
- SYSCTL_CLOCK_CT16B0 : clock_11xx.h , clock_13xx.h
- SYSCTL_CLOCK_CT16B1 : clock_11xx.h , clock_13xx.h
- SYSCTL_CLOCK_CT32B0 : clock_11xx.h , clock_13xx.h
- SYSCTL_CLOCK_CT32B1 : clock_11xx.h , clock_13xx.h
- SYSCTL_CLOCK_EMC : clock_17xx_40xx.h
- SYSCTL_CLOCK_ENET : clock_17xx_40xx.h
- SYSCTL_CLOCK_FLASH : clock_8xx.h
- SYSCTL_CLOCK_FLASHARRAY : clock_13xx.h , clock_11xx.h
- SYSCTL_CLOCK_FLASHREG : clock_13xx.h , clock_11xx.h , clock_8xx.h
- SYSCTL_CLOCK_GPDMA : clock_17xx_40xx.h
- SYSCTL_CLOCK_GPIO : clock_11xx.h , clock_8xx.h , clock_17xx_40xx.h , clock_13xx.h
- SYSCTL_CLOCK_GROUP0INT : clock_11xx.h
- SYSCTL_CLOCK_GROUP1INT : clock_11xx.h
- SYSCTL_CLOCK_I2C : clock_13xx.h , clock_11xx.h , clock_8xx.h
- SYSCTL_CLOCK_I2C0 : clock_17xx_40xx.h
- SYSCTL_CLOCK_I2C1 : clock_17xx_40xx.h
- SYSCTL_CLOCK_I2C2 : clock_17xx_40xx.h
- SYSCTL_CLOCK_I2S : clock_17xx_40xx.h
- SYSCTL_CLOCK_IOCON : clock_11xx.h , clock_8xx.h , clock_13xx.h
- SYSCTL_CLOCK_LCD : clock_17xx_40xx.h
- SYSCTL_CLOCK_MCPWM : clock_17xx_40xx.h
- SYSCTL_CLOCK_MRT : clock_8xx.h
- SYSCTL_CLOCK_P0INT : clock_11xx.h
- SYSCTL_CLOCK_P1INT : clock_11xx.h
- SYSCTL_CLOCK_PINT : clock_11xx.h
- SYSCTL_CLOCK_PWM0 : clock_17xx_40xx.h
- SYSCTL_CLOCK_PWM1 : clock_17xx_40xx.h
- SYSCTL_CLOCK_QEI : clock_17xx_40xx.h
- SYSCTL_CLOCK_RAM : clock_8xx.h , clock_13xx.h , clock_11xx.h
- SYSCTL_CLOCK_RESERVED14 : clock_11xx.h
- SYSCTL_CLOCK_RESERVED17 : clock_11xx.h , clock_13xx.h
- SYSCTL_CLOCK_RESERVED20 : clock_11xx.h
- SYSCTL_CLOCK_RESERVED21 : clock_11xx.h
- SYSCTL_CLOCK_RESERVED22 : clock_11xx.h
- SYSCTL_CLOCK_RESERVED25 : clock_11xx.h
- SYSCTL_CLOCK_RESERVED26 : clock_11xx.h
- SYSCTL_CLOCK_RESERVED27 : clock_11xx.h
- SYSCTL_CLOCK_ROM : clock_8xx.h , clock_11xx.h , clock_13xx.h
- SYSCTL_CLOCK_RSVD32 : clock_17xx_40xx.h
- SYSCTL_CLOCK_RSVD33 : clock_17xx_40xx.h
- SYSCTL_CLOCK_RSVD34 : clock_17xx_40xx.h
- SYSCTL_CLOCK_RSVD35 : clock_17xx_40xx.h
- SYSCTL_CLOCK_RTC : clock_17xx_40xx.h
- SYSCTL_CLOCK_SCT : clock_8xx.h
- SYSCTL_CLOCK_SDC : clock_17xx_40xx.h
- SYSCTL_CLOCK_SPI0 : clock_8xx.h
- SYSCTL_CLOCK_SPI1 : clock_8xx.h
- SYSCTL_CLOCK_SPIFI : clock_17xx_40xx.h
- SYSCTL_CLOCK_SSP0 : clock_13xx.h , clock_17xx_40xx.h , clock_11xx.h
- SYSCTL_CLOCK_SSP1 : clock_13xx.h , clock_11xx.h , clock_17xx_40xx.h
- SYSCTL_CLOCK_SSP2 : clock_17xx_40xx.h
- SYSCTL_CLOCK_SWM : clock_8xx.h
- SYSCTL_CLOCK_SYS : clock_13xx.h , clock_8xx.h , clock_11xx.h
- SYSCTL_CLOCK_TIMER0 : clock_17xx_40xx.h
- SYSCTL_CLOCK_TIMER1 : clock_17xx_40xx.h
- SYSCTL_CLOCK_TIMER2 : clock_17xx_40xx.h
- SYSCTL_CLOCK_TIMER3 : clock_17xx_40xx.h
- SYSCTL_CLOCK_UART0 : clock_11xx.h , clock_8xx.h , clock_13xx.h , clock_17xx_40xx.h
- SYSCTL_CLOCK_UART1 : clock_8xx.h , clock_17xx_40xx.h
- SYSCTL_CLOCK_UART2 : clock_8xx.h , clock_17xx_40xx.h
- SYSCTL_CLOCK_UART3 : clock_17xx_40xx.h
- SYSCTL_CLOCK_UART4 : clock_17xx_40xx.h
- SYSCTL_CLOCK_USB : clock_17xx_40xx.h , clock_13xx.h
- SYSCTL_CLOCK_WDT : clock_13xx.h , clock_11xx.h
- SYSCTL_CLOCK_WKT : clock_8xx.h
- SYSCTL_CLOCK_WWDT : clock_8xx.h
- SYSCTL_DEEPSLP_BOD_PD : sysctl_11xx.h , sysctl_13xx.h , syscon_8xx.h
- SYSCTL_DEEPSLP_WDTOSC_PD : sysctl_13xx.h , sysctl_11xx.h , syscon_8xx.h
- SYSCTL_EMC_DIV1 : clock_17xx_40xx.h
- SYSCTL_EMC_DIV2 : clock_17xx_40xx.h
- SYSCTL_IRC_FREQ : clock_11xx.h , clock_13xx.h , clock_8xx.h , clock_17xx_40xx.h
- SYSCTL_MAIN_PLL : sysctl_17xx_40xx.h
- SYSCTL_MAINCLKSRC_IRC : clock_11xx.h , clock_8xx.h , clock_13xx.h
- SYSCTL_MAINCLKSRC_LFOSC : clock_11xx.h
- SYSCTL_MAINCLKSRC_PLLIN : clock_13xx.h , clock_8xx.h , clock_11xx.h
- SYSCTL_MAINCLKSRC_PLLOUT : clock_11xx.h , clock_13xx.h , clock_8xx.h
- SYSCTL_MAINCLKSRC_WDTOSC : clock_11xx.h , clock_8xx.h , clock_13xx.h
- SYSCTL_NMISRC_ENABLE : syscon_8xx.h , sysctl_11xx.h
- SYSCTL_OSCEC : clock_17xx_40xx.h
- SYSCTL_OSCRANGE_15_25 : clock_17xx_40xx.h
- SYSCTL_OSCSTAT : clock_17xx_40xx.h
- SYSCTL_PD_DPDFLAG : sysctl_17xx_40xx.h
- SYSCTL_PD_DSFLAG : sysctl_17xx_40xx.h
- SYSCTL_PD_PDFLAG : sysctl_17xx_40xx.h
- SYSCTL_PD_SMFLAG : sysctl_17xx_40xx.h
- SYSCTL_PLL_ENABLE : clock_17xx_40xx.h
- SYSCTL_PLLCLKSRC_EXT_CLKIN : clock_8xx.h
- SYSCTL_PLLCLKSRC_IRC : clock_13xx.h , clock_8xx.h , clock_17xx_40xx.h , clock_11xx.h
- SYSCTL_PLLCLKSRC_MAINOSC : clock_17xx_40xx.h , clock_11xx.h
- SYSCTL_PLLCLKSRC_RESERVED : clock_8xx.h
- SYSCTL_PLLCLKSRC_RESERVED1 : clock_17xx_40xx.h , clock_11xx.h , clock_13xx.h
- SYSCTL_PLLCLKSRC_RESERVED2 : clock_13xx.h , clock_11xx.h , clock_17xx_40xx.h
- SYSCTL_PLLCLKSRC_SYSOSC : clock_13xx.h , clock_8xx.h
- SYSCTL_PLLSTS_ENABLED : clock_17xx_40xx.h
- SYSCTL_PLLSTS_LOCKED : clock_17xx_40xx.h
- SYSCTL_POWERDOWN_ADC_PD : sysctl_11xx.h , sysctl_13xx.h
- SYSCTL_POWERDOWN_BOD_PD : sysctl_11xx.h , sysctl_13xx.h
- SYSCTL_POWERDOWN_FLASH_PD : sysctl_11xx.h , sysctl_13xx.h
- SYSCTL_POWERDOWN_IRC_PD : sysctl_11xx.h , sysctl_13xx.h
- SYSCTL_POWERDOWN_IRCOUT_PD : sysctl_13xx.h , sysctl_11xx.h
- SYSCTL_POWERDOWN_SYSOSC_PD : sysctl_11xx.h , sysctl_13xx.h
- SYSCTL_POWERDOWN_SYSPLL_PD : sysctl_11xx.h , sysctl_13xx.h
- SYSCTL_POWERDOWN_USBPAD_PD : sysctl_13xx.h
- SYSCTL_POWERDOWN_USBPLL_PD : sysctl_13xx.h
- SYSCTL_POWERDOWN_WDTOSC_PD : sysctl_11xx.h , sysctl_13xx.h
- SYSCTL_RESET_ADC : sysctl_17xx_40xx.h
- SYSCTL_RESET_CAN1 : sysctl_17xx_40xx.h
- SYSCTL_RESET_CAN2 : sysctl_17xx_40xx.h
- SYSCTL_RESET_CANACC : sysctl_17xx_40xx.h
- SYSCTL_RESET_DAC : sysctl_17xx_40xx.h
- SYSCTL_RESET_EMC : sysctl_17xx_40xx.h
- SYSCTL_RESET_ENET : sysctl_17xx_40xx.h
- SYSCTL_RESET_GPDMA : sysctl_17xx_40xx.h
- SYSCTL_RESET_GPIO : sysctl_17xx_40xx.h
- SYSCTL_RESET_I2C0 : sysctl_17xx_40xx.h
- SYSCTL_RESET_I2C1 : sysctl_17xx_40xx.h
- SYSCTL_RESET_I2C2 : sysctl_17xx_40xx.h
- SYSCTL_RESET_I2S : sysctl_17xx_40xx.h
- SYSCTL_RESET_IOCON : sysctl_17xx_40xx.h
- SYSCTL_RESET_LCD : sysctl_17xx_40xx.h
- SYSCTL_RESET_MCPWM : sysctl_17xx_40xx.h
- SYSCTL_RESET_PCSDC : sysctl_17xx_40xx.h
- SYSCTL_RESET_PWM0 : sysctl_17xx_40xx.h
- SYSCTL_RESET_PWM1 : sysctl_17xx_40xx.h
- SYSCTL_RESET_QEI : sysctl_17xx_40xx.h
- SYSCTL_RESET_RTC : sysctl_17xx_40xx.h
- SYSCTL_RESET_SPIFI : sysctl_17xx_40xx.h
- SYSCTL_RESET_SSP0 : sysctl_17xx_40xx.h
- SYSCTL_RESET_SSP1 : sysctl_17xx_40xx.h
- SYSCTL_RESET_SSP2 : sysctl_17xx_40xx.h
- SYSCTL_RESET_TIMER0 : sysctl_17xx_40xx.h
- SYSCTL_RESET_TIMER1 : sysctl_17xx_40xx.h
- SYSCTL_RESET_TIMER2 : sysctl_17xx_40xx.h
- SYSCTL_RESET_TIMER3 : sysctl_17xx_40xx.h
- SYSCTL_RESET_UART0 : sysctl_17xx_40xx.h
- SYSCTL_RESET_UART1 : sysctl_17xx_40xx.h
- SYSCTL_RESET_UART2 : sysctl_17xx_40xx.h
- SYSCTL_RESET_UART3 : sysctl_17xx_40xx.h
- SYSCTL_RESET_UART4 : sysctl_17xx_40xx.h
- SYSCTL_RESET_USB : sysctl_17xx_40xx.h
- SYSCTL_RST_BOD : sysctl_17xx_40xx.h , syscon_8xx.h , sysctl_13xx.h , sysctl_11xx.h
- SYSCTL_RST_EXTRST : sysctl_11xx.h , sysctl_17xx_40xx.h , syscon_8xx.h , sysctl_13xx.h
- SYSCTL_RST_POR : syscon_8xx.h , sysctl_11xx.h , sysctl_17xx_40xx.h , sysctl_13xx.h
- SYSCTL_RST_SYSRST : sysctl_11xx.h , sysctl_13xx.h , syscon_8xx.h
- SYSCTL_RST_WDT : sysctl_17xx_40xx.h , syscon_8xx.h , sysctl_11xx.h , sysctl_13xx.h
- SYSCTL_SLPWAKE_ACMP_PD : syscon_8xx.h
- SYSCTL_SLPWAKE_ADC_PD : sysctl_13xx.h , sysctl_11xx.h
- SYSCTL_SLPWAKE_BOD_PD : sysctl_13xx.h , sysctl_11xx.h , syscon_8xx.h
- SYSCTL_SLPWAKE_FLASH_PD : sysctl_13xx.h , sysctl_11xx.h , syscon_8xx.h
- SYSCTL_SLPWAKE_IRC_PD : syscon_8xx.h , sysctl_13xx.h , sysctl_11xx.h
- SYSCTL_SLPWAKE_IRCOUT_PD : sysctl_13xx.h , syscon_8xx.h , sysctl_11xx.h
- SYSCTL_SLPWAKE_SYSOSC_PD : sysctl_11xx.h , sysctl_13xx.h , syscon_8xx.h
- SYSCTL_SLPWAKE_SYSPLL_PD : sysctl_11xx.h , sysctl_13xx.h , syscon_8xx.h
- SYSCTL_SLPWAKE_USBPAD_PD : sysctl_13xx.h
- SYSCTL_SLPWAKE_USBPLL_PD : sysctl_13xx.h
- SYSCTL_SLPWAKE_WDTOSC_PD : sysctl_11xx.h , syscon_8xx.h , sysctl_13xx.h
- SYSCTL_SPIFICLKSRC_MAINPLL : clock_17xx_40xx.h
- SYSCTL_SPIFICLKSRC_RESERVED : clock_17xx_40xx.h
- SYSCTL_SPIFICLKSRC_SYSCLK : clock_17xx_40xx.h
- SYSCTL_SPIFICLKSRC_USBPLL : clock_17xx_40xx.h
- SYSCTL_STARTST_PIN : sysctl_13xx.h
- SYSCTL_STARTST_PIN_BIT : sysctl_13xx.h
- SYSCTL_STARTST_PIN_INDEX : sysctl_13xx.h
- SYSCTL_USB_PLL : sysctl_17xx_40xx.h
- SYSCTL_USBCLKSRC_MAINPLL : clock_17xx_40xx.h
- SYSCTL_USBCLKSRC_MAINSYSCLK : clock_13xx.h
- SYSCTL_USBCLKSRC_PLLOUT : clock_13xx.h
- SYSCTL_USBCLKSRC_RESERVED : clock_17xx_40xx.h
- SYSCTL_USBCLKSRC_SYSCLK : clock_17xx_40xx.h
- SYSCTL_USBCLKSRC_USBPLL : clock_17xx_40xx.h
- SYSCTL_WAKEUP_BODINT : syscon_8xx.h
- SYSCTL_WAKEUP_I2CINT : syscon_8xx.h
- SYSCTL_WAKEUP_SPI0TINT : syscon_8xx.h
- SYSCTL_WAKEUP_SPI1INT : syscon_8xx.h
- SYSCTL_WAKEUP_USART0INT : syscon_8xx.h
- SYSCTL_WAKEUP_USART1INT : syscon_8xx.h
- SYSCTL_WAKEUP_USART2INT : syscon_8xx.h
- SYSCTL_WAKEUP_WKTINT : syscon_8xx.h
- SYSCTL_WAKEUP_WWDTINT : syscon_8xx.h
- SystemCoreClock : board_keil_mcb_18574357.c , board_ngx_xplorer_18304330.c , board_nxp_xpresso_812.c , board_hitex_eva_18504350.c , board_nxp_xpresso_11u14.c , board_nxp_xpresso_11c24.c , board_api.h , board_ea_devkit_17884088.c , board_nxp_xpresso_1347.c , board_nxp_xpresso_1769.c , lpc43xx_systick.c
- SystemCoreClockUpdate() : board_keil_mcb_18574357.c , board_api.h , board_nxp_xpresso_1769.c , board_ea_devkit_17884088.c , board_ngx_xplorer_18304330.c , board_nxp_xpresso_812.c , board_nxp_xpresso_11u14.c , board_nxp_xpresso_11c24.c , board_nxp_xpresso_1347.c , board_hitex_eva_18504350.c
- SystemInit() : sysinit_keil_mcb_18574357.c , cr_startup_lpc43xx_m0.c , cr_startup_lpc17xx40xx.c , cr_startup_lpc43xx_m0.c , sysinit_nxp_xpresso_1769.c , cr_startup_lpc18xx43xx.c , cr_ucos_iii_startup_lpc17xx40xx.c , cr_freertos_startup_lpc17xx40xx.c , cr_freertos_startup_lpc11xx.c , cr_freertos_startup_lpc13xx.c , cr_freertos_startup_lpc17xx40xx.c , sysinit_nxp_xpresso_11c24.c , cr_startup_lpc13xx.c , sysinit_ea_devkit_17884088.c , cr_startup_lpc11xx.c , cr_freertos_startup_lpc18xx43xx.c , sysinit_nxp_xpresso_11u14.c , sysinit_ngx_xplorer_18304330.c , cr_ucos_iii_startup_lpc18xx43xx.c , cr_startup_lpc18xx43xx.c , sysinit_hitex_eva_18504350.c , sysinit_nxp_xpresso_1347.c , sysinit_nxp_xpresso_812.c , cr_freertos_startup_lpc18xx43xx.c
- SystemSetupClocking() : sysinit_ea_devkit_17884088.c , sysinit_nxp_xpresso_812.c , sysinit_hitex_eva_18504350.c , sysinit_nxp_xpresso_1347.c , sysinit_ngx_xplorer_18304330.c , sysinit_nxp_xpresso_1769.c , sysinit_keil_mcb_18574357.c , sysinit_nxp_xpresso_11c24.c , sysinit_nxp_xpresso_11u14.c
- SystemSetupMemory() : sysinit_ea_devkit_17884088.c , sysinit_hitex_eva_18504350.c , sysinit_keil_mcb_18574357.c , sysinit_ngx_xplorer_18304330.c
- SystemSetupMuxing() : sysinit_nxp_xpresso_11u14.c , sysinit_ngx_xplorer_18304330.c , sysinit_hitex_eva_18504350.c , sysinit_nxp_xpresso_1769.c , sysinit_keil_mcb_18574357.c , sysinit_nxp_xpresso_812.c , sysinit_ea_devkit_17884088.c , sysinit_nxp_xpresso_1347.c , sysinit_nxp_xpresso_11c24.c
- SysTick_Disable() : lpc43xx_systick.c
- SysTick_Enable() : dualcore_emwin.c
- SysTick_Handler() : cr_startup_lpc17xx40xx.c , lpc43xx_systick.c , watchdog.c , crc.c , dfuutil_programming_dfu_ops.c , sdmmc.c , i2c.c , watchdog.c , blinky.c , watchdog.c , lcd.c , blinky.c , clkout.c , main.c , i2c.c , mrt.c , blinky.c , clkout.c , sct.c , cr_ucos_iii_startup_lpc17xx40xx.c , i2c.c , cr_freertos_startup_lpc8xx.c , clkout.c , cr_startup_lpc11xx.c , cr_startup_lpc43xx_m0.c , main.c , cr_startup_lpc43xx_m0.c , lcd.c , cr_freertos_startup_lpc11xx.c , cr_startup_8xx.c , cr_startup_lpc18xx43xx.c , cr_startup_lpc13xx.c , cr_freertos_startup_lpc13xx.c , cr_startup_lpc18xx43xx.c , watchdog.c , cr_ucos_iii_startup_lpc18xx43xx.c
- systick_timems : main.c , lpc43xx_systick.c , GUI_X.c
- SZ_DIR : ff.c
- SZ_PTE : ff.c
- SZT_F : cc.h