| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- a
- b
- c
- d
- e
- f
- g
- h
- i
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages

### - c -

- CAN_AF_BYBASS_MODE : can_17xx_40xx.h
- CAN_AF_FULL_MODE : can_17xx_40xx.h
- CAN_AF_NORMAL_MODE : can_17xx_40xx.h
- CAN_AF_OFF_MODE : can_17xx_40xx.h
- CAN_BUFFER_1 : can_001.h
- CAN_BUFFER_2 : can_001.h
- CAN_BUFFER_3 : can_001.h
- CAN_BUFFER_LAST : can_001.h
- CAN_LISTEN_ONLY_MODE : can_17xx_40xx.h
- CAN_OPERATION_MODE : can_17xx_40xx.h
- CAN_RECEIVE_PRIORITY_MODE : can_17xx_40xx.h
- CAN_RESET_MODE : can_17xx_40xx.h
- CAN_SELFTEST_MODE : can_17xx_40xx.h
- CAN_SLEEP_MODE : can_17xx_40xx.h
- CAN_TEST_MODE : can_17xx_40xx.h
- CAN_TRANSMIT_PRIORITY_MODE : can_17xx_40xx.h
- CANAF_RAM_EFF_GRP_SEC : can_001.h
- CANAF_RAM_EFF_SEC : can_001.h
- CANAF_RAM_FULLCAN_SEC : can_001.h
- CANAF_RAM_SECTION_NUM : can_001.h
- CANAF_RAM_SFF_GRP_SEC : can_001.h
- CANAF_RAM_SFF_SEC : can_001.h
- CCAN_BASIC_TEST_MODE : ccan_001.h
- CCAN_ERR_INT : ccan_001.h
- CCAN_LOOPBACK_TEST_MODE : ccan_001.h
- CCAN_MODULE_INT : ccan_001.h
- CCAN_RX_MODE : ccan_001.h
- CCAN_SILENT_TEST_MODE : ccan_001.h
- CCAN_STAT_BOFF : ccan_001.h
- CCAN_STAT_EPASS : ccan_001.h
- CCAN_STAT_EWARN : ccan_001.h
- CCAN_STAT_LEC : ccan_001.h
- CCAN_STAT_RXOK : ccan_001.h
- CCAN_STAT_TXOK : ccan_001.h
- CCAN_STATUS_CHANGE_INT : ccan_001.h
- CCAN_TX_MODE : ccan_001.h
- CDC_CSCP_ACMSubclass : CDCClassCommon.h
- CDC_CSCP_ATCommandProtocol : CDCClassCommon.h
- CDC_CSCP_CDCClass : CDCClassCommon.h
- CDC_CSCP_CDCDataClass : CDCClassCommon.h
- CDC_CSCP_NoDataProtocol : CDCClassCommon.h
- CDC_CSCP_NoDataSubclass : CDCClassCommon.h
- CDC_CSCP_NoSpecificProtocol : CDCClassCommon.h
- CDC_CSCP_NoSpecificSubclass : CDCClassCommon.h
- CDC_CSCP_VendorSpecificProtocol : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_ACM : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_ATM : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_CallManagement : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_CAPI : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_CountrySelection : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_DirectLine : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_Ethernet : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_ExtensionUnit : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_Header : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_MultiChannel : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_NetworkChannel : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_ProtocolUnit : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_TelephoneCall : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_TelephoneOpModes : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_TelephoneRinger : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_Union : CDCClassCommon.h
- CDC_DSUBTYPE_CSInterface_USBTerminal : CDCClassCommon.h
- CDC_ENUMERROR_InvalidConfigDescriptor : CDCClassHost.h
- CDC_ENUMERROR_NoCompatibleInterfaceFound : CDCClassHost.h
- CDC_ENUMERROR_NoError : CDCClassHost.h
- CDC_ENUMERROR_PipeConfigurationFailed : CDCClassHost.h
- CDC_LINEENCODING_OneAndAHalfStopBits : CDCClassCommon.h
- CDC_LINEENCODING_OneStopBit : CDCClassCommon.h
- CDC_LINEENCODING_TwoStopBits : CDCClassCommon.h
- CDC_NOTIF_SerialState : CDCClassCommon.h
- CDC_PARITY_Even : CDCClassCommon.h
- CDC_PARITY_Mark : CDCClassCommon.h
- CDC_PARITY_None : CDCClassCommon.h
- CDC_PARITY_Odd : CDCClassCommon.h
- CDC_PARITY_Space : CDCClassCommon.h
- CDC_REQ_GetEncapsulatedResponse : CDCClassCommon.h
- CDC_REQ_GetLineEncoding : CDCClassCommon.h
- CDC_REQ_SendBreak : CDCClassCommon.h
- CDC_REQ_SendEncapsulatedCommand : CDCClassCommon.h
- CDC_REQ_SetControlLineState : CDCClassCommon.h
- CDC_REQ_SetLineEncoding : CDCClassCommon.h
- CGU_AUDIO_PLL : cguccu_18xx_43xx.h
- CGU_USB_PLL : cguccu_18xx_43xx.h
- CHIP_AES_API_CMD_DECODE_CBC : aes_18xx_43xx.h
- CHIP_AES_API_CMD_DECODE_ECB : aes_18xx_43xx.h
- CHIP_AES_API_CMD_ENCODE_CBC : aes_18xx_43xx.h
- CHIP_AES_API_CMD_ENCODE_ECB : aes_18xx_43xx.h
- CHIP_OTP_BOOTSRC_EMC16 : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_EMC32 : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_EMC8 : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_PINS : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_SPI : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_SPIFI : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_UART0 : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_UART3 : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_USB0 : otp_18xx_43xx.h
- CHIP_OTP_BOOTSRC_USB1 : otp_18xx_43xx.h
- CHIP_SSP_FRAME_FORMAT_TI : ssp_11xx.h , ssp_13xx.h , ssp_17xx_40xx.h , ssp_18xx_43xx.h
- CLK_APB0_SSP0 : chip_clocks.h
- CLK_APB0_UART0 : chip_clocks.h
- CLK_APB0_UART1 : chip_clocks.h
- CLK_APB1_BUS : chip_clocks.h
- CLK_APB1_CAN1 : chip_clocks.h
- CLK_APB1_I2C0 : chip_clocks.h
- CLK_APB1_I2S : chip_clocks.h
- CLK_APB1_MOTOCON : chip_clocks.h
- CLK_APB2_SDIO : chip_clocks.h
- CLK_APB2_SSP1 : chip_clocks.h
- CLK_APB2_UART2 : chip_clocks.h
- CLK_APB2_UART3 : chip_clocks.h
- CLK_APB3_ADC0 : chip_clocks.h
- CLK_APB3_ADC1 : chip_clocks.h
- CLK_APB3_BUS : chip_clocks.h
- CLK_APB3_CAN0 : chip_clocks.h
- CLK_APB3_DAC : chip_clocks.h
- CLK_APB3_I2C1 : chip_clocks.h
- CLK_APLL : chip_clocks.h
- CLK_BASE_APB1 : chip_clocks.h
- CLK_BASE_APB3 : chip_clocks.h
- CLK_BASE_APLL : chip_clocks.h
- CLK_BASE_CGU_OUT0 : chip_clocks.h
- CLK_BASE_CGU_OUT1 : chip_clocks.h
- CLK_BASE_LAST : chip_clocks.h
- CLK_BASE_LCD : chip_clocks.h
- CLK_BASE_MX : chip_clocks.h
- CLK_BASE_NONE : chip_clocks.h
- CLK_BASE_OUT : chip_clocks.h
- CLK_BASE_PHY_RX : chip_clocks.h
- CLK_BASE_PHY_TX : chip_clocks.h
- CLK_BASE_RESERVED1 : chip_clocks.h
- CLK_BASE_RESERVED2 : chip_clocks.h
- CLK_BASE_RESERVED3 : chip_clocks.h
- CLK_BASE_RESERVED4 : chip_clocks.h
- CLK_BASE_RESERVED5 : chip_clocks.h
- CLK_BASE_RESERVED6 : chip_clocks.h
- CLK_BASE_RESERVED7 : chip_clocks.h
- CLK_BASE_SAFE : chip_clocks.h
- CLK_BASE_SDIO : chip_clocks.h
- CLK_BASE_SPIFI : chip_clocks.h
- CLK_BASE_SSP0 : chip_clocks.h
- CLK_BASE_SSP1 : chip_clocks.h
- CLK_BASE_UART0 : chip_clocks.h
- CLK_BASE_UART1 : chip_clocks.h
- CLK_BASE_UART2 : chip_clocks.h
- CLK_BASE_UART3 : chip_clocks.h
- CLK_BASE_USB0 : chip_clocks.h
- CLK_BASE_USB1 : chip_clocks.h
- CLK_CCU1_LAST : chip_clocks.h
- CLK_CCU2_LAST : chip_clocks.h
- CLK_CCU2_START : chip_clocks.h
- CLK_IDIV_A : chip_clocks.h
- CLK_IDIV_B : chip_clocks.h
- CLK_IDIV_C : chip_clocks.h
- CLK_IDIV_D : chip_clocks.h
- CLK_IDIV_E : chip_clocks.h
- CLK_IDIV_LAST : chip_clocks.h
- CLK_MX_BUS : chip_clocks.h
- CLK_MX_CREG : chip_clocks.h
- CLK_MX_DMA : chip_clocks.h
- CLK_MX_EEPROM : chip_clocks.h
- CLK_MX_EMC : chip_clocks.h
- CLK_MX_EMC_DIV : chip_clocks.h
- CLK_MX_ETHERNET : chip_clocks.h
- CLK_MX_FLASHA : chip_clocks.h
- CLK_MX_FLASHB : chip_clocks.h
- CLK_MX_GPIO : chip_clocks.h
- CLK_MX_LCD : chip_clocks.h
- CLK_MX_MXCORE : chip_clocks.h
- CLK_MX_QEI : chip_clocks.h
- CLK_MX_RITIMER : chip_clocks.h
- CLK_MX_SCT : chip_clocks.h
- CLK_MX_SCU : chip_clocks.h
- CLK_MX_SDIO : chip_clocks.h
- CLK_MX_SPIFI : chip_clocks.h
- CLK_MX_SSP0 : chip_clocks.h
- CLK_MX_SSP1 : chip_clocks.h
- CLK_MX_TIMER0 : chip_clocks.h
- CLK_MX_TIMER1 : chip_clocks.h
- CLK_MX_TIMER2 : chip_clocks.h
- CLK_MX_TIMER3 : chip_clocks.h
- CLK_MX_UART0 : chip_clocks.h
- CLK_MX_UART1 : chip_clocks.h
- CLK_MX_UART2 : chip_clocks.h
- CLK_MX_UART3 : chip_clocks.h
- CLK_MX_USB0 : chip_clocks.h
- CLK_MX_USB1 : chip_clocks.h
- CLK_MX_WWDT : chip_clocks.h
- CLK_RESERVED1 : chip_clocks.h
- CLK_RESERVED2 : chip_clocks.h
- CLK_RESERVED3 : chip_clocks.h
- CLK_RESERVED3A : chip_clocks.h
- CLK_RESERVED4 : chip_clocks.h
- CLK_RESERVED5 : chip_clocks.h
- CLK_RESERVED7 : chip_clocks.h
- CLK_RESERVED8 : chip_clocks.h
- CLK_SPIFI : chip_clocks.h
- CLK_USB0 : chip_clocks.h
- CLK_USB1 : chip_clocks.h
- CLKIN : swm_8xx.h
- CLKIN_32K : chip_clocks.h
- CLKIN_AUDIOPLL : chip_clocks.h
- CLKIN_CLKIN : chip_clocks.h
- CLKIN_CRYSTAL : chip_clocks.h
- CLKIN_ENET_RX : chip_clocks.h
- CLKIN_ENET_TX : chip_clocks.h
- CLKIN_IDIVA : chip_clocks.h
- CLKIN_IDIVB : chip_clocks.h
- CLKIN_IDIVC : chip_clocks.h
- CLKIN_IDIVD : chip_clocks.h
- CLKIN_IDIVE : chip_clocks.h
- CLKIN_IRC : chip_clocks.h
- CLKIN_MAINPLL : chip_clocks.h
- CLKIN_RESERVED1 : chip_clocks.h
- CLKIN_RESERVED2 : chip_clocks.h
- CLKIN_RESERVED3 : chip_clocks.h
- CLKIN_USBPLL : chip_clocks.h
- CLKINPUT_PD : chip_clocks.h
- CMD_SUCCESS : flash_001.h
- CMP_ENCTRL_DIS_IN_DS_PWD : cmp_001.h
- CMP_ENCTRL_DIS_IN_PWD : cmp_001.h
- CMP_ENCTRL_DISABLE : cmp_001.h
- CMP_ENCTRL_ENABLE : cmp_001.h
- CMP_HYS_10MV : cmp_001.h
- CMP_HYS_15MV : cmp_001.h
- CMP_HYS_5MV : cmp_001.h
- CMP_HYS_NONE : cmp_001.h
- CMP_INPUT_CMP_OTHER_IN0 : cmp_001.h
- CMP_INPUT_CMPx_IN0 : cmp_001.h
- CMP_INPUT_CMPx_IN1 : cmp_001.h
- CMP_INPUT_CMPx_IN2 : cmp_001.h
- CMP_INPUT_CMPx_IN3 : cmp_001.h
- CMP_INPUT_INTERNAL_09VBG : cmp_001.h
- CMP_INPUT_VREF_DIV : cmp_001.h
- CMP_INTEDGE_BOTH : cmp_001.h
- CMP_INTEDGE_FALLING : cmp_001.h
- CMP_INTEDGE_RISING : cmp_001.h
- COMPARE_ERROR : flash_001.h
- CONTROL_TRANSFER : HCD.h
- COUNT_ERROR : flash_001.h
- CRC_POLY_CCITT : crc_001.h
- CRC_POLY_CRC16 : crc_001.h
- CRC_POLY_CRC32 : crc_001.h
- CRC_POLY_LAST : crc_001.h