| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Embedded Artists' LPC4088 Developer's Kit

Documentation links
Embedded Artists LPC4088 Developer's Kit

Jumper configuration
The image below shows the default jumper configuration used for all EA4088 examples. Use this configuration for the examples unless an example alters this default setting in it's description.
EA1788 and EA4088 boards use the same default jumper setting.

Board recovery using the ISP pin
If the board's FLASH can no longer be programmed, the image in FLASH may be corrupt. To recover the board, the board must be reset with the ISP pin. To do this, hold down the SW6 button while pressing and releasing the reset button (SW1). On debuggers that reset the board prior to programming, the SW6 button should be held down until the programming cycle is started. Once started, it can be released.