| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
IP_CAN_STD_ID_RANGE_Entry_T Struct Reference
IP: CAN register block and driver

## Detailed Description

Standard ID Range structure.

Definition at line 695 of file can_001.h.

`#include "can_001.h"`

## Data Fields
IP_CAN_STD_ID_Entry_T | LowerID
IP_CAN_STD_ID_Entry_T | UpperID

## Field Documentation

IP_CAN_STD_ID_Entry_T LowerID

Lower ID Bound, should be in 11-bit value

Definition at line 696 of file can_001.h.

IP_CAN_STD_ID_Entry_T UpperID

Upper ID Bound, should be in 11-bit value

Definition at line 697 of file can_001.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/can_001.h