| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Structures | Macros
Class descriptors
Audio input device example | Audio input device example

## Detailed Description

## Data Structures
struct | USB_Descriptor_Configuration_t
| Type define for the device configuration descriptor structure. This must be defined in the application code, as the configuration descriptor contains several sub-descriptors which vary between devices, and which describe the device's usage to the host. More...

## Macros
#define | AUDIO_STREAM_EPNUM 1
| Endpoint number of the Audio isochronous streaming data endpoint.
#define | AUDIO_STREAM_EPSIZE ENDPOINT_MAX_SIZE(AUDIO_STREAM_EPNUM)
| Endpoint size in bytes of the Audio isochronous streaming data endpoint. The Windows audio stack requires at least 192 bytes for correct output, thus the smaller 128 byte maximum endpoint size on some of the smaller USB models will result in unavoidable distorted output.

## Macro Definition Documentation

#define AUDIO_STREAM_EPNUM 1

Endpoint number of the Audio isochronous streaming data endpoint.

Definition at line 53 of file Descriptors.h.

#define AUDIO_STREAM_EPSIZE ENDPOINT_MAX_SIZE(AUDIO_STREAM_EPNUM)

Endpoint size in bytes of the Audio isochronous streaming data endpoint. The Windows audio stack requires at least 192 bytes for correct output, thus the smaller 128 byte maximum endpoint size on some of the smaller USB models will result in unavoidable distorted output.

Definition at line 61 of file Descriptors.h.