| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
LPC18xx/43xx OTP Controller example
Misc examples

## Detailed Description

Example description
This example demonstrates the use of OTP controller functions in ROM driver.

Special connection requirements
There are no special connection requirements for this example.

Build procedures:
LPC18xx/43xx example quickstart for Keil uVision4
LPC18xx/43xx example quickstart for IAR EWARM
LPC18xx/43xx example quickstart for Code Red Xpresso

Supported boards and board setup:
Hitex 1850 evaluation boards
Hitex 4350 evaluation boards
Keil 1857 evaluation boards
Keil 4357 evaluation boards
NGX 1830 Xplorer boards
NGX 4330 Xplorer boards

Submitting LPCOpen issues:
Community support for LPCOpen

## Functions
static void | OTP_fix (volatile uint32_t dummy0, volatile uint32_t dummy1, volatile uint32_t dummy2, volatile uint32_t dummy3)
int | main (void)
| Main entry point.

## Function Documentation

int main | ( | void |  | ) |

Main entry point.

Main program body.

Returns
  Nothing

Definition at line 88 of file app_otp_funcs.c.

static void OTP_fix | ( | volatile uint32_t | dummy0,
|  | volatile uint32_t | dummy1,
|  | volatile uint32_t | dummy2,
|  | volatile uint32_t | dummy3
| ) |  |
| static

Definition at line 73 of file app_otp_funcs.c.