| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - u -

- U16_F : cc.h
- u16_t : cc.h
- U32_F : cc.h
- u32_t : cc.h
- u32Milliseconds : dfuutil_programming_dfu_ops.c
- u8_t : cc.h
- uart : uart_rom.c
- UART0_IRQHandler() : uart_rom.c
- UART1_IER_BITMASK : usart_001.h , usart_004.h
- UART1_IRQHandler() : uart.c
- UART_0 : usart_001.h
- UART_002_ENABLE : usart_002.h
- UART_002_SYNCEN : usart_002.h
- UART_1 : usart_001.h
- UART_2 : usart_001.h
- UART_3 : usart_001.h
- UART_4 : usart_001.h
- UART_ACCEPTED_BAUDRATE_ERROR : usart_001.h , usart_004.c
- UART_ACR_ABEOINT_CLR : usart_001.h , usart_004.h
- UART_ACR_ABTOINT_CLR : usart_001.h , usart_004.h
- UART_ACR_AUTO_RESTART : usart_001.h , usart_004.h
- UART_ACR_BITMASK : usart_001.h , usart_004.h
- UART_ACR_MODE : usart_001.h , usart_004.h
- UART_ACR_START : usart_004.h , usart_001.h
- UART_AUTOBAUD_MODE0 : usart_001.h
- UART_AUTOBAUD_MODE1 : usart_001.h
- UART_BLOCKING_TIMEOUT : usart_001.h
- UART_CALLBK_T : uartd_8xx.h
- UART_CLKPOL_FALLING : usart_002.h
- UART_CLKPOL_RISING : usart_002.h
- UART_DATABIT_5 : usart_001.h
- UART_DATABIT_6 : usart_001.h
- UART_DATABIT_7 : usart_001.h
- UART_DATABIT_8 : usart_001.h
- UART_DATALEN_7 : usart_002.h
- UART_DATALEN_8 : usart_002.h
- UART_DATALEN_9 : usart_002.h
- UART_DLL_MASKBIT : usart_001.h , usart_004.h
- UART_DLM_MASKBIT : usart_001.h , usart_004.h
- UART_DMA_REQ_T : uartd_8xx.h
- UART_FCR_BITMASK : usart_001.h , usart_004.h
- UART_FCR_DMAMODE_SEL : usart_001.h , usart_004.h
- UART_FCR_FIFO_EN : usart_001.h , usart_004.h
- UART_FCR_RX_RS : usart_001.h , usart_004.h
- UART_FCR_TRG_LEV0 : usart_001.h , usart_004.h
- UART_FCR_TRG_LEV1 : usart_001.h , usart_004.h
- UART_FCR_TRG_LEV2 : usart_004.h , usart_001.h
- UART_FCR_TRG_LEV3 : usart_001.h , usart_004.h
- UART_FCR_TX_RS : usart_001.h , usart_004.h
- UART_FDR_BITMASK : usart_001.h
- UART_FDR_DIVADDVAL : usart_001.h
- UART_FDR_MULVAL : usart_001.h , usart_004.c
- UART_FIFO_TRGLEV0 : usart_001.h , usart_002.h
- UART_FIFO_TRGLEV1 : usart_001.h , usart_002.h
- UART_FIFO_TRGLEV2 : usart_001.h , usart_002.h
- UART_FIFO_TRGLEV3 : usart_001.h , usart_002.h
- UART_FIFOLVL_BITMASK : usart_001.h
- UART_FIFOLVL_RXFIFOLVL : usart_001.h
- UART_FIFOLVL_TXFIFOLVL : usart_001.h
- UART_HANDLE_T : uartd_8xx.h
- UART_HDEN_HDEN : usart_001.h
- UART_ICR_BITMASK : usart_001.h
- UART_ICR_FIXPULSE_EN : usart_001.h
- UART_ICR_IRDAEN : usart_001.h
- UART_ICR_IRDAINV : usart_001.h
- UART_ICR_PULSEDIV : usart_001.h
- UART_IER_ABEOINT : usart_004.h
- UART_IER_ABEOINT_EN : usart_001.h
- UART_IER_ABTOINT : usart_004.h
- UART_IER_ABTOINT_EN : usart_001.h
- UART_IER_BITMASK : usart_001.h , usart_004.h
- UART_IER_CTSINT : usart_004.h
- UART_IER_CTSINT_EN : usart_001.h
- UART_IER_MSINT : usart_004.h
- UART_IER_MSINT_EN : usart_001.h
- UART_IER_RBRINT : usart_004.h
- UART_IER_RBRINT_EN : usart_001.h
- UART_IER_RLSINT : usart_004.h
- UART_IER_RLSINT_EN : usart_001.h
- UART_IER_THREINT : usart_004.h
- UART_IER_THREINT_EN : usart_001.h
- UART_IIR_ABEO_INT : usart_001.h , usart_004.h
- UART_IIR_ABTO_INT : usart_001.h , usart_004.h
- UART_IIR_BITMASK : usart_001.h , usart_004.h
- UART_IIR_FIFO_EN : usart_001.h , usart_004.h
- UART_IIR_INTID_CTI : usart_001.h , usart_004.h
- UART_IIR_INTID_MASK : usart_001.h , usart_004.h
- UART_IIR_INTID_MODEM : usart_001.h , usart_004.h
- UART_IIR_INTID_RDA : usart_001.h , usart_004.h
- UART_IIR_INTID_RLS : usart_001.h , usart_004.h
- UART_IIR_INTID_THRE : usart_001.h , usart_004.h
- UART_IIR_INTSTAT_PEND : usart_004.h , usart_001.h
- UART_INTCFG_ABEO : usart_001.h
- UART_INTCFG_ABTO : usart_001.h
- UART_INTCFG_CTS : usart_001.h
- UART_INTCFG_MS : usart_001.h
- UART_INTCFG_RBR : usart_001.h
- UART_INTCFG_RLS : usart_001.h
- UART_INTCFG_THRE : usart_001.h
- uart_interrupt_menu : uart.c
- uart_interrupt_menu1 : uart.c
- uart_interrupt_menu2 : uart.c
- uart_interrupt_menu3 : uart.c
- uart_interrupt_menu4 : uart.c
- UART_INTSTS_ABEO : usart_001.h
- UART_INTSTS_ABTO : usart_001.h
- UART_INTSTS_ERROR : usart_001.h
- UART_INTSTS_RTR : usart_001.h
- UART_INTSTS_RTS : usart_001.h
- UART_IRQHandler() : uart.c
- UART_LCR_BITMASK : usart_001.h , usart_004.h
- UART_LCR_BREAK_EN : usart_001.h , usart_004.h
- UART_LCR_DLAB_EN : usart_001.h , usart_004.h
- UART_LCR_PARITY_DIS : usart_001.h , usart_004.h
- UART_LCR_PARITY_EN : usart_001.h , usart_004.h
- UART_LCR_PARITY_EVEN : usart_001.h , usart_004.h
- UART_LCR_PARITY_F_0 : usart_001.h , usart_004.h
- UART_LCR_PARITY_F_1 : usart_001.h , usart_004.h
- UART_LCR_PARITY_ODD : usart_001.h , usart_004.h
- UART_LCR_SBS_1BIT : usart_001.h , usart_004.h
- UART_LCR_SBS_2BIT : usart_001.h , usart_004.h
- UART_LCR_WLEN5 : usart_001.h , usart_004.h
- UART_LCR_WLEN6 : usart_001.h , usart_004.h
- UART_LCR_WLEN7 : usart_001.h , usart_004.h
- UART_LCR_WLEN8 : usart_001.h , usart_004.h
- UART_LINESTAT_BI : usart_001.h
- UART_LINESTAT_FE : usart_001.h
- UART_LINESTAT_OE : usart_001.h
- UART_LINESTAT_PE : usart_001.h
- UART_LINESTAT_RDR : usart_001.h
- UART_LINESTAT_RXFE : usart_001.h
- UART_LINESTAT_TEMT : usart_001.h
- UART_LINESTAT_THRE : usart_001.h
- UART_LOAD_DLL : usart_001.h
- UART_LOAD_DLM : usart_001.h
- UART_LSR_BI : usart_001.h , usart_004.h
- UART_LSR_BITMASK : usart_001.h , usart_004.h
- UART_LSR_FE : usart_001.h , usart_004.h
- UART_LSR_OE : usart_001.h , usart_004.h
- UART_LSR_PE : usart_001.h , usart_004.h
- UART_LSR_RDR : usart_001.h , usart_004.h
- UART_LSR_RXFE : usart_001.h , usart_004.h
- UART_LSR_TEMT : usart_001.h , usart_004.h
- UART_LSR_THRE : usart_001.h , usart_004.h
- UART_MCR_AUTO_CTS_EN : usart_001.h , usart_004.h
- UART_MCR_AUTO_RTS_EN : usart_001.h , usart_004.h
- UART_MCR_BITMASK : usart_001.h , usart_004.h
- UART_MCR_DTR_CTRL : usart_001.h , usart_004.h
- UART_MCR_LOOPB_EN : usart_001.h , usart_004.h
- UART_MCR_RTS_CTRL : usart_001.h , usart_004.h
- UART_MODEM_MODE_AUTO_CTS : usart_001.h
- UART_MODEM_MODE_AUTO_RTS : usart_001.h
- UART_MODEM_MODE_LOOPBACK : usart_001.h
- UART_MODEM_PIN_DTR : usart_001.h
- UART_MODEM_PIN_RTS : usart_001.h
- UART_MODEM_STAT_CTS : usart_001.h
- UART_MODEM_STAT_DCD : usart_001.h
- UART_MODEM_STAT_DELTA_CTS : usart_001.h
- UART_MODEM_STAT_DELTA_DCD : usart_001.h
- UART_MODEM_STAT_DELTA_DSR : usart_001.h
- UART_MODEM_STAT_DSR : usart_001.h
- UART_MODEM_STAT_LO2HI_RI : usart_001.h
- UART_MODEM_STAT_RI : usart_001.h
- UART_MSR_BITMASK : usart_001.h , usart_004.h
- UART_MSR_CTS : usart_001.h , usart_004.h
- UART_MSR_DCD : usart_001.h , usart_004.h
- UART_MSR_DELTA_CTS : usart_001.h , usart_004.h
- UART_MSR_DELTA_DCD : usart_001.h , usart_004.h
- UART_MSR_DELTA_DSR : usart_001.h , usart_004.h
- UART_MSR_DSR : usart_001.h , usart_004.h
- UART_MSR_LO2HI_RI : usart_001.h , usart_004.h
- UART_MSR_RI : usart_001.h , usart_004.h
- UART_PARITY_EVEN : usart_001.h , usart_002.h
- UART_PARITY_NONE : usart_001.h , usart_002.h
- UART_PARITY_ODD : usart_001.h , usart_002.h
- UART_PARITY_SP_0 : usart_001.h
- UART_PARITY_SP_1 : usart_001.h
- UART_RB_SIZE : uart.c
- UART_RBR_MASKBIT : usart_001.h , usart_004.h
- UART_RING_BUFSIZE : usart_001.h
- UART_ROM_MEM_SIZE : uartd_8xx.h
- UART_RS485ADRMATCH_BITMASK : usart_001.h
- UART_RS485CTRL_AADEN : usart_001.h , usart_004.h
- UART_RS485CTRL_BITMASK : usart_001.h , usart_004.h
- UART_RS485CTRL_DCTRL_EN : usart_001.h , usart_004.h
- UART_RS485CTRL_NMM_EN : usart_001.h , usart_004.h
- UART_RS485CTRL_OINV_1 : usart_001.h , usart_004.h
- UART_RS485CTRL_RX_DIS : usart_001.h , usart_004.h
- UART_RS485CTRL_SEL_DTR : usart_001.h , usart_004.h
- UART_RS485DLY_BITMASK : usart_001.h
- UART_SCICTRL_GUARDTIME : usart_001.h
- UART_SCICTRL_NACKDIS : usart_001.h
- UART_SCICTRL_PROTSEL_T1 : usart_001.h
- UART_SCICTRL_SCIEN : usart_001.h
- UART_SCICTRL_TXRETRY : usart_001.h
- UART_SCR_BIMASK : usart_001.h
- UART_STOPBIT_1 : usart_001.h
- UART_STOPBIT_2 : usart_001.h
- UART_STOPLEN_1 : usart_002.h
- UART_STOPLEN_2 : usart_002.h
- UART_SYNCCTRL_CCCLR : usart_001.h
- UART_SYNCCTRL_CSCEN : usart_001.h
- UART_SYNCCTRL_CSRC_MASTER : usart_001.h
- UART_SYNCCTRL_FES : usart_001.h
- UART_SYNCCTRL_STARTSTOPDISABLE : usart_001.h
- UART_SYNCCTRL_SYNC : usart_001.h
- UART_SYNCCTRL_TSBYPASS : usart_001.h
- UART_TER1_BITMASK : usart_001.h
- UART_TER1_TXEN : usart_001.h
- UART_TER2_BITMASK : usart_001.h
- UART_TER2_TXEN : usart_001.h
- UART_TEST_DEFAULT_BAUDRATE : uart.c
- UART_TEST_REPEAT_NUMBER : uart.c
- UART_THR_MASKBIT : usart_001.h
- UART_TX_FIFO_SIZE : usart_001.h , usart_004.h
- uartABComplete : uart.c
- uartDMA_menu : uart.c
- uartPolling_menu1 : uart.c
- uartPolling_menu2 : uart.c
- uartPolling_menu3 : uart.c
- uartPolling_menu4 : uart.c
- uartPolling_menu5 : uart.c
- UARTx_IRQHandler : uart.c
- UARTx_IRQn : uart.c
- UCHAR : integer.h
- UCOS_MIN_STACK_SZ : lpc43xx_dualcore_config.h
- UDA1380_I2C_BUS : board_ea_devkit_17884088.h , board_hitex_eva_18504350.h , board_keil_mcb_18574357.h , board_ngx_xplorer_18304330.h
- UDA1380_Init() : uda1380.c , uda1380.h
- UDA1380_LINE_IN : uda1380.h
- UDA1380_MIC_IN_L : uda1380.h
- UDA1380_MIC_IN_LR : uda1380.h
- UDA1380_REG_ADC_DEFAULT_VALUE : uda1380.h
- UDA1380_REG_AGC_DEFAULT_VALUE : uda1380.h
- UDA1380_REG_ANAMIX_DEFAULT_VALUE : uda1380.h
- UDA1380_REG_DECVOL_DEFAULT_VALUE : uda1380.h
- UDA1380_REG_EVALCLK_DEFAULT_VALUE : uda1380.h
- UDA1380_REG_HEADAMP_DEFAULT_VALUE : uda1380.h
- UDA1380_REG_I2S_DEFAULT_VALUE : uda1380.h
- UDA1380_REG_L3_DEFAULT_VALUE : uda1380.h
- UDA1380_REG_MIXSDO_DEFAULT_VALUE : uda1380.h
- UDA1380_REG_MIXVOL_DEFAULT_VALUE : uda1380.h
- UDA1380_REG_MODEBBT_DEFAULT_VALUE : uda1380.h
- UDA1380_REG_MSTRMUTE_DEFAULT_VALUE : uda1380.h
- UDA1380_REG_MSTRVOL_DEFAULT_VALUE : uda1380.h
- UDA1380_REG_PGA_DEFAULT_VALUE : uda1380.h
- UDA1380_REG_PWRCTRL_DEFAULT_VALUE : uda1380.h
- UDA1380_REG_Read() : uda1380.c , uda1380.h
- UDA1380_REG_VerifyMult() : uda1380.c , uda1380.h
- UDA1380_REG_Write() : uda1380.c , uda1380.h
- UDA1380_REG_WriteMult() : uda1380.c , uda1380.h
- UDA1380_REG_WriteVerify() : uda1380.c , uda1380.h
- UDA1380_U8 : uda1380.h
- UDA_ADC_CTRL : uda1380.h
- UDA_AGC_CTRL : uda1380.h
- UDA_ANALOG_CTRL : uda1380.h
- UDA_BUS_CTRL : uda1380.h
- UDA_DEC_VOL_CTRL : uda1380.h
- UDA_decimator_regs_dat : uda1380.c
- UDA_EVALM_CLK : uda1380.h
- UDA_HPAMP_CTRL : uda1380.h
- UDA_interfil_regs_dat : uda1380.c
- UDA_MASTER_VOL_CTRL : uda1380.h
- UDA_MIXER_FILTER_CTRL : uda1380.h
- UDA_MIXER_VOL_CTRL : uda1380.h
- UDA_MODE_CTRL : uda1380.h
- UDA_MUTE_CTRL : uda1380.h
- UDA_PGA_CTRL : uda1380.h
- UDA_POWER_CTRL : uda1380.h
- UDA_sys_regs_dat : uda1380.c
- UDA_TOTAL_REG : uda1380.h
- UDIV_ROUNDUP : fatutil.h
- UDP_DEBUG : lwipopts.h
- UDP_LPC_EMAC : lwipopts.h
- uFrameCMask : EHCI.h
- uFrameCProgMask : EHCI.h
- uFrameSMask : EHCI.h
- UINT : integer.h
- uint32_t : EHCI.h
- uint_reg_t : Common.h
- ULONG : integer.h
- umem : uart_rom.c
- UNDERRUN_ERR_EN : uartd_8xx.h
- UNICODE_STRING_LENGTH : StillImageClassCommon.h
- UnicodeString : StdDescriptors.h
- UnitID : AudioClassCommon.h
- UNRECOVERABLE_ERROR_INTERRUPT : OHCI.h
- UNS_16 : lpc_types.h
- UNS_32 : lpc_types.h
- UNS_64 : lpc_types.h
- UNS_8 : lpc_types.h
- US_TIMEOUT : sdif_18xx_43xx.h
- UsageFault_Handler() : cr_startup_lpc18xx43xx.c , cr_startup_lpc43xx_m0.c , cr_freertos_startup_lpc18xx43xx.c , cr_ucos_iii_startup_lpc18xx43xx.c , cr_startup_lpc18xx43xx.c , cr_startup_lpc43xx_m0.c , cr_freertos_startup_lpc17xx40xx.c , cr_ucos_iii_startup_lpc17xx40xx.c , cr_startup_lpc17xx40xx.c
- USB : diskio.c
- USB0_IRQHandler() : dfuutil_programming_dfu_ops.c
- USB1_IRQHandler() : dfuutil_programming_dfu_ops.c
- USB_Attach() : USBController.h
- USB_Audio_Descriptor_FeatureUnit_t : AudioClassCommon.h
- USB_Audio_Descriptor_Format_t : AudioClassCommon.h
- USB_Audio_Descriptor_InputTerminal_t : AudioClassCommon.h
- USB_Audio_Descriptor_Interface_AC_t : AudioClassCommon.h
- USB_Audio_Descriptor_Interface_AS_t : AudioClassCommon.h
- USB_Audio_Descriptor_OutputTerminal_t : AudioClassCommon.h
- USB_Audio_Descriptor_StreamEndpoint_Spc_t : AudioClassCommon.h
- USB_Audio_Descriptor_StreamEndpoint_Std_t : AudioClassCommon.h
- USB_Audio_SampleFreq_t : AudioClassCommon.h
- USB_Audio_StdDescriptor_FeatureUnit_t : AudioClassCommon.h
- USB_Audio_StdDescriptor_Format_t : AudioClassCommon.h
- USB_Audio_StdDescriptor_InputTerminal_t : AudioClassCommon.h
- USB_Audio_StdDescriptor_Interface_AC_t : AudioClassCommon.h
- USB_Audio_StdDescriptor_Interface_AS_t : AudioClassCommon.h
- USB_Audio_StdDescriptor_OutputTerminal_t : AudioClassCommon.h
- USB_Audio_StdDescriptor_StreamEndpoint_Spc_t : AudioClassCommon.h
- USB_Audio_StdDescriptor_StreamEndpoint_Std_t : AudioClassCommon.h
- USB_CAN_BE_BOTH : USBMode.h
- USB_CAN_BE_DEVICE : USBMode.h
- USB_CAN_BE_HOST : USBMode.h
- USB_CB_T : usbd_api.h , usbd_core.h
- USB_CDC_Descriptor_FunctionalACM_t : CDCClassCommon.h
- USB_CDC_Descriptor_FunctionalHeader_t : CDCClassCommon.h
- USB_CDC_Descriptor_FunctionalUnion_t : CDCClassCommon.h
- USB_CDC_StdDescriptor_FunctionalACM_t : CDCClassCommon.h
- USB_CDC_StdDescriptor_FunctionalHeader_t : CDCClassCommon.h
- USB_CDC_StdDescriptor_FunctionalUnion_t : CDCClassCommon.h
- USB_CONFIG_ATTR_BUSPOWERED : StdDescriptors.h
- USB_CONFIG_ATTR_REMOTEWAKEUP : StdDescriptors.h
- USB_CONFIG_ATTR_SELFPOWERED : StdDescriptors.h
- USB_CONFIG_BUS_POWERED : usbd.h
- USB_CONFIG_POWER_MA : usbd.h , StdDescriptors.h
- USB_CONFIG_POWERED_MASK : usbd.h
- USB_CONFIG_REMOTE_WAKEUP : usbd.h
- USB_CONFIG_SELF_POWERED : usbd.h
- USB_CONFIGUARTION_DESC_SIZE : usbd_desc.h , usbd.h
- USB_CONFIGURATION_DESCRIPTOR_TYPE : usbd.h
- USB_Control_Request_t : StdRequestType.h
- USB_ControlRequest : USBTask.h
- USB_CSCP_IADDeviceClass : StdDescriptors.h
- USB_CSCP_IADDeviceProtocol : StdDescriptors.h
- USB_CSCP_IADDeviceSubclass : StdDescriptors.h
- USB_CSCP_NoDeviceClass : StdDescriptors.h
- USB_CSCP_NoDeviceProtocol : StdDescriptors.h
- USB_CSCP_NoDeviceSubclass : StdDescriptors.h
- USB_CSCP_VendorSpecificClass : StdDescriptors.h
- USB_CSCP_VendorSpecificProtocol : StdDescriptors.h
- USB_CSCP_VendorSpecificSubclass : StdDescriptors.h
- USB_CurrentMode : USBController.c , USBController.h
- usb_data_buffer : EndpointCommon.h
- usb_data_buffer_IN : EndpointCommon.h
- usb_data_buffer_IN_index : EndpointCommon.h
- usb_data_buffer_index : EndpointCommon.h
- usb_data_buffer_OUT : EndpointCommon.h
- usb_data_buffer_OUT_index : EndpointCommon.h
- usb_data_buffer_OUT_size : EndpointCommon.h
- usb_data_buffer_size : EndpointCommon.h
- USB_DATA_BUFFER_TEM_LENGTH : EndpointCommon.h
- USB_DCON : Endpoint_LPC11Uxx.h
- USB_DCON_C : Endpoint_LPC11Uxx.h
- USB_DEBUG_DESCRIPTOR_TYPE : usbd.h
- USB_Descriptor_ClassSubclassProtocol_t : StdDescriptors.h
- USB_Descriptor_Configuration_Header_t : StdDescriptors.h
- USB_Descriptor_Device_t : StdDescriptors.h
- USB_Descriptor_DeviceQualifier_t : StdDescriptors.h
- USB_Descriptor_Endpoint_t : StdDescriptors.h
- USB_Descriptor_Header_t : StdDescriptors.h
- USB_Descriptor_HIDReport_Datatype_t : HIDClassCommon.h
- USB_Descriptor_Interface_Association_t : StdDescriptors.h
- USB_Descriptor_Interface_t : StdDescriptors.h
- USB_Descriptor_String_t : StdDescriptors.h
- USB_DescriptorMemorySpaces_t : DeviceStandardReq.h
- USB_DescriptorTypes_t : StdDescriptors.h
- USB_Detach() : USBController.h
- USB_DEVICE_CLASS_APP : usbd.h
- USB_DEVICE_CLASS_AUDIO : usbd.h
- USB_DEVICE_CLASS_COMMUNICATIONS : usbd.h
- USB_DEVICE_CLASS_HUB : usbd.h
- USB_DEVICE_CLASS_HUMAN_INTERFACE : usbd.h
- USB_DEVICE_CLASS_MISCELLANEOUS : usbd.h
- USB_DEVICE_CLASS_MONITOR : usbd.h
- USB_DEVICE_CLASS_PHYSICAL_INTERFACE : usbd.h
- USB_DEVICE_CLASS_POWER : usbd.h
- USB_DEVICE_CLASS_PRINTER : usbd.h
- USB_DEVICE_CLASS_RESERVED : usbd.h
- USB_DEVICE_CLASS_STORAGE : usbd.h
- USB_DEVICE_CLASS_VENDOR_SPECIFIC : usbd.h
- USB_Device_ClearSetFeature() : DeviceStandardReq.c
- USB_Device_ConfigurationNumber : DeviceStandardReq.c , DeviceStandardReq.h
- USB_Device_ControlEndpointSize : Endpoint_LPC11Uxx.h , Endpoint_LPC17xx.h , Endpoint_LPC18xx.h
- USB_Device_CurrentlySelfPowered : DeviceStandardReq.c , DeviceStandardReq.h
- USB_DEVICE_DESC_SIZE : usbd_desc.h , usbd.h
- USB_DEVICE_DESCRIPTOR_TYPE : usbd.h
- USB_Device_DisableSOFEvents() : Device_LPC11Uxx.h , Device_LPC18xx.h , Device_LPC17xx.h
- USB_Device_EnableSOFEvents() : Device_LPC11Uxx.h , Device_LPC17xx.h , Device_LPC18xx.h
- USB_Device_GetConfiguration() : DeviceStandardReq.c
- USB_Device_GetDescriptor() : DeviceStandardReq.c
- USB_Device_GetFrameNumber() : Device_LPC11Uxx.h , Device_LPC18xx.h , Endpoint_LPC17xx.h
- USB_Device_GetStatus() : DeviceStandardReq.c
- USB_DEVICE_OPT_FULLSPEED : Device_LPC11Uxx.h , Device_LPC18xx.h , Device_LPC17xx.h
- USB_DEVICE_OPT_LOWSPEED : Device_LPC11Uxx.h , Device_LPC17xx.h
- USB_Device_ProcessControlRequest() : DeviceStandardReq.c
- USB_DEVICE_QUALI_SIZE : usbd_desc.h , usbd.h
- USB_DEVICE_QUALIFIER_DESCRIPTOR_TYPE : usbd.h
- USB_Device_RemoteWakeupEnabled : DeviceStandardReq.c , DeviceStandardReq.h
- USB_Device_SendRemoteWakeup() : Device_LPC11Uxx.h , Device_LPC18xx.h , Device.c , Device_LPC17xx.h
- USB_Device_SetAddress() : DeviceStandardReq.c
- USB_Device_SetConfiguration() : DeviceStandardReq.c
- USB_Device_SetDeviceAddress() : Endpoint_LPC17xx.h
- USB_Device_States_t : Device.h
- usb_device_tasks() : dualcore_common.h , MassStorage_ucosiii.c
- USB_DeviceDescriptor : dfuutil_programming_dfu_ops.c
- USB_DeviceQualifier : dfuutil_programming_dfu_ops.c
- USB_DeviceState : USBTask.h
- USB_DeviceTask() : USBTask.c
- USB_DFU_CAN_DOWNLOAD : usbd_dfu.h
- USB_DFU_CAN_UPLOAD : usbd_dfu.h
- USB_DFU_DESCRIPTOR_SIZE : usbd_dfu.h
- USB_DFU_DESCRIPTOR_TYPE : usbd_dfu.h
- USB_DFU_IF_NUM : usbd_dfu.h
- usb_dfu_init() : dfuutil_programming_dfu_ops.c
- USB_DFU_MANIFEST_TOL : usbd_dfu.h
- USB_DFU_SUBCLASS : usbd_dfu.h
- USB_DFU_WILL_DETACH : usbd_dfu.h
- USB_DFU_XFER_SIZE : usbd_dfu.h , app_usbd_cfg.h
- USB_Disable() : USBController.h , USBController.c
- USB_DRESET_C : Endpoint_LPC11Uxx.h
- USB_DSUS : Endpoint_LPC11Uxx.h
- USB_DSUS_C : Endpoint_LPC11Uxx.h
- USB_EN : Endpoint_LPC11Uxx.h
- USB_ENDPOINT_0_HS_MAXP : usbd.h
- USB_ENDPOINT_0_LS_MAXP : usbd.h
- USB_ENDPOINT_BULK_HS_MAXP : usbd.h
- USB_ENDPOINT_DESC_SIZE : usbd_desc.h , usbd.h
- USB_ENDPOINT_DESCRIPTOR_TYPE : usbd.h
- USB_ENDPOINT_DIRECTION_MASK : usbd.h
- USB_ENDPOINT_IN : usbd.h
- USB_ENDPOINT_OUT : usbd.h
- USB_ENDPOINT_SYNC_ADAPTIVE : usbd.h
- USB_ENDPOINT_SYNC_ASYNCHRONOUS : usbd.h
- USB_ENDPOINT_SYNC_MASK : usbd.h
- USB_ENDPOINT_SYNC_NO_SYNCHRONIZATION : usbd.h
- USB_ENDPOINT_SYNC_SYNCHRONOUS : usbd.h
- USB_ENDPOINT_TYPE_BULK : usbd.h
- USB_ENDPOINT_TYPE_CONTROL : usbd.h
- USB_ENDPOINT_TYPE_INTERRUPT : usbd.h
- USB_ENDPOINT_TYPE_ISOCHRONOUS : usbd.h
- USB_ENDPOINT_TYPE_MASK : usbd.h
- USB_ENDPOINT_USAGE_DATA : usbd.h
- USB_ENDPOINT_USAGE_FEEDBACK : usbd.h
- USB_ENDPOINT_USAGE_IMPLICIT_FEEDBACK : usbd.h
- USB_ENDPOINT_USAGE_MASK : usbd.h
- USB_ENDPOINT_USAGE_RESERVED : usbd.h
- USB_EP_HANDLER_T : usbd_core.h , usbd_api.h
- USB_Event_Stub() : Events.c
- USB_EVT_DEV_ERROR : usbd_hw.h
- USB_EVT_DEV_STATE : usbd_hw.h
- USB_EVT_IN : usbd_hw.h
- USB_EVT_IN_DMA_EOT : usbd_hw.h
- USB_EVT_IN_DMA_ERR : usbd_hw.h
- USB_EVT_IN_DMA_NDR : usbd_hw.h
- USB_EVT_IN_NAK : usbd_hw.h
- USB_EVT_IN_STALL : usbd_hw.h
- USB_EVT_OUT : usbd_hw.h
- USB_EVT_OUT_DMA_EOT : usbd_hw.h
- USB_EVT_OUT_DMA_ERR : usbd_hw.h
- USB_EVT_OUT_DMA_NDR : usbd_hw.h
- USB_EVT_OUT_NAK : usbd_hw.h
- USB_EVT_OUT_STALL : usbd_hw.h
- USB_EVT_RESET : usbd_hw.h
- USB_EVT_SETUP : usbd_hw.h
- USB_EVT_SOF : usbd_hw.h
- USB_FEATURE_ENDPOINT_STALL : usbd.h
- USB_FEATURE_REMOTE_WAKEUP : usbd.h
- USB_Feature_Selectors_t : StdRequestType.h
- USB_FEATURE_TEST_MODE : usbd.h
- USB_FORCED_FULLSPEED : LPCUSBlibConfig.h
- USB_FS_MAX_BULK_PACKET : app_usbd_cfg.h
- USB_FsConfigDescriptor : dfuutil_programming_dfu_ops.c
- USB_GetHIDReportItemInfo() : HIDParser.c , HIDParser.h
- USB_GetHIDReportSize() : HIDParser.h , HIDParser.c
- USB_GetNextDescriptor() : ConfigDescriptor.h
- USB_GetNextDescriptorComp() : ConfigDescriptor.c , ConfigDescriptor.h
- USB_GetNextDescriptorOfType() : ConfigDescriptor.h , ConfigDescriptor.c
- USB_GetNextDescriptorOfTypeAfter() : ConfigDescriptor.h , ConfigDescriptor.c
- USB_GetNextDescriptorOfTypeBefore() : ConfigDescriptor.h , ConfigDescriptor.c
- USB_GETSTATUS_ENDPOINT_STALL : usbd.h
- USB_GETSTATUS_REMOTE_WAKEUP : usbd.h
- USB_GETSTATUS_SELF_POWERED : usbd.h
- USB_HID_Descriptor_HID_t : HIDClassCommon.h
- USB_HID_StdDescriptor_HID_t : HIDClassCommon.h
- USB_Host_ClearEndpointStall() : HostStandardReq.c , HostStandardReq.h
- USB_Host_ClearRemoteWakeupSent() : Host.h
- USB_Host_ConfigurationNumber : HostStandardReq.c , HostStandardReq.h
- USB_Host_ControlPipeSize : Host.c , Host.h
- USB_Host_DeEnumerate() : EHCI.h , Host.c
- USB_HOST_DEVICEADDRESS : Host.h
- USB_Host_DisableSOFEvents() : Host.h
- USB_Host_EnableSOFEvents() : Host.h
- USB_Host_Enumerate() : EHCI.h , Host.c
- USB_Host_EnumerationErrorCodes_t : Host.h
- USB_Host_ErrorCodes_t : Host.h
- USB_Host_GetActiveHost() : Host.c , Host.h
- USB_Host_GetConfigDescriptor_ErrorCodes_t : ConfigDescriptor.h
- USB_Host_GetDeviceConfigDescriptor() : ConfigDescriptor.h , ConfigDescriptor.c
- USB_Host_GetDeviceDescriptor() : HostStandardReq.c , HostStandardReq.h
- USB_Host_GetDeviceSpeed() : Host.c
- USB_Host_GetDeviceStatus() : HostStandardReq.c , HostStandardReq.h
- USB_Host_GetDeviceStringDescriptor() : HostStandardReq.c , HostStandardReq.h
- USB_Host_GetFrameNumber() : Host.c
- USB_Host_IsBusResetComplete() : Host.h
- USB_Host_IsBusSuspended() : Host.h
- USB_Host_IsDeviceFullSpeed() : Host.h
- USB_Host_IsRemoteWakeupSent() : Host.h
- USB_Host_IsResumeFromWakeupRequestSent() : Host.h
- USB_Host_ProcessNextHostState() : Host.c
- USB_Host_ResetBus() : Host.h
- USB_Host_ResumeBus() : Host.h
- USB_Host_ResumeFromWakeupRequest() : Host.h
- USB_Host_SendControlErrorCodes_t : HostStandardReq.h
- USB_Host_SendControlRequest() : HostStandardReq.h , HostStandardReq.c
- USB_Host_SetActiveHost() : Host.c
- USB_Host_SetDeviceConfiguration() : HostStandardReq.c , HostStandardReq.h
- USB_Host_SetDeviceSpeed() : Host.c
- USB_Host_SetInterfaceAltSetting() : HostStandardReq.c , HostStandardReq.h
- USB_Host_States_t : Host.h
- USB_Host_SuspendBus() : Host.h
- usb_host_tasks() : dualcore_common.h
- USB_HOST_TIMEOUT_MS : HostStandardReq.h , Host.h
- USB_Host_WaitMS() : Host.c
- USB_HostState : USBTask.h
- USB_HostTask() : USBTask.c
- USB_HS_MAX_BULK_PACKET : app_usbd_cfg.h
- USB_HsConfigDescriptor : dfuutil_programming_dfu_ops.c
- USB_Init() : USBController.h , USBController.c
- USB_Init_Device() : USBController.c
- USB_Init_Host() : USBController.c
- USB_INTERFACE_ASSOCIATION_DESCRIPTOR_TYPE : usbd.h
- USB_INTERFACE_DESC_SIZE : usbd.h , usbd_desc.h
- USB_INTERFACE_DESCRIPTOR_TYPE : usbd.h
- USB_Interface_Event() : usbd_adcuser.h
- USB_INTERFACE_POWER_DESCRIPTOR_TYPE : usbd.h
- USB_IntOnNAK_AI : Endpoint_LPC11Uxx.h
- USB_IntOnNAK_AO : Endpoint_LPC11Uxx.h
- USB_IntOnNAK_CI : Endpoint_LPC11Uxx.h
- USB_IntOnNAK_CO : Endpoint_LPC11Uxx.h
- USB_IsInitialized : USBTask.h , USBTask.c
- USB_KeyboardReport_Data_t : HIDClassCommon.h
- USB_LPM : Endpoint_LPC11Uxx.h
- USB_LPM_SUS : Endpoint_LPC11Uxx.h
- USB_MAX_EP_NUM : app_usbd_cfg.h
- USB_MAX_IF_NUM : app_usbd_cfg.h
- USB_MAX_PACKET0 : app_usbd_cfg.h
- USB_Memory_Alloc() : USBMemory.c , USBMemory.h
- USB_Memory_Free() : USBMemory.c , USBMemory.h
- USB_Memory_Init() : USBMemory.h
- USB_MIDI_Descriptor_AudioInterface_AS_t : MIDIClassCommon.h
- USB_MIDI_Descriptor_InputJack_t : MIDIClassCommon.h
- USB_MIDI_Descriptor_Jack_Endpoint_t : MIDIClassCommon.h
- USB_MIDI_Descriptor_OutputJack_t : MIDIClassCommon.h
- USB_MIDI_StdDescriptor_AudioInterface_AS_t : MIDIClassCommon.h
- USB_MIDI_StdDescriptor_InputJack_t : MIDIClassCommon.h
- USB_MIDI_StdDescriptor_Jack_Endpoint_t : MIDIClassCommon.h
- USB_MIDI_StdDescriptor_OutputJack_t : MIDIClassCommon.h
- USB_MODE_Device : USBController.h
- USB_MODE_Host : USBController.h
- USB_MODE_None : USBController.h
- USB_MODE_UID : USBController.h
- USB_Modes_t : USBController.h
- USB_MouseReport_Data_t : HIDClassCommon.h
- usb_msdev_func() : MassStorage_ucosiii.c , usbmsdev.c
- usb_msdev_task() : MassStorage_ucosiii.c
- USB_OPT_AUTO_PLL : USBController.h
- USB_OPT_MANUAL_PLL : USBController.h
- USB_OPT_REG_DISABLED : USBController.h
- USB_OPT_REG_ENABLED : USBController.h
- USB_Options : USBController.h
- USB_OTG_DESCRIPTOR_TYPE : usbd.h
- USB_OTHER_SPEED_CONF_SIZE : usbd.h , usbd_desc.h
- USB_OTHER_SPEED_CONFIG_DESCRIPTOR_TYPE : usbd.h
- USB_PARAM_CB_T : usbd_core.h , usbd_api.h
- USB_PLL_ON : Endpoint_LPC11Uxx.h
- USB_ProcessHIDReport() : HIDParser.c , HIDParser.h
- USB_ReadWriteFile() : MassStorageHost.c
- USB_REG : HAL_LPC17xx.h , HAL_LPC18xx.h
- USB_REG_BASE_ADDR : HAL_LPC18xx.h
- USB_REMOTE_WAKE : Endpoint_LPC11Uxx.h
- USB_REQ_DFU_ABORT : usbd_dfu.h
- USB_REQ_DFU_CLRSTATUS : usbd_dfu.h
- USB_REQ_DFU_DETACH : usbd_dfu.h
- USB_REQ_DFU_DNLOAD : usbd_dfu.h
- USB_REQ_DFU_GETSTATE : usbd_dfu.h
- USB_REQ_DFU_GETSTATUS : usbd_dfu.h
- USB_REQ_DFU_UPLOAD : usbd_dfu.h
- USB_REQUEST_CLEAR_FEATURE : usbd.h
- USB_REQUEST_GET_CONFIGURATION : usbd.h
- USB_REQUEST_GET_DESCRIPTOR : usbd.h
- USB_REQUEST_GET_INTERFACE : usbd.h
- USB_REQUEST_GET_STATUS : usbd.h
- USB_Request_Header_t : StdRequestType.h
- USB_REQUEST_SET_ADDRESS : usbd.h
- USB_REQUEST_SET_CONFIGURATION : usbd.h
- USB_REQUEST_SET_DESCRIPTOR : usbd.h
- USB_REQUEST_SET_FEATURE : usbd.h
- USB_REQUEST_SET_INTERFACE : usbd.h
- USB_REQUEST_SYNC_FRAME : usbd.h
- USB_ResetInterface() : USBController.c , USBController.h
- USB_SetHIDReportItemInfo() : HIDParser.h , HIDParser.c
- USB_SETUP_RCVD : Endpoint_LPC11Uxx.h
- USB_StdDescriptor_Configuration_Header_t : StdDescriptors.h
- USB_StdDescriptor_Device_t : StdDescriptors.h
- USB_StdDescriptor_DeviceQualifier_t : StdDescriptors.h
- USB_StdDescriptor_Endpoint_t : StdDescriptors.h
- USB_StdDescriptor_Header_t : StdDescriptors.h
- USB_StdDescriptor_Interface_Association_t : StdDescriptors.h
- USB_StdDescriptor_Interface_t : StdDescriptors.h
- USB_StdDescriptor_String_t : StdDescriptors.h
- USB_STREAM_TIMEOUT_MS : USBController.h
- USB_STRING_DESCRIPTOR_TYPE : usbd.h
- USB_STRING_LEN : StdDescriptors.h
- USB_StringDescriptor : dfuutil_programming_dfu_ops.c
- USB_USBTask() : USBTask.h
- USB_VBUS_DBOUNCE : Endpoint_LPC11Uxx.h
- USB_VBUS_GetStatus() : USBController.h
- usbBuff : dfuutil_programming_dfu_ops.c
- USBD_API : usbd_rom_api.h
- USBD_EVENT_T : usbd_hw.h
- USBD_HANDLE_T : usbd.h , usbd_api.h
- USBD_HID_HANDLE_T : usbd_api.h
- UsbdAdc_ep0_hdlr() : usbd_adcuser.h
- UsbdAdc_Init() : usbd_adcuser.h
- UsbdAdc_ISO_Hdlr() : usbd_adcuser.h
- UsbdAdc_start_xfr() : usbd_adcuser.h
- UsbdAdc_stop_xfr() : usbd_adcuser.h
- USBDATARAM : ramdisk.c
- UsbdCdc_Init() : usbd_rom_api.h
- UsbdCdc_IO_Buffer_Sync_Task() : usbd_cdcuser.h
- UsbdCdc_RecvData() : usbd_cdcuser.h
- UsbdCdc_SendData() : usbd_cdcuser.h
- usbDebug() : dfuutil_programming_api.h , dfuutil_programming_dfu_ops.c
- usbDebugFill() : dfuutil_programming_dfu_ops.c
- usbDebugSetup() : dfuutil_programming_dfu_ops.c
- USBDEV_ADDR : HAL_LPC18xx.h
- USBDEV_ADDR_AD : HAL_LPC18xx.h
- USBDEV_Init() : dualcore_common.h , usbmsdev.c , MassStorage_ucosiii.c
- usbDFUAppend() : dfuutil_programming_dfu_ops.c
- usbDFUBuildStatus() : dfuutil_programming_dfu_ops.c
- usbDFUEraseAll() : dfuutil_programming_dfu_ops.c
- usbDFUEraseRegion() : dfuutil_programming_dfu_ops.c
- usbDFUExecute() : dfuutil_programming_dfu_ops.c
- usbDFUProgRegion() : dfuutil_programming_dfu_ops.c
- usbDFUReadRegion() : dfuutil_programming_dfu_ops.c
- usbDFUReset() : dfuutil_programming_dfu_ops.c
- usbDFUReturnStatus() : dfuutil_programming_dfu_ops.c
- usbDFUSetVerbose() : dfuutil_programming_dfu_ops.c
- UsbdHid_Init() : usbd_rom_api.h
- UsbdMsc_Init() : usbd_rom_api.h
- UsbdRom_Init() : usbd_rom_api.h
- UsbdRom_IrqHandler() : usbd_rom_api.h
- UsbErrorIsr() : EHCI.h
- UsbHandle : usbd_rom_api.h
- USBHOST_Init() : dualcore_common.h
- USBMODE_DeviceController : EHCI.h
- USBMODE_HostController : EHCI.h
- USBMODE_VBusPowerSelect_High : EHCI.h
- USBMSDEV_STACK_SZ : MassStorage_ucosiii.c
- USBMSDEV_STACK_SZ_FULL : MassStorage_ucosiii.c
- USBMSDEV_STACK_SZ_LIMIT : MassStorage_ucosiii.c
- USBMSGBUFFSIZE : dfuutil_programming_dfu_ops.c
- usbPLLSetup : sysinit_ngx_xplorer_18304330.c
- usbPllSetup() : dfuutil_programming_dfu_ops.c
- usbPLLSetup : sysinit_hitex_eva_18504350.c , sysinit_keil_mcb_18574357.c
- USBPortNum : HAL.h
- USBRAM_BUFFER_SIZE : LPCUSBlibConfig.h
- USBRAM_SECTION : HAL_LPC18xx.h , HAL_LPC11Uxx.h , HAL_LPC17xx.h
- USBROMBUFFSIZE : dfuutil_programming_dfu_ops.c
- USBSpecification : StdDescriptors.h
- usbStrIn : dfuutil_programming_dfu_ops.c
- usbStrOut : dfuutil_programming_dfu_ops.c
- USE_INTERNAL_SERIAL : Device_LPC17xx.h , Device_LPC18xx.h , Device_LPC11Uxx.h
- USE_RMII : sys_config.h
- USE_SPIFI_LIB : dfuutil_programming_spiflash_algorithm.c , flash_config.h
- USE_TEST_TONE : AudioOutputHost.c
- USE_TOUCH : LCDConf.c
- USE_USB0 : app_usbd_cfg.h
- USE_USB_ROM_STACK : LPCUSBlibConfig.h
- USED_PHYSICAL_ENDPOINTS : Endpoint_LPC11Uxx.h
- USHORT : integer.h