| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Modules
Virtual Serial Device
USB examples

## Detailed Description

Example description
This example implements a CDC/ACM (USB-to-COM) virtual serial device. The example reads and writes data through a serial port on the chip which is connected to either 9pin UART connector or a dedicated USB-to-COM chip (FTDI) on the board.

CDC demo need driver for running, follow these steps for install this driver: Right click on "My Computer" and select manage Go to device manager, right click to undefined device and select "Update Driver Software" Select "Browse for driver software on your computer", point to "lpcusblib_VirtualSerial" folder and select "Next" until finish Sometime this driver can be conflicted with Audio driver (Audio Input Device), in this case, follow these steps : Right click on "My Computer" and select manage Go to device manager, uninstall this example's driver(exactly driver in Universal Serial Bus controllers) Unplug and plug this device again, it will work well.

Special connection requirements

- EA1788 and EA4088 Developer's Kits
  - Short jumper JP15 near 20 pin JTAG connector

Build procedures:
LPC17xx/40xx example quickstart for Keil uVision4
LPC17xx/40xx example quickstart for IAR EWARM
LPC17xx/40xx example quickstart for Code Red Xpresso

Supported boards and board setup:
Embedded Artists' LPC1788 Developer's Kit
Embedded Artists' LPC4088 Developer's Kit

Submitting LPCOpen issues:
Community support for LPCOpen

## Modules
| Class descriptors
| Main definitions