| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
board_hitex_eva_18504350.h
Go to the documentation of this file.
1 /*
2 * @brief Hitex EVA 1850/4350 board file
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __BOARD_HITEX_EVA_18504350_H_
33 #define __BOARD_HITEX_EVA_18504350_H_
34
35 #include "chip.h"
36 #include "board_api.h"
37 #include "lpc_phy.h"
38 #include "uda1380.h"
39
40 #ifdef __cplusplus
41 extern "C" {
42 #endif
43
76 #define BOARD_HITEX_EVA_18504350
77
78 /* For USBLIB examples */
79 #define LEDS_LED1 0x01
80 #define LEDS_LED2 0x02
81 #define LEDS_LED3 0x04
82 #define LEDS_LED4 0x08
83 #define LEDS_NO_LEDS 0x00
84 #define BUTTONS_BUTTON1 0x01
85 #define JOY_UP 0x01
86 #define JOY_DOWN 0x02
87 #define JOY_LEFT 0x04
88 #define JOY_RIGHT 0x08
89 #define JOY_PRESS 0x10
90 #define NO_BUTTON_PRESSED 0x00
91
92 #define BUTTONS_BUTTON1_GPIO_PORT_NUM 6
93 #define BUTTONS_BUTTON1_GPIO_BIT_NUM 21
94
95 #define I2CDEV_PCA9502_ADDR (0x9A >> 1)
96 #define PCA9502_REG_IODIR 0x0A
97 #define PCA9502_REG_IOSTATE 0x0B
98 #define PCA9502_REG_IOINTENA 0x0C
99 #define PCA9502_REG_IOCONTROL 0x0E
100 #define PCA9502_REG_ADDR(x) (((x) & 0x0F) << 3)
101
102 /*Define if use SDCARD for Mass Storage Example*/
103 // #define CFG_SDCARD
104
108 #define I2CDEV_UDA1380_ADDR (0x34 >> 1)
109
113 #define UDA1380_I2C_BUS I2C0
114
118 #define FRAMEBUFFER_ADDR 0x28000000
119
123 extern const LCD_Config_T EA320x240;
124
128 #define BOARD_LCD EA320x240
129
135 void Board_UART_Init(LPC_USART_T *pUART);
136
141 void Board_Buttons_Init(void);
142
147 uint32_t Buttons_GetStatus(void);
148
153 void Board_Joystick_Init(void);
154
159 uint8_t Joystick_GetStatus(void);
160
166 void Board_ENET_GetMacADDR(uint8_t *mcaddr);
167
172 void Board_ADC_Init(void);
173
179 void Board_I2C_Init(I2C_ID_T id);
180
190 STATIC INLINE void Board_I2C_EnableFastPlus(I2C_ID_T id)
191 {
192 Chip_SCU_I2C0PinConfig(I2C0_FAST_MODE_PLUS);
193 }
194
201 STATIC INLINE void Board_I2C_DisableFastPlus(I2C_ID_T id)
202 {
203 Chip_SCU_I2C0PinConfig(I2C0_STANDARD_FAST_MODE);
204 }
205
210 void Board_LCD_Init(void);
211
216 void Board_InitLCDController(void);
217
222 void Board_InitTouchController(void);
223
230 bool Board_GetTouchPos(int16_t *pX, int16_t *pY);
231
236 void Board_SetLCDBacklight(uint8_t Intensity);
237
242 void Board_SDMMC_Init(void);
243
249 void Board_SSP_Init(LPC_SSP_T *pSSP);
250
257 void Board_Audio_Init(LPC_I2S_T *pI2S, int micIn);
258
264 void Board_DAC_Init(LPC_DAC_T *pDAC);
265
271 void Serial_CreateStream(void *Stream);
272
277 #ifdef __cplusplus
278 }
279 #endif
280
281 #endif /* __BOARD_HITEX_EVA_18504350_H_ */