| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
uart_8xx.h File Reference

Go to the source code of this file.

## Functions
STATIC INLINE void | Chip_UART_ConfigData (LPC_USART_T *pUART, IP_UART_002_DATALEN_T Databits, IP_UART_002_PARITY_T Parity, IP_UART_002_STOPLEN_T Stopbits)
| Configure the UART protocol.
STATIC INLINE void | Chip_UART_IntEnable (LPC_USART_T *pUART, uint32_t UARTIntCfg, FunctionalState NewState)
| Enable/Disable UART Interrupts.
STATIC INLINE uint32_t | Chip_UART_GetIntStatus (LPC_USART_T *pUART)
| Get UART interrupt status.
void | Chip_UART_Init (LPC_USART_T *pUART)
| Initialize the UART peripheral.
void | Chip_UART_SetBaudRate (LPC_USART_T *pUART, uint32_t baudrate)
| Set baud rate for UART.
Status | Chip_UART_SendByte (LPC_USART_T *pUART, uint8_t data)
| Transmit a 8 bits data.
Status | Chip_UART_ReceiveByte (LPC_USART_T *pUART, uint8_t *Data)
| Receive a 8 bits data.