| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions | Variables
LPC18xx/43xx uC/OS-III blinky example
uCos-III examples

## Detailed Description

Example description
Welcome to the uC/OS-III basic blinky example. This example starts up uC/OS-III and creates 3 tasks. Tasks 1 and 2 blink different LEDs at different rates. Task 3 outputs a tick count to the debug channel (UART) every second.

To use the example, connect a serial cable to the board's RS232/UART port and start a terminal program (115.2K8N1) to monitor the port. The LEDs will also toggle based on the task execution.

Special connection requirements
There are no special connection requirements for this example.

Micrium uC/OS license

Build procedures:
LPC18xx/43xx example quickstart for Keil uVision4
LPC18xx/43xx example quickstart for IAR EWARM
LPC18xx/43xx example quickstart for Code Red Xpresso

Supported boards and board setup:
Hitex 1850 evaluation boards
Hitex 4350 evaluation boards
Keil 1857 evaluation boards
Keil 4357 evaluation boards
NGX 1830 Xplorer boards
NGX 4330 Xplorer boards

Submitting LPCOpen issues:
Community support for LPCOpen

## Functions
void | OS_CSP_TickInit (void)
static void | prvSetupHardware (void)
static void | vLEDTask2 (void *p_arg)
static void | vUARTTask (void *p_arg)
static void | vLEDTask1 (void *p_arg)
int | main (void)
| main routine for uC/OS-III blinky example

## Variables
static OS_TCB | vLEDTask1TCB
static OS_TCB | vLEDTask2TCB
static OS_TCB | vUARTTaskTCB
static CPU_STK | vLEDTask1Stk [APP_CFG_TASK_START_STK_SIZE]
static CPU_STK | vLEDTask2Stk [APP_CFG_TASK_START_STK_SIZE]
static CPU_STK | vUARTTaskStk [APP_CFG_TASK_START_STK_SIZE]

## Function Documentation

int main | ( | void |  | ) |

main routine for uC/OS-III blinky example

Main program body.

Returns
  Function should not exit.

Definition at line 170 of file ucos_iii_blinky.c.

void OS_CSP_TickInit | ( | void |  | ) |

Definition at line 95 of file cpu_bsp.c.

static void prvSetupHardware | ( | void |  | ) |
| static

Definition at line 82 of file ucos_iii_blinky.c.

static void vLEDTask1 | ( | void * | p_arg | ) |
| static

Definition at line 121 of file ucos_iii_blinky.c.

static void vLEDTask2 | ( | void * | p_arg | ) |
| static

Definition at line 91 of file ucos_iii_blinky.c.

static void vUARTTask | ( | void * | p_arg | ) |
| static

Definition at line 106 of file ucos_iii_blinky.c.

## Variable Documentation

CPU_STK vLEDTask1Stk[APP_CFG_TASK_START_STK_SIZE]
| static

Definition at line 76 of file ucos_iii_blinky.c.

OS_TCB vLEDTask1TCB
| static

Definition at line 75 of file ucos_iii_blinky.c.

CPU_STK vLEDTask2Stk[APP_CFG_TASK_START_STK_SIZE]
| static

Definition at line 77 of file ucos_iii_blinky.c.

OS_TCB vLEDTask2TCB
| static

Definition at line 75 of file ucos_iii_blinky.c.

CPU_STK vUARTTaskStk[APP_CFG_TASK_START_STK_SIZE]
| static

Definition at line 78 of file ucos_iii_blinky.c.

OS_TCB vUARTTaskTCB
| static

Definition at line 75 of file ucos_iii_blinky.c.