| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
SCSI_Capacity_t Struct Reference
Mass Storage Class Host Mode Driver

## Detailed Description

SCSI Device LUN Capacity Structure.

SCSI capacity structure, to hold the total capacity of the device in both the number of blocks in the current LUN, and the size of each block. This structure is filled by the device when the MS_Host_ReadDeviceCapacity() function is called.

Definition at line 113 of file MassStorageClassHost.h.

`#include "MassStorageClassHost.h"`

## Data Fields
uint32_t | Blocks
uint32_t | BlockSize

## Field Documentation

uint32_t Blocks

Number of blocks in the addressed LUN of the device.

Definition at line 115 of file MassStorageClassHost.h.

uint32_t BlockSize

Number of bytes in each block in the addressed LUN.

Definition at line 116 of file MassStorageClassHost.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/LPCUSBLib/Drivers/USB/Class/Host/MassStorageClassHost.h