| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
IP_EMC_DYN_DEVICE_CONFIG_T Struct Reference
IP: EMC register block and driver

## Detailed Description

EMC Dynamic Device Configuration structure used for IP drivers.

Definition at line 228 of file emc_001.h.

`#include "emc_001.h"`

## Data Fields
uint32_t | BaseAddr
uint8_t | RAS
uint32_t | ModeRegister
uint32_t | DynConfig

## Field Documentation

uint32_t BaseAddr

Base Address

Definition at line 229 of file emc_001.h.

uint32_t DynConfig

Dynamic Configuration value

Definition at line 232 of file emc_001.h.

uint32_t ModeRegister

Mode Register value

Definition at line 231 of file emc_001.h.

uint8_t RAS

RAS value

Definition at line 230 of file emc_001.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/emc_001.h