| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
ritimer_17xx_40xx.h
Go to the documentation of this file.
1 /*
2 * @brief LPC17xx/40xx RITimer chip driver
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __RITIMER_17XX_40XX_H_
33 #define __RITIMER_17XX_40XX_H_
34
35 #if defined(CHIP_LPC175X_6X)
36
37 #ifdef __cplusplus
38 extern "C" {
39 #endif
40
51 void Chip_RIT_Init(LPC_RITIMER_T *pRITimer);
52
58 void Chip_RIT_DeInit(LPC_RITIMER_T *pRITimer);
59
65 STATIC INLINE void Chip_RIT_Enable(LPC_RITIMER_T *pRITimer)
66 {
67 IP_RIT_Enable(pRITimer);
68 }
69
75 STATIC INLINE void Chip_RIT_Disable(LPC_RITIMER_T *pRITimer)
76 {
77 IP_RIT_Disable(pRITimer);
78 }
79
80
86 STATIC INLINE void Chip_RIT_TimerDebugEnable(LPC_RITIMER_T *pRITimer)
87 {
88 IP_RIT_TimerDebugEnable(pRITimer);
89 }
90
96 STATIC INLINE void Chip_RIT_TimerDebugDisable(LPC_RITIMER_T *pRITimer)
97 {
98 IP_RIT_TimerDebugDisable(pRITimer);
99 }
100
101
107 STATIC INLINE IntStatus Chip_RIT_GetIntStatus(LPC_RITIMER_T *pRITimer)
108 {
109 return IP_RIT_GetIntStatus(pRITimer);
110 }
111
118 STATIC INLINE void Chip_RIT_SetCOMPVAL(LPC_RITIMER_T *pRITimer, uint32_t val)
119 {
120 IP_RIT_SetCOMPVAL(pRITimer, val);
121 }
122
129 STATIC INLINE void Chip_RIT_EnableCTRL(LPC_RITIMER_T *pRITimer, uint32_t val)
130 {
131 IP_RIT_EnableCTRL(pRITimer, val);
132 }
133
139 STATIC INLINE void Chip_RIT_ClearInt(LPC_RITIMER_T *pRITimer)
140 {
141 IP_RIT_EnableCTRL(pRITimer, RIT_CTRL_INT);
142 }
143
149 STATIC INLINE uint32_t Chip_RIT_GetCounter(LPC_RITIMER_T *pRITimer)
150 {
151 return IP_RIT_GetCounter(pRITimer);
152 }
153
160 void Chip_RIT_SetTimerInterval(LPC_RITIMER_T *pRITimer, uint32_t time_interval);
161
166 #ifdef __cplusplus
167 }
168 #endif
169
170 #endif /* defined(CHIP_LPC175X_6X) */
171
172 #endif /* __RITIMER_17XX_40XX_H_ */