| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Modules
Virtual Serial Device and Keyboard Host
USB examples

## Detailed Description

Example description
This example implements a Dual Mode USB device.
check the Virtual Serial Device for Device mode.
check the Keyboard Host for Host mode.

Note
  By default, device run on port 0 and host run on port 1

Special connection requirements
For Keil 1858 and 4357 boards, the host examples requires an external power supply via the PWR power connector.

Build procedures:
LPC18xx/43xx example quickstart for Keil uVision4
LPC18xx/43xx example quickstart for IAR EWARM
LPC18xx/43xx example quickstart for Code Red Xpresso

Supported boards and board setup:
Hitex 1850 evaluation boards
Hitex 4350 evaluation boards
Keil 1857 evaluation boards
Keil 4357 evaluation boards
NGX 1830 Xplorer boards
NGX 4330 Xplorer boards

Submitting LPCOpen issues:
Community support for LPCOpen

## Modules
| Class descriptors
| Functions prototypes
| Main definitions for Keyboard Host
| Main definitions for Virtual Serial