| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
IP_SPI_DELAY_CONFIG_T Struct Reference
IP: SPI register block and driver (002)

## Detailed Description

SPI Delay Configure Struct.

Definition at line 299 of file spi_002.h.

`#include "spi_002.h"`

## Data Fields
uint8_t | PreDelay
uint8_t | PostDelay
uint8_t | FrameDelay
uint8_t | TransferDelay

## Field Documentation

uint8_t FrameDelay

Definition at line 302 of file spi_002.h.

uint8_t PostDelay

Definition at line 301 of file spi_002.h.

uint8_t PreDelay

Definition at line 300 of file spi_002.h.

uint8_t TransferDelay

Definition at line 303 of file spi_002.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/spi_002.h