| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
UsbRom.h File Reference
`#include "..\Keyboard.h"`

Go to the source code of this file.

## Functions
uint32_t | CALLBACK_UsbdRom_Register_DeviceDescriptor (void)
| Call back function registers device descriptor array's address to ROM stack.
uint32_t | CALLBACK_UsbdRom_Register_ConfigurationDescriptor (void)
| Call back function registers device configuration descriptor array's address to ROM stack.
uint32_t | CALLBACK_UsbdRom_Register_StringDescriptor (void)
| Call back function registers string descriptor array's address to ROM stack.
uint32_t | CALLBACK_UsbdRom_Register_DeviceQualifierDescriptor (void)
| Call back function registers device qualifier descriptor array's address to ROM stack.
uint8_t | CALLBACK_UsbdRom_Register_ConfigureEndpoint (void)
| Call back function registers endpoint configuration descriptor array's address to ROM stack.
uint32_t | CALLBACK_UsbdHid_Register_InterfaceDescriptor (void)
| Call back function registers interface descriptor.
uint32_t | CALLBACK_UsbdHid_Register_ReportDescriptor (uint8_t **dest)
| Call back function registers report descriptor.
uint32_t | CALLBACK_UsbdHid_Register_ReportInBuffer (uint8_t **dest)
| Call back function registers report In buffer.
void | CALLBACK_UsbdHid_SetReport (uint8_t **reportoutbuffer, uint32_t reportoutsize)
| Call back function set report.
void | CALLBACK_UsbdHid_SetReportChange (bool newstate)
| Call back function set report change.
bool | CALLBACK_UsbdHid_IsReportChanged (void)
| Determine if report has been changed.