| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
usbd_adcuser.h File Reference
`#include "usbd_adc.h"`

Go to the source code of this file.

## Functions
void | UsbdAdc_Init (USB_ClassInfo_Audio_Device_t *AudioInterface)
| Initialize ROM based audio device class.
void | UsbdAdc_start_xfr (void)
| Start streaming audio data.
void | UsbdAdc_stop_xfr (void)
| Stop streaming audio data.
ErrorCode_t | USB_Interface_Event (USBD_HANDLE_T hUsb)
| Determind start or stop transfer audio data.
ErrorCode_t | UsbdAdc_ISO_Hdlr (USBD_HANDLE_T hUsb, void *data, uint32_t event)
| Handle response to IN isochronous coming packets.
ErrorCode_t | UsbdAdc_ep0_hdlr (USBD_HANDLE_T hUsb, void *data, uint32_t event)
| Handle response to standard requests (chapter9) from host.