| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
eeprom_17xx_40xx.h
Go to the documentation of this file.
1 /*
2 * @brief LPC17xx/40xx EEPROM driver
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef EEPROM_17XX_40XX_H_
33 #define EEPROM_17XX_40XX_H_
34
35 #ifdef __cplusplus
36 extern "C" {
37 #endif
38
44 /* EEPROM read write size type */
45 typedef IP_EEPROM_RWSIZE_T EEPROM_RWSIZE_T;
46
52 void Chip_EEPROM_Init(LPC_EEPROM_T *pEEPROM);
53
59 STATIC INLINE void Chip_EEPROM_DeInit(LPC_EEPROM_T *pEEPROM)
60 {
61 IP_EEPROM_DeInit(pEEPROM);
62 }
63
70 STATIC INLINE void Chip_EEPROM_SetWaitState(LPC_EEPROM_T *pEEPROM, uint32_t ws)
71 {
72 IP_EEPROM_SetWaitState(pEEPROM, ws);
73 }
74
90 STATIC INLINE Status Chip_EEPROM_Write(LPC_EEPROM_T *pEEPROM, uint16_t pageOffset,
91 uint16_t pageAddress,
92 void *pData,
93 EEPROM_RWSIZE_T wsize,
94 uint32_t byteNum)
95 {
96 return IP_EEPROM_Write(pEEPROM, pageOffset, pageAddress, pData, wsize, byteNum);
97 }
98
112 STATIC INLINE void Chip_EEPROM_Read(LPC_EEPROM_T *pEEPROM, uint16_t pageOffset,
113 uint16_t pageAddress,
114 void *pData,
115 EEPROM_RWSIZE_T rsize,
116 uint32_t byteNum)
117 {
118 IP_EEPROM_Read(pEEPROM, pageOffset, pageAddress, pData, rsize, byteNum);
119 }
120
127 STATIC INLINE void Chip_EEPROM_Erase(LPC_EEPROM_T *pEEPROM, uint16_t address)
128 {
129 IP_EEPROM_Erase(pEEPROM, address);
130 }
131
137 STATIC INLINE void Chip_EEPROM_EnablePowerDown(LPC_EEPROM_T *pEEPROM)
138 {
139 IP_EEPROM_EnablePowerDown(pEEPROM);
140 }
141
147 STATIC INLINE void Chip_EEPROM_DisablePowerDown(LPC_EEPROM_T *pEEPROM)
148 {
149 IP_EEPROM_DisablePowerDown(pEEPROM);
150 }
151
158 STATIC INLINE void Chip_EEPROM_EnableInt(LPC_EEPROM_T *pEEPROM, uint32_t mask)
159 {
160 IP_EEPROM_EnableInt(pEEPROM, mask);
161 }
162
169 STATIC INLINE void Chip_EEPROM_DisableInt(LPC_EEPROM_T *pEEPROM, uint32_t mask)
170 {
171 IP_EEPROM_DisableInt(pEEPROM, mask);
172 }
173
179 STATIC INLINE uint32_t Chip_EEPROM_GetIntEnable(LPC_EEPROM_T *pEEPROM)
180 {
181 return IP_EEPROM_GetIntEnable(pEEPROM);
182 }
183
189 STATIC INLINE uint32_t Chip_EEPROM_GetIntStatus(LPC_EEPROM_T *pEEPROM)
190 {
191 return IP_EEPROM_GetIntStatus(pEEPROM);
192 }
193
200 STATIC INLINE void Chip_EEPROM_SetIntStatus(LPC_EEPROM_T *pEEPROM, uint32_t mask)
201 {
202 IP_EEPROM_SetIntStatus(pEEPROM, mask);
203 }
204
211 STATIC INLINE void Chip_EEPROM_ClearIntStatus(LPC_EEPROM_T *pEEPROM, uint32_t mask)
212 {
213 IP_EEPROM_ClearIntStatus(pEEPROM, mask);
214 }
215
220 #ifdef __cplusplus
221 }
222 #endif
223
224 #endif /* EEPROM_17XX_40XX_H_ */