| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages

### - c -

- C_GLCD_H_SIZE : board_keil_mcb_18574357.h
- C_GLCD_V_SIZE : board_keil_mcb_18574357.h
- CAN_BTR_BITMASK : can_001.h
- CAN_BTR_BRP : can_001.h
- CAN_BTR_SAM : can_001.h
- CAN_BTR_SJW : can_001.h
- CAN_BTR_TESG1 : can_001.h
- CAN_BTR_TESG2 : can_001.h
- CAN_CMR_AT : can_001.h
- CAN_CMR_BITMASK : can_001.h
- CAN_CMR_CDO : can_001.h
- CAN_CMR_RRB : can_001.h
- CAN_CMR_SRR : can_001.h
- CAN_CMR_STB : can_001.h
- CAN_CMR_TR : can_001.h
- CAN_CTRL_NO : can.c
- CAN_ERROR_ACK : ccand_11xx.h
- CAN_ERROR_BIT0 : ccand_11xx.h
- CAN_ERROR_BIT1 : ccand_11xx.h
- CAN_ERROR_BOFF : ccand_11xx.h
- CAN_ERROR_CRC : ccand_11xx.h
- CAN_ERROR_FORM : ccand_11xx.h
- CAN_ERROR_NONE : ccand_11xx.h
- CAN_ERROR_PASS : ccand_11xx.h
- CAN_ERROR_STUF : ccand_11xx.h
- CAN_ERROR_WARN : ccand_11xx.h
- CAN_EWL_BITMASK : can_001.h
- CAN_EWL_VAL : can_001.h
- CAN_EXT_ENTRY_CTRL_NO_MASK : can_001.h
- CAN_EXT_ENTRY_CTRL_NO_POS : can_001.h
- CAN_EXT_ENTRY_ID_MASK : can_001.h
- CAN_EXT_ENTRY_ID_POS : can_001.h
- CAN_EXTEND_ID_USAGE : can_001.h
- CAN_GSR_BITMASK : can_001.h
- CAN_GSR_BS : can_001.h
- CAN_GSR_DOS : can_001.h
- CAN_GSR_ES : can_001.h
- CAN_GSR_RBS : can_001.h
- CAN_GSR_RS : can_001.h
- CAN_GSR_RXERR : can_001.h
- CAN_GSR_TBS : can_001.h
- CAN_GSR_TCS : can_001.h
- CAN_GSR_TS : can_001.h
- CAN_GSR_TXERR : can_001.h
- CAN_ICR_ALCBIT_VAL : can_001.h
- CAN_ICR_ALI : can_001.h
- CAN_ICR_BEI : can_001.h
- CAN_ICR_BIT_ERROR : can_001.h
- CAN_ICR_BITMASK : can_001.h
- CAN_ICR_DOI : can_001.h
- CAN_ICR_EI : can_001.h
- CAN_ICR_EPI : can_001.h
- CAN_ICR_ERR_ACK : can_001.h
- CAN_ICR_ERR_ACK_DELIMITER : can_001.h
- CAN_ICR_ERR_CRC_DELIMITER : can_001.h
- CAN_ICR_ERR_CRC_SEQ : can_001.h
- CAN_ICR_ERR_DATA_FIELD : can_001.h
- CAN_ICR_ERR_DLC : can_001.h
- CAN_ICR_ERR_EOF : can_001.h
- CAN_ICR_ERR_ID12_ID5 : can_001.h
- CAN_ICR_ERR_ID17_ID13 : can_001.h
- CAN_ICR_ERR_ID20_ID18 : can_001.h
- CAN_ICR_ERR_ID28_ID21 : can_001.h
- CAN_ICR_ERR_ID4_ID0 : can_001.h
- CAN_ICR_ERR_IDE : can_001.h
- CAN_ICR_ERR_INTERMISSION : can_001.h
- CAN_ICR_ERR_ReservedBit_0 : can_001.h
- CAN_ICR_ERR_ReservedBit_1 : can_001.h
- CAN_ICR_ERR_RTR : can_001.h
- CAN_ICR_ERR_SOF : can_001.h
- CAN_ICR_ERR_SRTR : can_001.h
- CAN_ICR_ERRBIT_VAL : can_001.h
- CAN_ICR_ERRC_VAL : can_001.h
- CAN_ICR_ERRDIR_RECEIVE : can_001.h
- CAN_ICR_FORM_ERROR : can_001.h
- CAN_ICR_IDI : can_001.h
- CAN_ICR_OTHER_ERROR : can_001.h
- CAN_ICR_RI : can_001.h
- CAN_ICR_STUFF_ERROR : can_001.h
- CAN_ICR_TI1 : can_001.h
- CAN_ICR_TI2 : can_001.h
- CAN_ICR_TI3 : can_001.h
- CAN_ICR_WUI : can_001.h
- CAN_IER_ALIE : can_001.h
- CAN_IER_BEIE : can_001.h
- CAN_IER_BITMASK : can_001.h
- CAN_IER_DOIE : can_001.h
- CAN_IER_EIE : can_001.h
- CAN_IER_EPIE : can_001.h
- CAN_IER_IDIE : can_001.h
- CAN_IER_RIE : can_001.h
- CAN_IER_TIE1 : can_001.h
- CAN_IER_TIE2 : can_001.h
- CAN_IER_TIE3 : can_001.h
- CAN_IER_WUIE : can_001.h
- CAN_MOD_BITMASK : can_001.h
- CAN_MOD_LOM : can_001.h
- CAN_MOD_OPERATION : can_001.h
- CAN_MOD_RM : can_001.h
- CAN_MOD_RPM : can_001.h
- CAN_MOD_SM : can_001.h
- CAN_MOD_STM : can_001.h
- CAN_MOD_TM : can_001.h
- CAN_MOD_TPM : can_001.h
- CAN_MSG_MAX_DATA_LEN : can_001.h
- CAN_MSGOBJ_DAT : ccand_11xx.h
- CAN_MSGOBJ_EXT : ccand_11xx.h
- CAN_MSGOBJ_RTR : ccand_11xx.h
- CAN_MSGOBJ_STD : ccand_11xx.h
- CAN_MSR_BITMASK : can_001.h
- CAN_MSR_BS : can_001.h
- CAN_MSR_E : can_001.h
- CAN_REMOTE_MSG : can_001.h
- CAN_RFS_BITMASK : can_001.h
- CAN_RFS_BP : can_001.h
- CAN_RFS_DLC : can_001.h
- CAN_RFS_FF : can_001.h
- CAN_RFS_ID_INDEX : can_001.h
- CAN_RFS_RTR : can_001.h
- CAN_RID_ID_11 : can_001.h
- CAN_RID_ID_29 : can_001.h
- CAN_RSR_BITMASK : can_001.h
- CAN_RSR_DOS : can_001.h
- CAN_RSR_RBS : can_001.h
- CAN_RSR_RS : can_001.h
- CAN_RX_MSG_ID : can.c
- CAN_SDOREQ_HANDLED_NOSEND : ccand_11xx.h
- CAN_SDOREQ_HANDLED_SEND : ccand_11xx.h
- CAN_SDOREQ_NOTHANDLED : ccand_11xx.h
- CAN_SDOSEG_CLOSE : ccand_11xx.h
- CAN_SDOSEG_OPEN : ccand_11xx.h
- CAN_SDOSEG_SEGMENT : ccand_11xx.h
- CAN_SEG1_DEFAULT_VAL : can_17xx_40xx.h
- CAN_SEG2_DEFAULT_VAL : can_17xx_40xx.h
- CAN_SJW_DEFAULT_VAL : can_17xx_40xx.h
- CAN_SR_BITMASK : can_001.h
- CAN_SR_BS : can_001.h
- CAN_SR_DOS : can_001.h
- CAN_SR_ES : can_001.h
- CAN_SR_RBS : can_001.h
- CAN_SR_RS : can_001.h
- CAN_SR_TBS : can_001.h
- CAN_SR_TCS : can_001.h
- CAN_SR_TS : can_001.h
- CAN_STD_ENTRY_CTRL_NO_MASK : can_001.h
- CAN_STD_ENTRY_CTRL_NO_POS : can_001.h
- CAN_STD_ENTRY_DISABLE_MASK : can_001.h
- CAN_STD_ENTRY_DISABLE_POS : can_001.h
- CAN_STD_ENTRY_ID_MASK : can_001.h
- CAN_STD_ENTRY_ID_POS : can_001.h
- CAN_STD_ENTRY_IE_MASK : can_001.h
- CAN_STD_ENTRY_IE_POS : can_001.h
- CAN_TFI_BITMASK : can_001.h
- CAN_TFI_DLC : can_001.h
- CAN_TFI_FF : can_001.h
- CAN_TFI_PRIO : can_001.h
- CAN_TFI_RTR : can_001.h
- CAN_TID_ID11 : can_001.h
- CAN_TID_ID29 : can_001.h
- CAN_TSR_BITMASK : can_001.h
- CAN_TSR_TBS : can_001.h
- CAN_TSR_TCS : can_001.h
- CAN_TSR_TS : can_001.h
- CAN_TX_MSG_EXT_ID : can.c
- CAN_TX_MSG_REMOTE_STD_ID : can.c
- CAN_TX_MSG_STD_ID : can.c
- CANAF_AFMR_ACCBP : can_001.h
- CANAF_AFMR_ACCOFF : can_001.h
- CANAF_AFMR_EFCAN : can_001.h
- CANAF_AFMR_OPERATION : can_001.h
- CANAF_ENDADDR : can_001.h
- CANAF_ENDADDR_VAL : can_001.h
- CANAF_FCAN_IC_INTPND : can_001.h
- CANAF_FCANIE : can_001.h
- CANAF_FCANIE_BITMASK : can_001.h
- CANAF_FULCAN_MSG_AF_FINISHED : can_001.h
- CANAF_FULCAN_MSG_AF_UPDATING : can_001.h
- CANAF_FULCAN_MSG_CPU_READING : can_001.h
- CANAF_FULLCAN_MSG_DLC_BITMASK : can_001.h
- CANAF_FULLCAN_MSG_DLC_POS : can_001.h
- CANAF_FULLCAN_MSG_FF_POS : can_001.h
- CANAF_FULLCAN_MSG_ID11_BITMASK : can_001.h
- CANAF_FULLCAN_MSG_ID11_POS : can_001.h
- CANAF_FULLCAN_MSG_LOST_POS : can_001.h
- CANAF_FULLCAN_MSG_RTR_POS : can_001.h
- CANAF_FULLCAN_MSG_SCC_BITMASK : can_001.h
- CANAF_FULLCAN_MSG_SCC_POS : can_001.h
- CANAF_FULLCAN_MSG_SEM_BITMASK : can_001.h
- CANAF_FULLCAN_MSG_SEM_POS : can_001.h
- CANAF_LUTERR : can_001.h
- CANAF_LUTERRAD : can_001.h
- CANAF_RAM_ENTRY_NUM : can_001.h
- CARD_TYPE_4BIT : lpc_sdmmc.h
- CARD_TYPE_8BIT : lpc_sdmmc.h
- CARD_TYPE_HC : lpc_sdmmc.h
- CARD_TYPE_SD : lpc_sdmmc.h
- CCAN_ARB : ccan_001.h
- CCAN_CLRINTPND : ccan_001.h
- CCAN_CTRL : ccan_001.h
- CCAN_CTRL_CCE : ccan_001.h
- CCAN_CTRL_DAR : ccan_001.h
- CCAN_CTRL_EIE : ccan_001.h
- CCAN_CTRL_IE : ccan_001.h
- CCAN_CTRL_INIT : ccan_001.h
- CCAN_CTRL_SIE : ccan_001.h
- CCAN_CTRL_TEST : ccan_001.h
- CCAN_DATAA : ccan_001.h
- CCAN_DATAB : ccan_001.h
- CCAN_DLC : ccan_001.h
- CCAN_DLC_MASK : ccan_001.h
- CCAN_EOB : ccan_001.h
- CCAN_ID_DIR : ccan_001.h
- CCAN_ID_EXT_MASK : ccan_001.h
- CCAN_ID_MTD : ccan_001.h
- CCAN_ID_MVAL : ccan_001.h
- CCAN_ID_STD_MASK : ccan_001.h
- CCAN_IF_Read : ccan_001.h
- CCAN_IF_Write : ccan_001.h
- CCAN_IFCREQ_BUSY : ccan_001.h
- CCAN_INTP : ccan_001.h
- CCAN_MASK : ccan_001.h
- CCAN_MASK_MDIR : ccan_001.h
- CCAN_MASK_MXTD : ccan_001.h
- CCAN_MLST : ccan_001.h
- CCAN_NEWD : ccan_001.h
- CCAN_NEWDAT : ccan_001.h
- CCAN_RD : ccan_001.h
- CCAN_RMTEN : ccan_001.h
- CCAN_RW : ccan_001.h
- CCAN_RX_DIR : ccan_001.h
- CCAN_RX_MSG_ID : ccan.c
- CCAN_RXIE : ccan_001.h
- CCAN_SEG1_DEFAULT_VAL : ccan_18xx_43xx.h
- CCAN_SEG2_DEFAULT_VAL : ccan_18xx_43xx.h
- CCAN_SJW_DEFAULT_VAL : ccan_18xx_43xx.h
- CCAN_STATUS_INT : ccan_001.h
- CCAN_TX_DIR : ccan_001.h
- CCAN_TX_MSG_ID : ccan.c
- CCAN_TX_MSG_REMOTE_ID : ccan.c
- CCAN_TXIE : ccan_001.h
- CCAN_TXRQ : ccan_001.h
- CCAN_UMSK : ccan_001.h
- CCAN_WR : ccan_001.h
- CCEMTY_INT : HAL_LPC17xx.h
- CDC_ABSTRACT_CONTROL_MANAGEMENT : usbd_cdc.h
- CDC_ABSTRACT_CONTROL_MODEL : usbd_cdc.h
- CDC_ABSTRACT_STATE : usbd_cdc.h
- CDC_ACTIVATE_CARRIER : usbd_cdc.h
- CDC_ATM_NETWORKING : usbd_cdc.h
- CDC_ATM_NETWORKING_CONTROL_MODEL : usbd_cdc.h
- CDC_AUX_JACK_HOOK_STATE : usbd_cdc.h
- CDC_BRIDGE_TASK : VirtualSerial.c , VirtualSerial.h
- CDC_BUF_MASK : usbd_cdcuser.h
- CDC_BUF_SIZE : usbd_cdcuser.h
- CDC_CALL_MANAGEMENT : usbd_cdc.h
- CDC_CALL_STATE_CHANGE : usbd_cdc.h
- CDC_CAPI_CONTROL_MANAGEMENT : usbd_cdc.h
- CDC_CAPI_CONTROL_MODEL : usbd_cdc.h
- CDC_CLEAR_COMM_FEATURE : usbd_cdc.h
- CDC_CLEAR_UNIT_PARAMETER : usbd_cdc.h
- CDC_COMMUNICATION_INTERFACE_CLASS : usbd_cdc.h
- CDC_CONNECTION_SPEED_CHANGE : usbd_cdc.h
- CDC_CONTROL_LINE_IN_BREAK : CDCClassCommon.h
- CDC_CONTROL_LINE_IN_DCD : CDCClassCommon.h
- CDC_CONTROL_LINE_IN_DSR : CDCClassCommon.h
- CDC_CONTROL_LINE_IN_FRAMEERROR : CDCClassCommon.h
- CDC_CONTROL_LINE_IN_OVERRUNERROR : CDCClassCommon.h
- CDC_CONTROL_LINE_IN_PARITYERROR : CDCClassCommon.h
- CDC_CONTROL_LINE_IN_RING : CDCClassCommon.h
- CDC_CONTROL_LINE_OUT_DTR : CDCClassCommon.h
- CDC_CONTROL_LINE_OUT_RTS : CDCClassCommon.h
- CDC_COUNTRY_SELECTION : usbd_cdc.h
- CDC_COUNTRY_SETTING : usbd_cdc.h
- CDC_CS_ENDPOINT : usbd_cdc.h
- CDC_CS_INTERFACE : usbd_cdc.h
- CDC_DATA_INTERFACE_CLASS : usbd_cdc.h
- CDC_DATA_MULTPLEXED_STATE : usbd_cdc.h
- CDC_DIAL_DIGITS : usbd_cdc.h
- CDC_DIRECT_LINE_CONTROL_MODEL : usbd_cdc.h
- CDC_DIRECT_LINE_MANAGEMENT : usbd_cdc.h
- CDC_DTE_PRESENT : usbd_cdc.h
- CDC_ETHERNET_NETWORKING : usbd_cdc.h
- CDC_ETHERNET_NETWORKING_CONTROL_MODEL : usbd_cdc.h
- CDC_EXTENSION_UNIT : usbd_cdc.h
- CDC_FUNCTIONAL_DESCRIPTOR : CDCClassCommon.h
- CDC_GET_ATM_DEVICE_STATISTICS : usbd_cdc.h
- CDC_GET_ATM_VC_STATISTICS : usbd_cdc.h
- CDC_GET_COMM_FEATURE : usbd_cdc.h
- CDC_GET_ENCAPSULATED_RESPONSE : usbd_cdc.h
- CDC_GET_ETHERNET_PMP_FILTER : usbd_cdc.h
- CDC_GET_ETHERNET_STATISTIC : usbd_cdc.h
- CDC_GET_LINE_CODING : usbd_cdc.h
- CDC_GET_LINE_PARMS : usbd_cdc.h
- CDC_GET_OPERATION_PARMS : usbd_cdc.h
- CDC_GET_PROFILE : usbd_cdc.h
- CDC_GET_RINGER_PARMS : usbd_cdc.h
- CDC_GET_UNIT_PARAMETER : usbd_cdc.h
- CDC_HEADER : usbd_cdc.h
- CDC_IDLE_SETTING : usbd_cdc.h
- CDC_LINE_STATE_CHANGE : usbd_cdc.h
- CDC_MULTI_CHANNEL_CONTROL_MODEL : usbd_cdc.h
- CDC_MULTI_CHANNEL_MANAGEMENT : usbd_cdc.h
- CDC_NETWORK_CHANNEL : usbd_cdc.h
- CDC_NOTIFICATION_EPNUM : Descriptors.h
- CDC_NOTIFICATION_EPSIZE : Descriptors.h
- CDC_NOTIFICATION_NETWORK_CONNECTION : usbd_cdc.h
- CDC_NOTIFICATION_SERIAL_STATE : usbd_cdc.h
- CDC_PROTOCOL_CAPI : usbd_cdc.h
- CDC_PROTOCOL_COMMON_AT_COMMANDS : usbd_cdc.h
- CDC_PROTOCOL_DESCRIBED_IN_PUFD : usbd_cdc.h
- CDC_PROTOCOL_EURO_ISDN : usbd_cdc.h
- CDC_PROTOCOL_HDLC : usbd_cdc.h
- CDC_PROTOCOL_HOST_BASED_DRIVER : usbd_cdc.h
- CDC_PROTOCOL_ISDN_BRI : usbd_cdc.h
- CDC_PROTOCOL_Q921_DATA_LINK : usbd_cdc.h
- CDC_PROTOCOL_Q921_MANAGEMENT : usbd_cdc.h
- CDC_PROTOCOL_Q921_MULTIPLEXOR : usbd_cdc.h
- CDC_PROTOCOL_TRANSPARENT : usbd_cdc.h
- CDC_PROTOCOL_UNIT : usbd_cdc.h
- CDC_PROTOCOL_V24_RATE_ADAPTATION : usbd_cdc.h
- CDC_PROTOCOL_V42 : usbd_cdc.h
- CDC_PULSE_SETUP : usbd_cdc.h
- CDC_REPORTING_CAPABILITIES : usbd_cdc.h
- CDC_RESPONSE_AVAILABLE : usbd_cdc.h
- CDC_RING_AUX_JACK : usbd_cdc.h
- CDC_RING_DETECT : usbd_cdc.h
- CDC_RX_EPNUM : Descriptors.h
- CDC_SEND_BREAK : usbd_cdc.h
- CDC_SEND_ENCAPSULATED_COMMAND : usbd_cdc.h
- CDC_SEND_PULSE : usbd_cdc.h
- CDC_SERIAL_STATE_BREAK : usbd_cdc.h
- CDC_SERIAL_STATE_FRAMING : usbd_cdc.h
- CDC_SERIAL_STATE_OVERRUN : usbd_cdc.h
- CDC_SERIAL_STATE_PARITY : usbd_cdc.h
- CDC_SERIAL_STATE_RING : usbd_cdc.h
- CDC_SERIAL_STATE_RX_CARRIER : usbd_cdc.h
- CDC_SERIAL_STATE_TX_CARRIER : usbd_cdc.h
- CDC_SET_ATM_DATA_FORMAT : usbd_cdc.h
- CDC_SET_ATM_DEFAULT_VC : usbd_cdc.h
- CDC_SET_AUX_LINE_STATE : usbd_cdc.h
- CDC_SET_COMM_FEATURE : usbd_cdc.h
- CDC_SET_CONTROL_LINE_STATE : usbd_cdc.h
- CDC_SET_ETHERNET_MULTICAST_FILTERS : usbd_cdc.h
- CDC_SET_ETHERNET_PACKET_FILTER : usbd_cdc.h
- CDC_SET_ETHERNET_PMP_FILTER : usbd_cdc.h
- CDC_SET_HOOK_STATE : usbd_cdc.h
- CDC_SET_LINE_CODING : usbd_cdc.h
- CDC_SET_LINE_PARMS : usbd_cdc.h
- CDC_SET_OPERATION_PARMS : usbd_cdc.h
- CDC_SET_PULSE_TIME : usbd_cdc.h
- CDC_SET_RINGER_PARMS : usbd_cdc.h
- CDC_SET_UNIT_PARAMETER : usbd_cdc.h
- CDC_TASK_SELECT : VirtualSerial.c
- CDC_TELEPHONE_CONTROL_MODEL : usbd_cdc.h
- CDC_TELEPHONE_OPERATIONAL_MODES : usbd_cdc.h
- CDC_TELEPHONE_RINGER : usbd_cdc.h
- CDC_TX_EPNUM : Descriptors.h
- CDC_TXRX_EPSIZE : Descriptors.h
- CDC_UNION : usbd_cdc.h
- CDC_USB_TERMINAL : usbd_cdc.h
- CDC_V1_10 : usbd_cdc.h
- CDFULL_INT : HAL_LPC17xx.h
- CENAF : pinint_8xx.h
- CENRL : pinint_8xx.h
- CGU_AUDIO_PLL_RATE : sys_config.h
- CGU_IRC_FREQ : clock_18xx_43xx.h
- CGU_PLL_FR : clock_18xx_43xx.h
- CGU_PLL_LOCKED : clock_18xx_43xx.h
- CGU_USB_PLL_RATE : sys_config.h
- CHECKSUM_CHECK_IP : lwipopts.h
- CHECKSUM_CHECK_TCP : lwipopts.h
- CHECKSUM_CHECK_UDP : lwipopts.h
- CHECKSUM_GEN_IP : lwipopts.h
- CHECKSUM_GEN_TCP : lwipopts.h
- CHECKSUM_GEN_UDP : lwipopts.h
- CHIP_CCAN_DETERMINECLK : ccan_18xx_43xx.c
- CHIP_LPC11CXX : sys_config.h
- CHIP_LPC11UXX : sys_config.h
- CHIP_LPC1347 : sys_config.h
- CHIP_LPC175X_6X : sys_config.h
- CHIP_LPC177X_8X : sys_config.h
- CHIP_LPC18XX : sys_config.h
- CHIP_LPC407X_8X : sys_config.h
- CHIP_LPC43XX : sys_config.h
- CHIP_LPC8XX : sys_config.h
- CHIP_SPI_BITS_T : spi_17xx_40xx.h
- CHIP_SPI_CLOCK_MODE_T : spi_17xx_40xx.h
- CHIP_SPI_DATA_ORDER_T : spi_17xx_40xx.h
- CHIP_SPI_MODE_T : spi_17xx_40xx.h
- CHKTAG : eeprom.c , nandflash.c , norflash.c , eeprom.c
- CHKTAG_SIZE : eeprom.c , nandflash.c , norflash.c , eeprom.c
- CLCDC_LCDCTRL_ENABLE : lcd_001.h
- CLCDC_LCDCTRL_PWR : lcd_001.h
- CLK0_DELAY : sysinit_ea_devkit_17884088.c , sysinit_hitex_eva_18504350.c , sysinit_keil_mcb_18574357.c
- CLR_BUF_PO : HAL_LPC17xx.h
- CMD : sdmmc_18xx_43xx.h
- CMD13_RCA : lpc_sdmmc.h
- CMD3_RCA : lpc_sdmmc.h
- CMD55_RCA : lpc_sdmmc.h
- CMD7_RCA : lpc_sdmmc.h
- CMD8_CHECKPATTERN : lpc_sdmmc.h
- CMD8_DEF_PATTERN : lpc_sdmmc.h
- CMD8_VOLTAGESUPPLIED_27_36 : lpc_sdmmc.h
- CMD9_RCA : lpc_sdmmc.h
- CMD_ALL_SEND_CID : sdmmc_18xx_43xx.h
- CMD_BIT_APP : sdmmc_18xx_43xx.h
- CMD_BIT_AUTO_STOP : sdmmc_18xx_43xx.h
- CMD_BIT_BUSY : sdmmc_18xx_43xx.h
- CMD_BIT_DATA : sdmmc_18xx_43xx.h
- CMD_BIT_INIT : sdmmc_18xx_43xx.h
- CMD_BIT_LS : sdmmc_18xx_43xx.h
- CMD_BIT_STREAM : sdmmc_18xx_43xx.h
- CMD_BIT_WRITE : sdmmc_18xx_43xx.h
- CMD_CFG_DEV : HAL_LPC17xx.h
- CMD_CLR_BUF : HAL_LPC17xx.h
- CMD_DESELECT_CARD : sdmmc_18xx_43xx.h
- CMD_GET_DEV_STAT : HAL_LPC17xx.h
- CMD_GET_ERR_CODE : HAL_LPC17xx.h
- CMD_IDLE : sdmmc_18xx_43xx.h
- CMD_MASK_CMD : sdmmc_18xx_43xx.h
- CMD_MASK_RESP : sdmmc_18xx_43xx.h
- CMD_MMC_OP_COND : sdmmc_18xx_43xx.h
- CMD_MMC_SET_RCA : sdmmc_18xx_43xx.h
- CMD_RD_ERR_STAT : HAL_LPC17xx.h
- CMD_RD_FRAME : HAL_LPC17xx.h
- CMD_RD_TEST : HAL_LPC17xx.h
- CMD_READ_MULTIPLE : sdmmc_18xx_43xx.h
- CMD_READ_SINGLE : sdmmc_18xx_43xx.h
- CMD_RESP : sdmmc_18xx_43xx.h
- CMD_RESP_R0 : sdmmc_18xx_43xx.h
- CMD_RESP_R1 : sdmmc_18xx_43xx.h
- CMD_RESP_R2 : sdmmc_18xx_43xx.h
- CMD_RESP_R3 : sdmmc_18xx_43xx.h
- CMD_SD_OP_COND : sdmmc_18xx_43xx.h
- CMD_SD_SEND_IF_COND : sdmmc_18xx_43xx.h
- CMD_SD_SEND_RCA : sdmmc_18xx_43xx.h
- CMD_SD_SET_WIDTH : sdmmc_18xx_43xx.h
- CMD_SEL_EP : HAL_LPC17xx.h
- CMD_SEL_EP_CLRI : HAL_LPC17xx.h
- CMD_SELECT_CARD : sdmmc_18xx_43xx.h
- CMD_SEND_CSD : sdmmc_18xx_43xx.h
- CMD_SEND_EXT_CSD : sdmmc_18xx_43xx.h
- CMD_SEND_STATUS : sdmmc_18xx_43xx.h
- CMD_SET_ADDR : HAL_LPC17xx.h
- CMD_SET_BLOCKLEN : sdmmc_18xx_43xx.h
- CMD_SET_DEV_STAT : HAL_LPC17xx.h
- CMD_SET_EP_STAT : HAL_LPC17xx.h
- CMD_SET_MODE : HAL_LPC17xx.h
- CMD_SHIFT_CMD : sdmmc_18xx_43xx.h
- CMD_STOP : sdmmc_18xx_43xx.h
- CMD_TIMEOUT : sdmmc_17xx_40xx.c
- CMD_VALID_BUF : HAL_LPC17xx.h
- CMD_WRITE_MULTIPLE : sdmmc_18xx_43xx.h
- CMD_WRITE_SINGLE : sdmmc_18xx_43xx.h
- CMDRESP_NONE_TYPE : sdmmc_17xx_40xx.h
- CMDRESP_R1_TYPE : sdmmc_17xx_40xx.h
- CMDRESP_R1b_TYPE : sdmmc_17xx_40xx.h
- CMDRESP_R2_TYPE : sdmmc_17xx_40xx.h
- CMDRESP_R3_HC_CCS : lpc_sdmmc.h
- CMDRESP_R3_INIT_COMPLETE : lpc_sdmmc.h
- CMDRESP_R3_OCR_VAL : lpc_sdmmc.h
- CMDRESP_R3_S18A : lpc_sdmmc.h
- CMDRESP_R3_TYPE : sdmmc_17xx_40xx.h
- CMDRESP_R6_CARD_STATUS : lpc_sdmmc.h
- CMDRESP_R6_RCA_VAL : lpc_sdmmc.h
- CMDRESP_R6_TYPE : sdmmc_17xx_40xx.h
- CMDRESP_R7_CHECK_PATTERN : lpc_sdmmc.h
- CMDRESP_R7_TYPE : sdmmc_17xx_40xx.h
- CMDRESP_R7_VOLTAGE_ACCEPTED : lpc_sdmmc.h
- CMP_CTRL_BITMASK : cmp_001.h
- CMP_CTRL_EXT_RESET_CMPRESET : cmp_001.h
- CMP_CTRL_EXT_RESET_INTERNAL : cmp_001.h
- CMP_CTRL_PD_IREF : cmp_001.h
- CMP_CTRL_PD_IREF_BITMASK : cmp_001.h
- CMP_CTRL_PD_VBG : cmp_001.h
- CMP_CTRL_PD_VBG_BITMASK : cmp_001.h
- CMP_CTRL_ROSC_BITMASK : cmp_001.h
- CMP_CTRL_ROSCCTL_CMP0 : cmp_001.h
- CMP_CTRL_ROSCCTL_CMP1 : cmp_001.h
- CMP_CTRL_T0CAP2_0LEVEL : cmp_001.h
- CMP_CTRL_T0CAP2_1LEVEL : cmp_001.h
- CMP_CTRL_T0CAP3_0EDGE : cmp_001.h
- CMP_CTRL_T0CAP3_1EDGE : cmp_001.h
- CMP_CTRL_T1CAP2_0LEVEL : cmp_001.h
- CMP_CTRL_T1CAP2_1EDGE : cmp_001.h
- CMP_CTRL_T1CAP3_0EDGE : cmp_001.h
- CMP_CTRL_T1CAP3_1LEVEL : cmp_001.h
- CMP_CTRL_TIMERCAPTURE_BITMASK : cmp_001.h
- CMP_CTRLx_BITMASK : cmp_001.h
- CMP_CTRLx_EN : cmp_001.h
- CMP_CTRLx_EN_BITMASK : cmp_001.h
- CMP_CTRLx_HYS : cmp_001.h
- CMP_CTRLx_HYS_BITMASK : cmp_001.h
- CMP_CTRLx_INTCTRL_BITMASK : cmp_001.h
- CMP_CTRLx_INTEDGE : cmp_001.h
- CMP_CTRLx_INTEDGE_BITMASK : cmp_001.h
- CMP_CTRLx_INTFLAG : cmp_001.h
- CMP_CTRLx_INTPOL_INV : cmp_001.h
- CMP_CTRLx_INTPOL_NORMAL : cmp_001.h
- CMP_CTRLx_INTTYPE_EDGE : cmp_001.h
- CMP_CTRLx_INTTYPE_LEVEL : cmp_001.h
- CMP_CTRLx_OE : cmp_001.h
- CMP_CTRLx_STAT : cmp_001.h
- CMP_CTRLx_SYNC : cmp_001.h
- CMP_CTRLx_VLADEN : cmp_001.h
- CMP_CTRLx_VLADEN_BITMASK : cmp_001.h
- CMP_CTRLx_VLADREF_VDDA : cmp_001.h
- CMP_CTRLx_VLADREF_VREFCMP : cmp_001.h
- CMP_CTRLx_VM : cmp_001.h
- CMP_CTRLx_VM_BITMASK : cmp_001.h
- CMP_CTRLx_VP : cmp_001.h
- CMP_CTRLx_VP_BITMASK : cmp_001.h
- CMP_CTRLx_VSEL : cmp_001.h
- CMP_CTRLx_VSEL_BITMASK : cmp_001.h
- CMP_ID : cmp.c
- CMP_NUM : cmp_001.h
- COLOR_CONVERSION : LCDConf.c
- COLORS_8_565_MODE : lpc_colors.h
- COLORS_DEF : lpc_colors.h
- COLUMN_ADDR : lpc_nandflash_k9f1g.c
- COMPILE_TIME_ASSERT : error.h
- CONF_DVICE : HAL_LPC17xx.h
- CONFIG_CPU_CLOCK_HZ : cpu_bsp_lpc43xx_m0.c
- CONFIG_SCT_nEV : sct_001.h
- CONFIG_SCT_nOU : sct_001.h
- CONFIG_SCT_nRG : sct_001.h
- configASSERT : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configCHECK_FOR_STACK_OVERFLOW : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configCPU_CLOCK_HZ : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configGENERATE_RUN_TIME_STATS : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configIDLE_SHOULD_YIELD : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configKERNEL_INTERRUPT_PRIORITY : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configLIBRARY_LOWEST_INTERRUPT_PRIORITY : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configLIBRARY_MAX_SYSCALL_INTERRUPT_PRIORITY : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configMAX_CO_ROUTINE_PRIORITIES : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configMAX_PRIORITIES : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configMAX_SYSCALL_INTERRUPT_PRIORITY : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configMAX_TASK_NAME_LEN : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configMINIMAL_STACK_SIZE : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configPRIO_BITS : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configQUEUE_REGISTRY_SIZE : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h
- configTICK_RATE_HZ : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configTIMER_QUEUE_LENGTH : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configTIMER_TASK_PRIORITY : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configTIMER_TASK_STACK_DEPTH : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configTOTAL_HEAP_SIZE : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_16_BIT_TICKS : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_ALTERNATIVE_API : FreeRTOSConfig.h
- configUSE_APPLICATION_TASK_TAG : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_CO_ROUTINES : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_COUNTING_SEMAPHORES : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_CUSTOM_TICK : lpc43xx_m0_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_IDLE_HOOK : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_MALLOC_FAILED_HOOK : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_MUTEXES : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_PREEMPTION : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_RECURSIVE_MUTEXES : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_TICK_HOOK : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_TICKLESS_IDLE : FreeRTOSConfig.h
- configUSE_TIMERS : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- configUSE_TRACE_FACILITY : lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , lpc43xx_m0_FreeRTOSConfig.h , lpc43xx_m4_FreeRTOSConfig.h , FreeRTOSConfig.h
- ContiguousBufferLength : RNDISClassHost.c
- CONTROL_BULK_SERVICE_RATIO : OHCI.h
- CONTROL_LIST_HEAD : OHCI.h
- CONTROL_REQTYPE_DIRECTION : StdRequestType.h
- CONTROL_REQTYPE_RECIPIENT : StdRequestType.h
- CONTROL_REQTYPE_TYPE : StdRequestType.h
- COORD_GET_NUM : board_ea_devkit_17884088.c , board_hitex_eva_18504350.c
- COUNTUP_TO : sct_001.h
- COUNTUP_TO_LIMIT_THEN_CLEAR_TO_ZERO : sct_001.h
- CPU_BIT_BAND_PERIPH_BASE : cpu_c_m0.c , cpu_c.c
- CPU_BIT_BAND_PERIPH_REG_HI : cpu_c_m0.c , cpu_c.c
- CPU_BIT_BAND_PERIPH_REG_LO : cpu_c_m0.c , cpu_c.c
- CPU_BIT_BAND_SRAM_BASE : cpu_c_m0.c , cpu_c.c
- CPU_BIT_BAND_SRAM_REG_HI : cpu_c_m0.c , cpu_c.c
- CPU_BIT_BAND_SRAM_REG_LO : cpu_c_m0.c , cpu_c.c
- CPU_BSP_MODULE : cpu_bsp.c
- CPU_CFG_ADDR_SIZE : cpu.h
- CPU_CFG_CRITICAL_METHOD : cpu.h
- CPU_CFG_DATA_SIZE : cpu.h
- CPU_CFG_ENDIAN_TYPE : cpu.h
- CPU_CFG_INT_DIS_MEAS_EN : cpu_cfg.h
- CPU_CFG_INT_DIS_MEAS_OVRHD_NBR : cpu_cfg.h
- CPU_CFG_LEAD_ZEROS_ASM_PRESENT : cpu.h , cpu_cfg.h , cpu.h
- CPU_CFG_NAME_EN : cpu_cfg.h
- CPU_CFG_NAME_SIZE : cpu_cfg.h
- CPU_CFG_STK_GROWTH : cpu.h
- CPU_CFG_TS_32_EN : cpu_cfg.h
- CPU_CFG_TS_64_EN : cpu_cfg.h
- CPU_CFG_TS_EN : cpu_core.h
- CPU_CFG_TS_TMR_EN : cpu_core.h
- CPU_CFG_TS_TMR_SIZE : cpu_cfg.h
- CPU_CORE_EXT : cpu_core.h
- CPU_CORE_MODULE : cpu_core.c
- CPU_CORE_VERSION : cpu_core.h
- CPU_CRITICAL_ENTER : cpu.h
- CPU_CRITICAL_EXIT : cpu.h
- CPU_CRITICAL_METHOD_INT_DIS_EN : cpu_def.h
- CPU_CRITICAL_METHOD_NONE : cpu_def.h
- CPU_CRITICAL_METHOD_STATUS_LOCAL : cpu_def.h
- CPU_CRITICAL_METHOD_STATUS_STK : cpu_def.h
- CPU_ENDIAN_TYPE_BIG : cpu_def.h
- CPU_ENDIAN_TYPE_LITTLE : cpu_def.h
- CPU_ENDIAN_TYPE_NONE : cpu_def.h
- CPU_ERR_NAME_SIZE : cpu_core.h
- CPU_ERR_NONE : cpu_core.h
- CPU_ERR_NULL_PTR : cpu_core.h
- CPU_ERR_TS_FREQ_INVALID : cpu_core.h
- CPU_INT_BUSFAULT : cpu.h
- CPU_INT_DBGMON : cpu.h
- CPU_INT_DIS : cpu.h
- CPU_INT_EN : cpu.h
- CPU_INT_EXT0 : cpu.h
- CPU_INT_HFAULT : cpu.h
- CPU_INT_MEM : cpu.h
- CPU_INT_NMI : cpu.h
- CPU_INT_PENDSV : cpu.h
- CPU_INT_RESET : cpu.h
- CPU_INT_RSVD_07 : cpu.h
- CPU_INT_RSVD_08 : cpu.h
- CPU_INT_RSVD_09 : cpu.h
- CPU_INT_RSVD_10 : cpu.h
- CPU_INT_RSVD_13 : cpu.h
- CPU_INT_SRC_POS_MAX : cpu_c.c , cpu_c_m0.c , cpu_c.c
- CPU_INT_STK_PTR : cpu.h
- CPU_INT_SVCALL : cpu.h
- CPU_INT_SYSTICK : cpu.h
- CPU_INT_USAGEFAULT : cpu.h
- CPU_MSK_NVIC_ICSR_VECT_ACTIVE : cpu.h
- CPU_REG_DBG_CTRL : cpu.h
- CPU_REG_DBG_DATA : cpu.h
- CPU_REG_DBG_INT : cpu.h
- CPU_REG_DBG_SELECT : cpu.h
- CPU_REG_MPU_CTRL : cpu.h
- CPU_REG_MPU_REG_ATTR : cpu.h
- CPU_REG_MPU_REG_BASE : cpu.h
- CPU_REG_MPU_REG_NBR : cpu.h
- CPU_REG_MPU_TYPE : cpu.h
- CPU_REG_NVIC_ACTIVE : cpu.h
- CPU_REG_NVIC_AFR0 : cpu.h
- CPU_REG_NVIC_AFSR : cpu.h
- CPU_REG_NVIC_AIRCR : cpu.h
- CPU_REG_NVIC_AIRCR_ENDIANNESS : cpu.h
- CPU_REG_NVIC_AIRCR_SYSRESETREQ : cpu.h
- CPU_REG_NVIC_AIRCR_VECTCLRACTIVE : cpu.h
- CPU_REG_NVIC_AIRCR_VECTRESET : cpu.h
- CPU_REG_NVIC_BFAR : cpu.h
- CPU_REG_NVIC_CCR : cpu.h
- CPU_REG_NVIC_CCR_BFHFNMIGN : cpu.h
- CPU_REG_NVIC_CCR_DIV_0_TRP : cpu.h
- CPU_REG_NVIC_CCR_NONBASETHRDENA : cpu.h
- CPU_REG_NVIC_CCR_STKALIGN : cpu.h
- CPU_REG_NVIC_CCR_UNALIGN_TRP : cpu.h
- CPU_REG_NVIC_CCR_USERSETMPEND : cpu.h
- CPU_REG_NVIC_CFSR : cpu.h
- CPU_REG_NVIC_CFSR_BFARVALID : cpu.h
- CPU_REG_NVIC_CFSR_DACCVIOL : cpu.h
- CPU_REG_NVIC_CFSR_DIVBYZERO : cpu.h
- CPU_REG_NVIC_CFSR_IACCVIOL : cpu.h
- CPU_REG_NVIC_CFSR_IBUSERR : cpu.h
- CPU_REG_NVIC_CFSR_IMPRECISERR : cpu.h
- CPU_REG_NVIC_CFSR_INVPC : cpu.h
- CPU_REG_NVIC_CFSR_INVSTATE : cpu.h
- CPU_REG_NVIC_CFSR_MMARVALID : cpu.h
- CPU_REG_NVIC_CFSR_MSTKERR : cpu.h
- CPU_REG_NVIC_CFSR_MUNSTKERR : cpu.h
- CPU_REG_NVIC_CFSR_NOCP : cpu.h
- CPU_REG_NVIC_CFSR_PRECISERR : cpu.h
- CPU_REG_NVIC_CFSR_STKERR : cpu.h
- CPU_REG_NVIC_CFSR_UNALIGNED : cpu.h
- CPU_REG_NVIC_CFSR_UNDEFINSTR : cpu.h
- CPU_REG_NVIC_CFSR_UNSTKERR : cpu.h
- CPU_REG_NVIC_CLREN : cpu.h
- CPU_REG_NVIC_CLRPEND : cpu.h
- CPU_REG_NVIC_CPUID : cpu.h
- CPU_REG_NVIC_DFR0 : cpu.h
- CPU_REG_NVIC_DFSR : cpu.h
- CPU_REG_NVIC_DFSR_BKPT : cpu.h
- CPU_REG_NVIC_DFSR_DWTTRAP : cpu.h
- CPU_REG_NVIC_DFSR_EXTERNAL : cpu.h
- CPU_REG_NVIC_DFSR_HALTED : cpu.h
- CPU_REG_NVIC_DFSR_VCATCH : cpu.h
- CPU_REG_NVIC_HFSR : cpu.h
- CPU_REG_NVIC_HFSR_DEBUGEVT : cpu.h
- CPU_REG_NVIC_HFSR_FORCED : cpu.h
- CPU_REG_NVIC_HFSR_VECTTBL : cpu.h
- CPU_REG_NVIC_ICSR : cpu.h
- CPU_REG_NVIC_ICSR_ISRPENDING : cpu.h
- CPU_REG_NVIC_ICSR_ISRPREEMPT : cpu.h
- CPU_REG_NVIC_ICSR_NMIPENDSET : cpu.h
- CPU_REG_NVIC_ICSR_PENDSTCLR : cpu.h
- CPU_REG_NVIC_ICSR_PENDSTSET : cpu.h
- CPU_REG_NVIC_ICSR_PENDSVCLR : cpu.h
- CPU_REG_NVIC_ICSR_PENDSVSET : cpu.h
- CPU_REG_NVIC_ICSR_RETTOBASE : cpu.h
- CPU_REG_NVIC_ISAFR0 : cpu.h
- CPU_REG_NVIC_ISAFR1 : cpu.h
- CPU_REG_NVIC_ISAFR2 : cpu.h
- CPU_REG_NVIC_ISAFR3 : cpu.h
- CPU_REG_NVIC_ISAFR4 : cpu.h
- CPU_REG_NVIC_MMFAR : cpu.h
- CPU_REG_NVIC_MMFR0 : cpu.h
- CPU_REG_NVIC_MMFR1 : cpu.h
- CPU_REG_NVIC_MMFR2 : cpu.h
- CPU_REG_NVIC_MMFR3 : cpu.h
- CPU_REG_NVIC_NVIC : cpu.h
- CPU_REG_NVIC_PFR0 : cpu.h
- CPU_REG_NVIC_PFR1 : cpu.h
- CPU_REG_NVIC_PRIO : cpu.h
- CPU_REG_NVIC_SCR : cpu.h
- CPU_REG_NVIC_SCR_SEVONPEND : cpu.h
- CPU_REG_NVIC_SCR_SLEEPDEEP : cpu.h
- CPU_REG_NVIC_SCR_SLEEPONEXIT : cpu.h
- CPU_REG_NVIC_SETEN : cpu.h
- CPU_REG_NVIC_SETPEND : cpu.h
- CPU_REG_NVIC_SHCSR : cpu.h
- CPU_REG_NVIC_SHCSR_BUSFAULTACT : cpu.h
- CPU_REG_NVIC_SHCSR_BUSFAULTENA : cpu.h
- CPU_REG_NVIC_SHCSR_BUSFAULTPENDED : cpu.h
- CPU_REG_NVIC_SHCSR_MEMFAULTACT : cpu.h
- CPU_REG_NVIC_SHCSR_MEMFAULTENA : cpu.h
- CPU_REG_NVIC_SHCSR_MEMFAULTPENDED : cpu.h
- CPU_REG_NVIC_SHCSR_MONITORACT : cpu.h
- CPU_REG_NVIC_SHCSR_PENDSVACT : cpu.h
- CPU_REG_NVIC_SHCSR_SVCALLACT : cpu.h
- CPU_REG_NVIC_SHCSR_SVCALLPENDED : cpu.h
- CPU_REG_NVIC_SHCSR_SYSTICKACT : cpu.h
- CPU_REG_NVIC_SHCSR_USGFAULTACT : cpu.h
- CPU_REG_NVIC_SHCSR_USGFAULTENA : cpu.h
- CPU_REG_NVIC_SHCSR_USGFAULTPENDED : cpu.h
- CPU_REG_NVIC_SHPRI1 : cpu.h
- CPU_REG_NVIC_SHPRI2 : cpu.h
- CPU_REG_NVIC_SHPRI3 : cpu.h
- CPU_REG_NVIC_ST_CAL : cpu.h
- CPU_REG_NVIC_ST_CAL_NOREF : cpu.h
- CPU_REG_NVIC_ST_CAL_SKEW : cpu.h
- CPU_REG_NVIC_ST_CTRL : cpu.h
- CPU_REG_NVIC_ST_CTRL_CLKSOURCE : cpu.h
- CPU_REG_NVIC_ST_CTRL_COUNTFLAG : cpu.h
- CPU_REG_NVIC_ST_CTRL_ENABLE : cpu.h
- CPU_REG_NVIC_ST_CTRL_TICKINT : cpu.h
- CPU_REG_NVIC_ST_CURRENT : cpu.h
- CPU_REG_NVIC_ST_RELOAD : cpu.h
- CPU_REG_NVIC_SW_TRIG : cpu.h
- CPU_REG_NVIC_VTOR : cpu.h
- CPU_REG_NVIC_VTOR_TBLBASE : cpu.h
- CPU_SR_ALLOC : cpu.h
- CPU_STK_GROWTH_HI_TO_LO : cpu_def.h
- CPU_STK_GROWTH_LO_TO_HI : cpu_def.h
- CPU_STK_GROWTH_NONE : cpu_def.h
- CPU_SW_EXCEPTION : cpu_core.h
- CPU_TIME_MEAS_NBR_MAX : cpu_core.h
- CPU_TIME_MEAS_NBR_MIN : cpu_core.h
- CPU_TO_BE16 : Endianness.h
- cpu_to_be16 : Endianness.h
- cpu_to_be32 : Endianness.h
- CPU_TO_BE32 : Endianness.h
- CPU_TO_LE16 : Endianness.h
- cpu_to_le16 : Endianness.h
- CPU_TO_LE32 : Endianness.h
- cpu_to_le32 : Endianness.h
- CPU_TYPE_CREATE : cpu_core.h
- CPU_WORD_SIZE_08 : cpu_def.h
- CPU_WORD_SIZE_16 : cpu_def.h
- CPU_WORD_SIZE_32 : cpu_def.h
- CPU_WORD_SIZE_64 : cpu_def.h
- CPUCLOCKFRQINKHZ : dfuutil_programming_iflash_algorithm.c
- CRC_MODE_POLY_BITMASK : crc_001.h
- CRC_MODE_POLY_CCITT : crc_001.h
- CRC_MODE_POLY_CRC16 : crc_001.h
- CRC_MODE_POLY_CRC32 : crc_001.h
- CRC_MODE_SUM_BIT_RVS : crc_001.h
- CRC_MODE_SUM_BITMASK : crc_001.h
- CRC_MODE_SUM_CMPL : crc_001.h
- CRC_MODE_WRDATA_BIT_RVS : crc_001.h
- CRC_MODE_WRDATA_BITMASK : crc_001.h
- CRC_MODE_WRDATA_CMPL : crc_001.h
- CRC_SEED_CCITT : crc_001.h
- CRC_SEED_CRC16 : crc_001.h
- CRC_SEED_CRC32 : crc_001.h
- CREATE_LINKMAP : ff.h
- CRYSTAL_32K_FREQ_IN : sys_config.h
- CRYSTAL_MAIN_FREQ_IN : sys_config.h
- CSW_CMD_FAILED : usbd_msc.h
- CSW_CMD_PASSED : usbd_msc.h
- CSW_PHASE_ERROR : usbd_msc.h
- CT_BLOCK : diskio.h
- CT_MMC : diskio.h
- CT_SD1 : diskio.h
- CT_SD2 : diskio.h
- CT_SDC : diskio.h
- CTRL_EJECT : diskio.h
- CTRL_ERASE_SECTOR : diskio.h
- CTRL_FORMAT : diskio.h
- CTRL_LOCK : diskio.h
- CTRL_POWER : diskio.h
- CTRL_RD_EN : HAL_LPC17xx.h
- CTRL_SYNC : diskio.h
- CTRL_WR_EN : HAL_LPC17xx.h
- CTS : usart_002.h
- CTS_DELTA : usart_002.h
- CTS_DELTA_INT : usart_002.h
- CURSOR_H_OFS : Cursor.h
- CURSOR_H_SIZE : Cursor.h
- CURSOR_V_OFS : Cursor.h
- CURSOR_V_SIZE : Cursor.h