| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
ritimer_18xx_43xx.h File Reference

Go to the source code of this file.

## Functions
void | Chip_RIT_Init (LPC_RITIMER_T *pRITimer)
| Initialize the RIT.
void | Chip_RIT_DeInit (LPC_RITIMER_T *pRITimer)
| Shutdown the RIT.
STATIC INLINE void | Chip_RIT_Enable (LPC_RITIMER_T *pRITimer)
| Enable Timer.
STATIC INLINE void | Chip_RIT_Disable (LPC_RITIMER_T *pRITimer)
| Disable Timer.
STATIC INLINE void | Chip_RIT_TimerDebugEnable (LPC_RITIMER_T *pRITimer)
| Enable timer debug.
STATIC INLINE void | Chip_RIT_TimerDebugDisable (LPC_RITIMER_T *pRITimer)
| Disable timer debug.
STATIC INLINE IntStatus | Chip_RIT_GetIntStatus (LPC_RITIMER_T *pRITimer)
| Check whether interrupt flag is set or not.
STATIC INLINE void | Chip_RIT_SetCOMPVAL (LPC_RITIMER_T *pRITimer, uint32_t val)
| Set a tick value for the interrupt to time out.
STATIC INLINE void | Chip_RIT_EnableCTRL (LPC_RITIMER_T *pRITimer, uint32_t val)
| Enables or clears the RIT or interrupt.
STATIC INLINE void | Chip_RIT_ClearInt (LPC_RITIMER_T *pRITimer)
| Clears the RIT interrupt.
STATIC INLINE uint32_t | Chip_RIT_GetCounter (LPC_RITIMER_T *pRITimer)
| Returns the current RIT Counter value.
void | Chip_RIT_SetTimerInterval (LPC_RITIMER_T *pRITimer, uint32_t time_interval)
| Set timer interval value.