| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Structures | Functions
MassStorageClassDevice.h File Reference
`#include "../../USB.h"`
`#include "../Common/MassStorageClassCommon.h"`

Go to the source code of this file.

## Data Structures
struct | USB_ClassInfo_MS_Device_t
| Mass Storage Class Device Mode Configuration and State Structure. More...

## Functions
bool | MS_Device_ConfigureEndpoints (USB_ClassInfo_MS_Device_t *const MSInterfaceInfo) ATTR_NON_NULL_PTR_ARG(1)
| Configures the endpoints of a given Mass Storage interface, ready for use. This should be linked to the library EVENT_USB_Device_ConfigurationChanged() event so that the endpoints are configured when the configuration containing the given Mass Storage interface is selected.
void | MS_Device_ProcessControlRequest (USB_ClassInfo_MS_Device_t *const MSInterfaceInfo) ATTR_NON_NULL_PTR_ARG(1)
| Processes incoming control requests from the host, that are directed to the given Mass Storage class interface. This should be linked to the library EVENT_USB_Device_ControlRequest() event.
void | MS_Device_USBTask (USB_ClassInfo_MS_Device_t *const MSInterfaceInfo) ATTR_NON_NULL_PTR_ARG(1)
| General management task for a given Mass Storage class interface, required for the correct operation of the interface. This should be called frequently in the main program loop, before the master USB management task USB_USBTask().
bool | CALLBACK_MS_Device_SCSICommandReceived (USB_ClassInfo_MS_Device_t *const MSInterfaceInfo) ATTR_NON_NULL_PTR_ARG(1)
| Mass Storage class driver callback for the user processing of a received SCSI command. This callback will fire each time the host sends a SCSI command which requires processing by the user application. Inside this callback the user is responsible for the processing of the received SCSI command from the host. The SCSI command is available in the CommandBlock structure inside the Mass Storage class state structure passed as a parameter to the callback function.