| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
IP_WWDT_001_T Struct Reference
IP: WWDT register block and driver

## Detailed Description

Windowed Watchdog register block structure.

Definition at line 59 of file wwdt_001.h.

`#include "wwdt_001.h"`

## Data Fields
__IO uint32_t | MOD
__IO uint32_t | TC
__O uint32_t | FEED
__I uint32_t | TV
__I uint32_t | RESERVED0
__IO uint32_t | WARNINT
__IO uint32_t | WINDOW

## Field Documentation

__O uint32_t FEED

Watchdog feed sequence register. Writing 0xAA followed by 0x55 to this register reloads the Watchdog timer with the value contained in WDTC.

Definition at line 62 of file wwdt_001.h.

__IO uint32_t MOD

< WWDT Structure Watchdog mode register. This register contains the basic mode and status of the Watchdog Timer.

Definition at line 60 of file wwdt_001.h.

__I uint32_t RESERVED0

Definition at line 67 of file wwdt_001.h.

__IO uint32_t TC

Watchdog timer constant register. This register determines the time-out value.

Definition at line 61 of file wwdt_001.h.

__I uint32_t TV

Watchdog timer value register. This register reads out the current value of the Watchdog timer.

Definition at line 63 of file wwdt_001.h.

__IO uint32_t WARNINT

Watchdog warning interrupt register. This register contains the Watchdog warning interrupt compare value.

Definition at line 70 of file wwdt_001.h.

__IO uint32_t WINDOW

Watchdog timer window register. This register contains the Watchdog window value.

Definition at line 71 of file wwdt_001.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/wwdt_001.h