| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions | Variables
MassStorage.c File Reference
`#include "MassStorage.h"`

Go to the source code of this file.

## Functions
static void | SetupHardware (void)
int | main (void)
| Main program entry point.
void | EVENT_USB_Device_Connect (void)
| Event handler for the library USB Connection event.
void | EVENT_USB_Device_Disconnect (void)
| Event handler for the library USB Disconnection event.
void | EVENT_USB_Device_ConfigurationChanged (void)
| Event handler for the library USB Configuration Changed event.
void | EVENT_USB_Device_ControlRequest (void)
| Event handler for the library USB Control Request reception event.
bool | CALLBACK_MS_Device_SCSICommandReceived (USB_ClassInfo_MS_Device_t *const MSInterfaceInfo)
| Mass Storage class driver callback function.

## Variables
static USB_ClassInfo_MS_Device_t | Disk_MS_Interface

## Function Documentation

static void SetupHardware | ( | void |  | ) |
| static

Definition at line 123 of file MassStorage.c.

## Variable Documentation

USB_ClassInfo_MS_Device_t Disk_MS_Interface
| static

Initial value:
= {
.Config = {
.InterfaceNumber = 0,
.DataINEndpointNumber = MASS_STORAGE_IN_EPNUM,
.DataINEndpointSize = MASS_STORAGE_IO_EPSIZE,
.DataINEndpointDoubleBank = false,
.DataOUTEndpointNumber = MASS_STORAGE_OUT_EPNUM,
.DataOUTEndpointSize = MASS_STORAGE_IO_EPSIZE,
.DataOUTEndpointDoubleBank = false,
.TotalLUNs = TOTAL_LUNS,
.PortNumber = 0,
},
}

nxpUSBlib Mass Storage Class driver interface configuration and state information. This structure is passed to all Mass Storage Class driver functions, so that multiple instances of the same class within a device can be differentiated from one another.

Definition at line 49 of file MassStorage.c.