| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

- All
- Functions
- Variables
- Typedefs
- Enumerations
- Enumerator
- Macros

- a
- b
- c
- d
- e
- f
- g
- h
- i
- j
- k
- l
- m
- n
- o
- p
- q
- r
- s
- t
- u
- v
- w
- x
- y
- z

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - d -

- DAC_BIAS_EN : dac_001.h
- DAC_CCNT_VALUE : dac_001.h
- DAC_CNT_ENA : dac_001.h
- DAC_DACCTRL_MASK : dac_001.h
- DAC_DBLBUF_ENA : dac_001.h
- DAC_DMA_ENA : dac_001.h
- DAC_Interrupt_Done_Flag : dac.c
- DAC_IRQHandler() : cr_startup_lpc18xx43xx.c , cr_freertos_startup_lpc18xx43xx.c , dac.c , cr_ucos_iii_startup_lpc18xx43xx.c , cr_startup_lpc18xx43xx.c
- DAC_MAX_UPDATE_RATE_1MHz : dac_001.h
- DAC_MAX_UPDATE_RATE_400kHz : dac_001.h
- DAC_TIMEOUT : dac.c
- DAC_VALUE : dac_001.h
- DARKGRAY : lpc_colors.h
- DAT_CLR_BUF : HAL_LPC17xx.h
- DAT_GET_DEV_STAT : HAL_LPC17xx.h
- DAT_GET_ERR_CODE : HAL_LPC17xx.h
- DAT_RD_ERR_STAT : HAL_LPC17xx.h
- DAT_RD_FRAME : HAL_LPC17xx.h
- DAT_RD_TEST : HAL_LPC17xx.h
- DAT_SEL_EP : HAL_LPC17xx.h
- DAT_SEL_EP_CLRI : HAL_LPC17xx.h
- DAT_WR_BYTE : HAL_LPC17xx.h
- Data1 : MIDIClassCommon.h
- Data2 : MIDIClassCommon.h
- Data3 : MIDIClassCommon.h
- data_buffer : main.c
- DATA_RAM_BLOCK_SIZE : DataRam.h
- DATA_READ : SCSI.h
- DATA_SIZE : dac.c
- DATA_TIMEOUT : sdmmc_17xx_40xx.c
- DATA_TIMER_VALUE_R : sdmmc_17xx_40xx.c
- DATA_TIMER_VALUE_W : sdmmc_17xx_40xx.c
- DATA_WRITE : SCSI.h
- DATA_X : board_keil_mcb_18574357.h
- DATA_XYZ : board_keil_mcb_18574357.h
- DATA_Y : board_keil_mcb_18574357.h
- DATA_Z : board_keil_mcb_18574357.h
- DataBits : CDCClassCommon.h
- DataflashManager_CheckDataflashOperation() : DataflashManager.c , DataflashManager.h
- DataflashManager_ReadBlocks() : DataflashManager.c , DataflashManager.h
- DataflashManager_ReadBlocks_RAM() : DataflashManager.c , DataflashManager.h
- DataflashManager_ResetDataflashProtections() : DataflashManager.c , DataflashManager.h
- DataflashManager_WriteBlocks() : DataflashManager.c
- DataflashManager_WriteBlocks_RAM() : DataflashManager.c , DataflashManager.h
- DataLength : RNDISClassCommon.h
- DataOffset : RNDISClassCommon.h
- DataRam_Initialize() : ramdisk.c , ramdisk.h , DataRam.c , DataRam.h
- DataRam_ReadBlocks() : ramdisk.c , ramdisk.h , DataRam.c , DataRam.h
- DataRam_WriteBlocks() : ramdisk.c , ramdisk.h , DataRam.c , DataRam.h
- DATASECTORS : fatutil.h
- DataToggle : OHCI.h
- DataToggleControl : EHCI.h
- DataTransferLength : MassStorageClassCommon.h
- DataTransferResidue : MassStorageClassCommon.h
- DATE_DAY : fatutil.h
- DATE_MONTH : fatutil.h
- DATE_YEAR : fatutil.h
- DcdDataTransfer() : Endpoint_LPC11Uxx.h
- DcdIrqHandler() : HAL_LPC18xx.h
- DCOMP_Audio_Host_NextAudioControlInterface() : AudioClassHost.c
- DCOMP_Audio_Host_NextAudioInterfaceDataEndpoint() : AudioClassHost.c
- DCOMP_Audio_Host_NextAudioStreamInterface() : AudioClassHost.c
- DCOMP_CDC_Host_NextCDCControlInterface() : CDCClassHost.c
- DCOMP_CDC_Host_NextCDCDataInterface() : CDCClassHost.c
- DCOMP_CDC_Host_NextCDCInterfaceEndpoint() : CDCClassHost.c
- DCOMP_HID_Host_NextHIDDescriptor() : HIDClassHost.c
- DCOMP_HID_Host_NextHIDInterface() : HIDClassHost.c
- DCOMP_HID_Host_NextHIDInterfaceEndpoint() : HIDClassHost.c
- DCOMP_MIDI_Host_NextMIDIStreamingDataEndpoint() : MIDIClassHost.c
- DCOMP_MIDI_Host_NextMIDIStreamingInterface() : MIDIClassHost.c
- DCOMP_MS_Host_NextMSInterface() : MassStorageClassHost.c
- DCOMP_MS_Host_NextMSInterfaceEndpoint() : MassStorageClassHost.c
- DCOMP_PRNT_Host_NextPRNTInterface() : PrinterClassHost.c
- DCOMP_PRNT_Host_NextPRNTInterfaceEndpoint() : PrinterClassHost.c
- DCOMP_RNDIS_Host_NextRNDISControlInterface() : RNDISClassHost.c
- DCOMP_RNDIS_Host_NextRNDISDataInterface() : RNDISClassHost.c
- DCOMP_RNDIS_Host_NextRNDISInterfaceEndpoint() : RNDISClassHost.c
- DCOMP_SI_Host_NextSIInterface() : StillImageClassHost.c
- DCOMP_SI_Host_NextSIInterfaceEndpoint() : StillImageClassHost.c
- DDE : ff.c
- DEBUG_ENABLE : sys_config.h
- DEBUG_UART : sys_config.h
- DEBUGIN : board_api.h
- DEBUGINIT : board_api.h
- DebugMon_Handler() : cr_freertos_startup_lpc18xx43xx.c , cr_ucos_iii_startup_lpc18xx43xx.c , cr_startup_lpc18xx43xx.c , cr_startup_lpc43xx_m0.c , cr_freertos_startup_lpc17xx40xx.c , cr_ucos_iii_startup_lpc17xx40xx.c , cr_startup_lpc17xx40xx.c , cr_startup_lpc18xx43xx.c , cr_startup_lpc43xx_m0.c , cr_freertos_startup_lpc18xx43xx.c
- DEBUGOUT : board_api.h
- debugstr : app_sdmmc_meas.c , sdmmc.c
- DEBUGSTR : board_api.h
- DEF_ABS : lib_def.h
- DEF_ACTIVE : lib_def.h
- DEF_BIT : lib_def.h
- DEF_BIT_00 : lib_def.h
- DEF_BIT_01 : lib_def.h
- DEF_BIT_02 : lib_def.h
- DEF_BIT_03 : lib_def.h
- DEF_BIT_04 : lib_def.h
- DEF_BIT_05 : lib_def.h
- DEF_BIT_06 : lib_def.h
- DEF_BIT_07 : lib_def.h
- DEF_BIT_08 : lib_def.h
- DEF_BIT_09 : lib_def.h
- DEF_BIT_10 : lib_def.h
- DEF_BIT_11 : lib_def.h
- DEF_BIT_12 : lib_def.h
- DEF_BIT_13 : lib_def.h
- DEF_BIT_14 : lib_def.h
- DEF_BIT_15 : lib_def.h
- DEF_BIT_16 : lib_def.h
- DEF_BIT_17 : lib_def.h
- DEF_BIT_18 : lib_def.h
- DEF_BIT_19 : lib_def.h
- DEF_BIT_20 : lib_def.h
- DEF_BIT_21 : lib_def.h
- DEF_BIT_22 : lib_def.h
- DEF_BIT_23 : lib_def.h
- DEF_BIT_24 : lib_def.h
- DEF_BIT_25 : lib_def.h
- DEF_BIT_26 : lib_def.h
- DEF_BIT_27 : lib_def.h
- DEF_BIT_28 : lib_def.h
- DEF_BIT_29 : lib_def.h
- DEF_BIT_30 : lib_def.h
- DEF_BIT_31 : lib_def.h
- DEF_BIT_32 : lib_def.h
- DEF_BIT_33 : lib_def.h
- DEF_BIT_34 : lib_def.h
- DEF_BIT_35 : lib_def.h
- DEF_BIT_36 : lib_def.h
- DEF_BIT_37 : lib_def.h
- DEF_BIT_38 : lib_def.h
- DEF_BIT_39 : lib_def.h
- DEF_BIT_40 : lib_def.h
- DEF_BIT_41 : lib_def.h
- DEF_BIT_42 : lib_def.h
- DEF_BIT_43 : lib_def.h
- DEF_BIT_44 : lib_def.h
- DEF_BIT_45 : lib_def.h
- DEF_BIT_46 : lib_def.h
- DEF_BIT_47 : lib_def.h
- DEF_BIT_48 : lib_def.h
- DEF_BIT_49 : lib_def.h
- DEF_BIT_50 : lib_def.h
- DEF_BIT_51 : lib_def.h
- DEF_BIT_52 : lib_def.h
- DEF_BIT_53 : lib_def.h
- DEF_BIT_54 : lib_def.h
- DEF_BIT_55 : lib_def.h
- DEF_BIT_56 : lib_def.h
- DEF_BIT_57 : lib_def.h
- DEF_BIT_58 : lib_def.h
- DEF_BIT_59 : lib_def.h
- DEF_BIT_60 : lib_def.h
- DEF_BIT_61 : lib_def.h
- DEF_BIT_62 : lib_def.h
- DEF_BIT_63 : lib_def.h
- DEF_BIT_CLR : lib_def.h
- DEF_BIT_FIELD : lib_def.h
- DEF_BIT_IS_CLR : lib_def.h
- DEF_BIT_IS_CLR_ANY : lib_def.h
- DEF_BIT_IS_SET : lib_def.h
- DEF_BIT_IS_SET_ANY : lib_def.h
- DEF_BIT_MASK : lib_def.h
- DEF_BIT_NONE : lib_def.h
- DEF_BIT_SET : lib_def.h
- DEF_CHK_VAL : lib_def.h
- DEF_CHK_VAL_MAX : lib_def.h
- DEF_CHK_VAL_MIN : lib_def.h
- DEF_CLR : lib_def.h
- DEF_DISABLED : lib_def.h
- DEF_ENABLED : lib_def.h
- DEF_FAIL : lib_def.h
- DEF_FALSE : lib_def.h
- DEF_INACTIVE : lib_def.h
- DEF_INT_08_MASK : lib_def.h
- DEF_INT_08_NBR_BITS : lib_def.h
- DEF_INT_08S_MAX_VAL : lib_def.h
- DEF_INT_08S_MAX_VAL_ONES_CPL : lib_def.h
- DEF_INT_08S_MIN_VAL : lib_def.h
- DEF_INT_08S_MIN_VAL_ONES_CPL : lib_def.h
- DEF_INT_08S_NBR_DIG_MAX : lib_def.h
- DEF_INT_08S_NBR_DIG_MIN : lib_def.h
- DEF_INT_08U_MAX_VAL : lib_def.h
- DEF_INT_08U_MIN_VAL : lib_def.h
- DEF_INT_08U_NBR_DIG_MAX : lib_def.h
- DEF_INT_08U_NBR_DIG_MIN : lib_def.h
- DEF_INT_16_MASK : lib_def.h
- DEF_INT_16_NBR_BITS : lib_def.h
- DEF_INT_16S_MAX_VAL : lib_def.h
- DEF_INT_16S_MAX_VAL_ONES_CPL : lib_def.h
- DEF_INT_16S_MIN_VAL : lib_def.h
- DEF_INT_16S_MIN_VAL_ONES_CPL : lib_def.h
- DEF_INT_16S_NBR_DIG_MAX : lib_def.h
- DEF_INT_16S_NBR_DIG_MIN : lib_def.h
- DEF_INT_16U_MAX_VAL : lib_def.h
- DEF_INT_16U_MIN_VAL : lib_def.h
- DEF_INT_16U_NBR_DIG_MAX : lib_def.h
- DEF_INT_16U_NBR_DIG_MIN : lib_def.h
- DEF_INT_32_MASK : lib_def.h
- DEF_INT_32_NBR_BITS : lib_def.h
- DEF_INT_32S_MAX_VAL : lib_def.h
- DEF_INT_32S_MAX_VAL_ONES_CPL : lib_def.h
- DEF_INT_32S_MIN_VAL : lib_def.h
- DEF_INT_32S_MIN_VAL_ONES_CPL : lib_def.h
- DEF_INT_32S_NBR_DIG_MAX : lib_def.h
- DEF_INT_32S_NBR_DIG_MIN : lib_def.h
- DEF_INT_32U_MAX_VAL : lib_def.h
- DEF_INT_32U_MIN_VAL : lib_def.h
- DEF_INT_32U_NBR_DIG_MAX : lib_def.h
- DEF_INT_32U_NBR_DIG_MIN : lib_def.h
- DEF_INT_64_MASK : lib_def.h
- DEF_INT_64_NBR_BITS : lib_def.h
- DEF_INT_64S_MAX_VAL : lib_def.h
- DEF_INT_64S_MAX_VAL_ONES_CPL : lib_def.h
- DEF_INT_64S_MIN_VAL : lib_def.h
- DEF_INT_64S_MIN_VAL_ONES_CPL : lib_def.h
- DEF_INT_64S_NBR_DIG_MAX : lib_def.h
- DEF_INT_64S_NBR_DIG_MIN : lib_def.h
- DEF_INT_64U_MAX_VAL : lib_def.h
- DEF_INT_64U_MIN_VAL : lib_def.h
- DEF_INT_64U_NBR_DIG_MAX : lib_def.h
- DEF_INT_64U_NBR_DIG_MIN : lib_def.h
- DEF_INT_CPU_NBR_BITS : lib_def.h
- DEF_INVALID : lib_def.h
- DEF_MAX : lib_def.h
- DEF_MIN : lib_def.h
- DEF_NAMEBUF : ff.c
- DEF_NBR_BASE_BIN : lib_def.h
- DEF_NBR_BASE_DEC : lib_def.h
- DEF_NBR_BASE_HEX : lib_def.h
- DEF_NBR_BASE_OCT : lib_def.h
- DEF_NIBBLE_MASK : lib_def.h
- DEF_NIBBLE_NBR_BITS : lib_def.h
- DEF_NO : lib_def.h
- DEF_OCTET_MASK : lib_def.h
- DEF_OCTET_NBR_BITS : lib_def.h
- DEF_OFF : lib_def.h
- DEF_OK : lib_def.h
- DEF_ON : lib_def.h
- DEF_SET : lib_def.h
- DEF_TIME_NBR_DAY_PER_WK : lib_def.h
- DEF_TIME_NBR_DAY_PER_YR : lib_def.h
- DEF_TIME_NBR_DAY_PER_YR_LEAP : lib_def.h
- DEF_TIME_NBR_HR_PER_DAY : lib_def.h
- DEF_TIME_NBR_HR_PER_WK : lib_def.h
- DEF_TIME_NBR_HR_PER_YR : lib_def.h
- DEF_TIME_NBR_HR_PER_YR_LEAP : lib_def.h
- DEF_TIME_NBR_MIN_PER_DAY : lib_def.h
- DEF_TIME_NBR_MIN_PER_HR : lib_def.h
- DEF_TIME_NBR_MIN_PER_WK : lib_def.h
- DEF_TIME_NBR_MIN_PER_YR : lib_def.h
- DEF_TIME_NBR_MIN_PER_YR_LEAP : lib_def.h
- DEF_TIME_NBR_mS_PER_SEC : lib_def.h
- DEF_TIME_NBR_nS_PER_SEC : lib_def.h
- DEF_TIME_NBR_SEC_PER_DAY : lib_def.h
- DEF_TIME_NBR_SEC_PER_HR : lib_def.h
- DEF_TIME_NBR_SEC_PER_MIN : lib_def.h
- DEF_TIME_NBR_SEC_PER_WK : lib_def.h
- DEF_TIME_NBR_SEC_PER_YR : lib_def.h
- DEF_TIME_NBR_SEC_PER_YR_LEAP : lib_def.h
- DEF_TIME_NBR_uS_PER_SEC : lib_def.h
- DEF_TRUE : lib_def.h
- DEF_VALID : lib_def.h
- DEF_YES : lib_def.h
- DEFAULT_ACCEPTMBOX_SIZE : lwipopts.h
- DEFAULT_I2C : i2c.c
- DEFAULT_TCP_RECVMBOX_SIZE : lwipopts.h
- DEFAULT_THREAD_PRIO : lwipopts.h
- DEFAULT_THREAD_STACKSIZE : lwipopts.h
- DEFAULT_UDP_RECVMBOX_SIZE : lwipopts.h
- DeInitTimer() : AudioOutputHost.c
- delay : sct_trafficlight.c , board_ea_devkit_17884088.c , board_hitex_eva_18504350.c , board_keil_mcb_18574357.c , board_ngx_xplorer_18304330.c
- Delay_MS() : Common.h
- DelayConfigStruct : spi.c
- DelayInterrupt : OHCI.h
- delayMs() : board_ea_devkit_17884088.c , board_hitex_eva_18504350.c
- DELTA_RXBRK : usart_002.h
- DELTA_RXBRK_INT : usart_002.h
- desc_array : gpdma_speed_test.c
- DESCRIPTOR_CAST : ConfigDescriptor.h
- DESCRIPTOR_PCAST : ConfigDescriptor.h
- DESCRIPTOR_SEARCH_COMP_EndOfDescriptor : ConfigDescriptor.h
- DESCRIPTOR_SEARCH_COMP_Fail : ConfigDescriptor.h
- DESCRIPTOR_SEARCH_COMP_Found : ConfigDescriptor.h
- DESCRIPTOR_SEARCH_Fail : ConfigDescriptor.h
- DESCRIPTOR_SEARCH_Found : ConfigDescriptor.h
- DESCRIPTOR_SEARCH_NotFound : ConfigDescriptor.h
- DESCRIPTOR_SIZE : ConfigDescriptor.h
- DESCRIPTOR_TYPE : ConfigDescriptor.h
- detectTSCTouch() : board_keil_mcb_18574357.c
- DEV_ADDR_MASK : HAL_LPC17xx.h
- DEV_CON : HAL_LPC17xx.h
- DEV_CON_CH : HAL_LPC17xx.h
- DEV_EN : HAL_LPC17xx.h
- DEV_RST : HAL_LPC17xx.h
- DEV_STAT_INT : HAL_LPC17xx.h , Endpoint_LPC11Uxx.h
- DEV_SUS : HAL_LPC17xx.h
- DEV_SUS_CH : HAL_LPC17xx.h
- DEVICE_STATE_Addressed : Device.h
- DEVICE_STATE_Configured : Device.h
- DEVICE_STATE_Default : Device.h
- DEVICE_STATE_Powered : Device.h
- DEVICE_STATE_Suspended : Device.h
- DEVICE_STATE_Unattached : Device.h
- DEVICE_TYPE_BLOCK : SCSI.h
- DEVICE_TYPE_CDROM : SCSI.h
- DeviceAddress : EHCI.h
- DeviceDescriptor : Descriptors.c
- DeviceFlags : RNDISClassCommon.h
- DeviceType : MassStorageClassCommon.h
- DeviceVcHandle : RNDISClassCommon.h
- DFU_BUFF_PROG_SIZE : dfuutil_programming_any_algorithm.c , dfuutil_programming_iflash_algorithm.c , dfuutil_programming_spiflash_algorithm.c
- dfu_detach() : dfuutil_programming_dfu_ops.c
- dfu_detach_algo : dfuutil_programming_dfu_ops.c
- dfu_done() : dfuutil_programming_dfu_ops.c
- dfu_done_algo : dfuutil_programming_dfu_ops.c
- DFU_EP0_DATA : usbd_dfu.h
- DFU_EP0_NONE : usbd_dfu.h
- DFU_EP0_STALL : usbd_dfu.h
- DFU_EP0_UNHANDLED : usbd_dfu.h
- DFU_EP0_ZLP : usbd_dfu.h
- DFU_FUNC_DESC_SIZE : usbd_dfu.h
- DFU_GET_STATUS_SIZE : usbd_dfu.h
- DFU_HOSTCMD_ERASE_ALL : dfuutil_programming_api.h
- DFU_HOSTCMD_ERASE_REGION : dfuutil_programming_api.h
- DFU_HOSTCMD_EXECUTE : dfuutil_programming_api.h
- DFU_HOSTCMD_PROGRAM : dfuutil_programming_api.h
- DFU_HOSTCMD_READBACK : dfuutil_programming_api.h
- DFU_HOSTCMD_RESET : dfuutil_programming_api.h
- DFU_HOSTCMD_SETDEBUG : dfuutil_programming_api.h
- DFU_HOSTCMD_T : dfuutil_programming_api.h
- DFU_OPSTS_ERASE : dfuutil_programming_api.h
- DFU_OPSTS_ERASE_ALL_ST : dfuutil_programming_api.h
- DFU_OPSTS_ERASE_ST : dfuutil_programming_api.h
- DFU_OPSTS_ERRER : dfuutil_programming_api.h
- DFU_OPSTS_ERRUN : dfuutil_programming_api.h
- DFU_OPSTS_EXEC : dfuutil_programming_api.h
- DFU_OPSTS_IDLE : dfuutil_programming_api.h
- DFU_OPSTS_LOOP : dfuutil_programming_api.h
- DFU_OPSTS_PROG : dfuutil_programming_api.h
- DFU_OPSTS_PROG_RSVD : dfuutil_programming_api.h
- DFU_OPSTS_PROG_STREAM : dfuutil_programming_api.h
- DFU_OPSTS_PROGER : dfuutil_programming_api.h
- DFU_OPSTS_READBUSY : dfuutil_programming_api.h
- DFU_OPSTS_READER : dfuutil_programming_api.h
- DFU_OPSTS_READREADY : dfuutil_programming_api.h
- DFU_OPSTS_READTRIG : dfuutil_programming_api.h
- DFU_OPSTS_RESET : dfuutil_programming_api.h
- DFU_OPSTS_T : dfuutil_programming_api.h
- dfu_rd() : dfuutil_programming_dfu_ops.c
- dfu_state : usbd_dfu.h
- DFU_STATE_appDETACH : usbd_dfu.h
- DFU_STATE_appIDLE : usbd_dfu.h
- DFU_STATE_dfuDNBUSY : usbd_dfu.h
- DFU_STATE_dfuDNLOAD_IDLE : usbd_dfu.h
- DFU_STATE_dfuDNLOAD_SYNC : usbd_dfu.h
- DFU_STATE_dfuERROR : usbd_dfu.h
- DFU_STATE_dfuIDLE : usbd_dfu.h
- DFU_STATE_dfuMANIFEST : usbd_dfu.h
- DFU_STATE_dfuMANIFEST_SYNC : usbd_dfu.h
- DFU_STATE_dfuMANIFEST_WAIT_RST : usbd_dfu.h
- DFU_STATE_dfuUPLOAD_IDLE : usbd_dfu.h
- DFU_STATUS_errADDRESS : usbd_dfu.h
- DFU_STATUS_errCHECK_ERASED : usbd_dfu.h
- DFU_STATUS_errERASE : usbd_dfu.h
- DFU_STATUS_errFILE : usbd_dfu.h
- DFU_STATUS_errFIRMWARE : usbd_dfu.h
- DFU_STATUS_errNOTDONE : usbd_dfu.h
- DFU_STATUS_errPOR : usbd_dfu.h
- DFU_STATUS_errPROG : usbd_dfu.h
- DFU_STATUS_errSTALLEDPKT : usbd_dfu.h
- DFU_STATUS_errTARGET : usbd_dfu.h
- DFU_STATUS_errUNKNOWN : usbd_dfu.h
- DFU_STATUS_errUSBR : usbd_dfu.h
- DFU_STATUS_errVENDOR : usbd_dfu.h
- DFU_STATUS_errVERIFY : usbd_dfu.h
- DFU_STATUS_errWRITE : usbd_dfu.h
- DFU_STATUS_OK : usbd_dfu.h
- dfu_util_process() : dfuutil_programming_dfu_ops.c
- dfu_wr() : dfuutil_programming_dfu_ops.c
- dfuIn : dfuutil_programming_dfu_ops.c
- dfuOut : dfuutil_programming_dfu_ops.c
- dfuprog_regions : dfuutil_programming_dfu_ops.c
- DFUPROG_VALIDVAL : dfuutil_programming_api.h
- dfuProgBuff : dfuutil_programming_dfu_ops.c
- dfuregion : dfuutil_programming_iflash_algorithm.c , dfuutil_programming_any_algorithm.c , dfuutil_programming_spiflash_algorithm.c
- dfuUtilSystemInit() : dfuutil_programming_spiiflash_systeminit.c , dfuutil_programming_iflash_systeminit.c , dfuutil_programming_any_systeminit.c
- DHCP_DEBUG : lwipopts.h
- die() : sdmmc.c , MassStorageHost.c
- DIR_Attr : ff.c
- DIR_CrtDate : ff.c
- DIR_CrtTime : ff.c
- DIR_CrtTimeTenth : ff.c
- DIR_FileSize : ff.c
- dir_find() : ff.c
- DIR_FstClusHI : ff.c
- DIR_FstClusLO : ff.c
- DIR_LstAccDate : ff.c
- DIR_Name : ff.c
- dir_next() : ff.c
- DIR_NTres : ff.c
- dir_read() : ff.c
- dir_register() : ff.c
- dir_remove() : ff.c
- dir_sdi() : ff.c
- DIR_WrtDate : ff.c
- DIR_WrtTime : ff.c
- Direction : EHCI.h , OHCI.h
- DirectionMenu : dac.c
- DirectionPID : OHCI.h
- DIRECTORYSECTORCNT : fatutil.h
- DISABLE : lpc_types.h
- DISABLE_WDT_TIMEOUT : watchdog.c
- DisableAsyncSchedule() : EHCI.h
- DisablePeriodSchedule() : EHCI.h
- DisableSchedule() : EHCI.h
- DISK_HANDLE_T : fsusb_cfg.h
- disk_initialize() : diskio.c , fs_mci.c , fs_usb.c , fs_mem.c , diskio.h
- disk_ioctl() : fs_mem.c , fs_usb.c , fs_mci.c , diskio.h , diskio.c
- Disk_MS_Interface : usbmsdev.c , MassStorage.c , MassStorage_ucosiii.c
- disk_read() : fs_mem.c , fs_usb.c , fs_mci.c , diskio.c , diskio.h
- DISK_READ_ONLY : usbmsdev.h , MassStorage.h
- disk_status() : fs_mci.c , diskio.c , fs_usb.c , fs_mem.c , diskio.h
- disk_write() : diskio.c , fs_mem.c , fs_usb.c , fs_mci.c , diskio.h
- DiskCapacity : MassStorageHost.c
- DiskImage : DataRam.c , ramdisk.c
- DISKSIZE : fatutil.h
- DISPLAY_DRIVER : LCDConf.c
- DISPLAY_HEIGHT : swim_color_bars.c
- DISPLAY_ORIENTATION : LCDConf.c
- DISPLAY_WIDTH : swim_color_bars.c
- DMA_BM_AAL : enet_001.h
- DMA_BM_ATDS : enet_001.h
- DMA_BM_DA : enet_001.h
- DMA_BM_DSL : enet_001.h
- DMA_BM_FB : enet_001.h
- DMA_BM_MB : enet_001.h
- DMA_BM_PBL : enet_001.h
- DMA_BM_PBL8X : enet_001.h
- DMA_BM_PR : enet_001.h
- DMA_BM_RPBL : enet_001.h
- DMA_BM_SWR : enet_001.h
- DMA_BM_TXPR : enet_001.h
- DMA_BM_USP : enet_001.h
- DMA_CONTROLLER : gpdma_18xx_43xx.h , gpdma_17xx_40xx.h
- DMA_DESCRIPTOR_COUNT : gpdma_speed_test.c
- DMA_IE_AIE : enet_001.h
- DMA_IE_ERE : enet_001.h
- DMA_IE_ETE : enet_001.h
- DMA_IE_FBE : enet_001.h
- DMA_IE_NIE : enet_001.h
- DMA_IE_OVE : enet_001.h
- DMA_IE_RIE : enet_001.h
- DMA_IE_RSE : enet_001.h
- DMA_IE_RUE : enet_001.h
- DMA_IE_RWE : enet_001.h
- DMA_IE_TIE : enet_001.h
- DMA_IE_TJE : enet_001.h
- DMA_IE_TSE : enet_001.h
- DMA_IE_TUE : enet_001.h
- DMA_IE_UNE : enet_001.h
- DMA_IRQHandler() : dac.c , uart.c , adc.c , i2s.c , ssp.c , spi.c , ssp.c , i2s.c , uart.c , dac.c , adc.c , gpdma_speed_test.c
- DMA_MFRM_FMA : enet_001.h
- DMA_MFRM_FMCMSK : enet_001.h
- DMA_MFRM_OC : enet_001.h
- DMA_MFRM_OF : enet_001.h
- DMA_OM_DFF : enet_001.h
- DMA_OM_DT : enet_001.h
- DMA_OM_FEF : enet_001.h
- DMA_OM_FTF : enet_001.h
- DMA_OM_FUF : enet_001.h
- DMA_OM_OSF : enet_001.h
- DMA_OM_RSF : enet_001.h
- DMA_OM_RTC : enet_001.h
- DMA_OM_SR : enet_001.h
- DMA_OM_ST : enet_001.h
- DMA_OM_TSF : enet_001.h
- DMA_OM_TTC : enet_001.h
- dma_send_receive : i2s.c
- DMA_ST_AIE : enet_001.h
- DMA_ST_ALL : enet_001.h
- DMA_ST_ERI : enet_001.h
- DMA_ST_ETI : enet_001.h
- DMA_ST_FBI : enet_001.h
- DMA_ST_NIS : enet_001.h
- DMA_ST_OVF : enet_001.h
- DMA_ST_RI : enet_001.h
- DMA_ST_RPS : enet_001.h
- DMA_ST_RU : enet_001.h
- DMA_ST_RWT : enet_001.h
- DMA_ST_TI : enet_001.h
- DMA_ST_TJT : enet_001.h
- DMA_ST_TPS : enet_001.h
- DMA_ST_TU : enet_001.h
- DMA_ST_UNF : enet_001.h
- DMA_TIMEOUT : uart.c
- dma_xfer_complete : gpdma_speed_test.c
- DMAbuffer : dac.c , adc.c , dac.c
- dmaChannelNum : adc.c , dac.c
- dmaChannelNum_I2S_Rx : i2s.c
- dmaChannelNum_I2S_Tx : i2s.c
- dmaChannelNumRx : uart.c
- dmaChannelNumTx : uart.c
- dmaChSSPRx : ssp.c
- dmaChSSPTx : ssp.c
- DMAMUX_Config() : gpdma_17xx_40xx.c , gpdma_18xx_43xx.c
- DP8_100BASE_T4 : lpc_phy_dp83848.c
- DP8_100BASE_TX_FD : lpc_phy_dp83848.c
- DP8_100BASE_TX_HD : lpc_phy_dp83848.c
- DP8_10BASE_T_FD : lpc_phy_dp83848.c
- DP8_10BASE_T_HD : lpc_phy_dp83848.c
- DP8_ANADV_REG : lpc_phy_dp83848.c
- DP8_ANEEXP_REG : lpc_phy_dp83848.c
- DP8_ANLPA_REG : lpc_phy_dp83848.c
- DP8_AUTONEG : lpc_phy_dp83848.c
- DP8_AUTONEG_ABILITY : lpc_phy_dp83848.c
- DP8_AUTONEG_COMP : lpc_phy_dp83848.c
- DP8_BMCR_REG : lpc_phy_dp83848.c
- DP8_BMSR_REG : lpc_phy_dp83848.c
- DP8_COLLISION_TEST : lpc_phy_dp83848.c
- DP8_DUPLEX_MODE : lpc_phy_dp83848.c
- DP8_EXTEND_CAPAB : lpc_phy_dp83848.c
- DP8_FULLDUPLEX : lpc_phy_dp83848.c
- DP8_ISOLATE : lpc_phy_dp83848.c
- DP8_JABBER_DETECT : lpc_phy_dp83848.c
- DP8_LINK_STATUS : lpc_phy_dp83848.c
- DP8_LOOPBACK : lpc_phy_dp83848.c
- DP8_MF_PREAMB_SUPPR : lpc_phy_dp83848.c
- DP8_PHY_INT_CTL_REG : lpc_phy_dp83848.c
- DP8_PHY_RBR_REG : lpc_phy_dp83848.c
- DP8_PHY_STAT_REG : lpc_phy_dp83848.c
- DP8_PHY_STS_REG : lpc_phy_dp83848.c
- DP8_PHYID1_OUI : lpc_phy_dp83848.c
- DP8_PHYID2_OUI : lpc_phy_dp83848.c
- DP8_POWER_DOWN : lpc_phy_dp83848.c
- DP8_RBR_RMII_MODE : lpc_phy_dp83848.c
- DP8_REMOTEFAULT : lpc_phy_dp83848.c
- DP8_RESET : lpc_phy_dp83848.c
- DP8_RESTART_AUTONEG : lpc_phy_dp83848.c
- DP8_RMT_FAULT : lpc_phy_dp83848.c
- DP8_SPEED10MBPS : lpc_phy_dp83848.c
- DP8_SPEED_SELECT : lpc_phy_dp83848.c
- DP8_VALID_LINK : lpc_phy_dp83848.c
- DRAM_BASE_ADDRESS : memtest.c
- DRAM_SIZE : memtest.c
- DRESULT : diskio.h
- DRIVER_MODE_DMA : uartd_8xx.h
- DRIVER_MODE_INTERRUPT : uartd_8xx.h
- DRIVER_MODE_POLLING : uartd_8xx.h
- DSearch_Comp_Return_ErrorCodes_t : ConfigDescriptor.h
- DSearch_Return_ErrorCodes_t : ConfigDescriptor.h
- DST_ADDR_ERROR : flash_001.h
- DST_ADDR_NOT_MAPPED : flash_001.h
- DST_PER_CONTROLLER : gpdma_18xx_43xx.h , gpdma_17xx_40xx.h
- DSTATUS : diskio.h
- DTYPE_Configuration : StdDescriptors.h
- DTYPE_CSEndpoint : StdDescriptors.h
- DTYPE_CSInterface : StdDescriptors.h
- DTYPE_Device : StdDescriptors.h
- DTYPE_DeviceQualifier : StdDescriptors.h
- DTYPE_Endpoint : StdDescriptors.h
- DTYPE_Interface : StdDescriptors.h
- DTYPE_InterfaceAssociation : StdDescriptors.h
- DTYPE_InterfacePower : StdDescriptors.h
- DTYPE_Other : StdDescriptors.h
- DTYPE_String : StdDescriptors.h
- DWORD : integer.h
- dwords : crc.c