| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
UsbRom.h File Reference
`#include "..\VirtualSerial.h"`

Go to the source code of this file.

## Functions
uint32_t | CALLBACK_UsbdRom_Register_DeviceDescriptor (void)
| Call back function registers device descriptor array's address to ROM stack.
uint32_t | CALLBACK_UsbdRom_Register_ConfigurationDescriptor (void)
| Call back function registers device configuration descriptor array's address to ROM stack.
uint32_t | CALLBACK_UsbdRom_Register_StringDescriptor (void)
| Call back function registers string descriptor array's address to ROM stack.
uint32_t | CALLBACK_UsbdRom_Register_DeviceQualifierDescriptor (void)
| Call back function registers device qualifier descriptor array's address to ROM stack.
uint8_t | CALLBACK_UsbdRom_Register_ConfigureEndpoint (void)
| Call back function registers endpoint configuration descriptor array's address to ROM stack.
uint32_t | CALLBACK_UsbdCdc_Register_ControlInterfaceDescriptor (void)
| Call back function registers control interface descriptor.
uint32_t | CALLBACK_UsbdCdc_Register_DataInterfaceDescriptor (void)
| Call back function registers data interface descriptor.
uint32_t | CALLBACK_UsbdCdc_Register_LineCoding (void)
| Call back function registers line encoding.
uint8_t | CALLBACK_UsbdCdc_Register_DataInEndpointNumber (void)
| Call back function registers data in endpoint number.
uint8_t | CALLBACK_UsbdCdc_Register_DataOutEndpointNumber (void)
| Call back function registers data out endpoint number.
uint8_t | CALLBACK_UsbdCdc_Register_NotificationEndpointNumber (void)
| Call back function registers notification endpoint number.
uint32_t | CALLBACK_UsbdCdc_Register_DataInEndpointSize (void)
| Call back function registers data in endpoint size.
uint32_t | CALLBACK_UsbdCdc_Register_DataOutEndpointSize (void)
| Call back function registers data out endpoint size.