| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions
LPC18xx/43xx State Configurable Timer Simple Match example
Misc examples

## Detailed Description

Example description
This example implements the Simple Match example using State Configurable Timer module. The FSM is built by using FZM tool. The FZM tool can be downloded from :
SCT Tools

Special connection requirements

- Hitex LPC1850EVA-A4-2 and LPC4350EVA-A4-2 boards
  Observe the outputs at CTOUT3, CTOUT2, CTOUT4, CTOUT5 using oscilloscope (and RGB LEDs toggling)
- Keil MCB1857 and MCB4357 boards
  Observe the outputs at CTOUT14, CTOUT10, CTOUT13, CTOUT11 using oscilloscope (and LEDs toggling)
- NGX Xplorer 1830 and 4330 boards
  Observe the outputs at CTOUT5, CTOUT4, CTOUT2, CTOUT3 using oscilloscope (and LEDs toggling)

Build procedures:
LPC18xx/43xx example quickstart for Keil uVision4
LPC18xx/43xx example quickstart for IAR EWARM
LPC18xx/43xx example quickstart for Code Red Xpresso

Supported boards and board setup:
Hitex 1850 evaluation boards
Hitex 4350 evaluation boards
Keil 1857 evaluation boards
Keil 4357 evaluation boards
NGX 1830 Xplorer boards
NGX 4330 Xplorer boards

Submitting LPCOpen issues:
Community support for LPCOpen

## Functions
void | SCT_PinsConfigure (void)
int | main (void)
| Main entry point.

## Function Documentation

int main | ( | void |  | ) |

Main entry point.

Main program body.

Returns
  Nothing

Definition at line 143 of file sct_simple_match.c.

void SCT_PinsConfigure | ( | void |  | ) |

Definition at line 87 of file sct_simple_match.c.