| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Fields
IP_CAN_MSG_T Struct Reference
IP: CAN register block and driver

## Detailed Description

CAN Message Object Structure.

Definition at line 663 of file can_001.h.

`#include "can_001.h"`

## Data Fields
uint32_t | ID
uint32_t | Type
uint32_t | DLC
uint8_t | Data [CAN_MSG_MAX_DATA_LEN]

## Field Documentation

uint8_t Data[CAN_MSG_MAX_DATA_LEN]

Message Data

Definition at line 668 of file can_001.h.

uint32_t DLC

Message Data Length: 0~8

Definition at line 667 of file can_001.h.

uint32_t ID

Message Identifier. If 30th-bit is set, this is 29-bit ID, othewise 11-bit ID

Definition at line 665 of file can_001.h.

uint32_t Type

Message Type. which can include: - CAN_REMOTE_MSG type

Definition at line 666 of file can_001.h.

The documentation for this struct was generated from the following file:

- C:/nxp/v1.03/lpcopen_v1.03/lpcopen/software/lpc_core/lpc_ip/can_001.h