| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
sdc_17xx_40xx.h
Go to the documentation of this file.
1 /*
2 * @brief LPC17xx/40xx SD Card Interface driver
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __SDC_17XX_40XX_H_
33 #define __SDC_17XX_40XX_H_
34
35 #ifdef __cplusplus
36 extern "C" {
37 #endif
38
47 typedef enum CHIP_SDC_RET_CODE {
48 SDC_RET_OK = 0,
49 SDC_RET_CMD_FAILED = -1,
50 SDC_RET_BAD_PARAMETERS = -2,
51 SDC_RET_BUS_NOT_IDLE = -3,
52 SDC_RET_TIMEOUT = -4,
53 SDC_RET_ERR_STATE = -5,
54 SDC_RET_NOT_READY = -6,
55 SDC_RET_FAILED = -7,
56 } CHIP_SDC_RET_CODE_T;
57
63 void Chip_SDC_Init(LPC_SDC_T *pSDC);
64
71 void Chip_SDC_SetClock(LPC_SDC_T *pSDC, uint32_t freq);
72
78 void Chip_SDC_DeInit(LPC_SDC_T *pSDC);
79
86 STATIC INLINE void Chip_SDC_SetIntMask(LPC_SDC_T *pSDC, uint32_t iVal)
87 {
88 IP_SDC_SetIntMask(pSDC, iVal);
89 }
90
96 STATIC INLINE uint32_t Chip_SDC_GetStatus(LPC_SDC_T *pSDC)
97 {
98 return IP_SDC_GetStatus(pSDC);
99 }
100
105 #ifdef __cplusplus
106 }
107 #endif
108
109 #endif /* __SDC_17XX_40XX_H_ */