| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Data Structures | Enumerations | Functions
rgu_18xx_43xx.h File Reference

Go to the source code of this file.

## Data Structures
struct | LPC_RGU_T
| RGU register structure. More...

## Enumerations
enum | CHIP_RGU_RST_T { RGU_CORE_RST, RGU_PERIPH_RST, RGU_MASTER_RST, RGU_WWDT_RST = 4, RGU_CREG_RST, RGU_BUS_RST = 8, RGU_SCU_RST, RGU_M3_RST = 13, RGU_LCD_RST = 16, RGU_USB0_RST, RGU_USB1_RST, RGU_DMA_RST, RGU_SDIO_RST, RGU_EMC_RST, RGU_ETHERNET_RST, RGU_FLASHA_RST = 25, RGU_EEPROM_RST = 27, RGU_GPIO_RST, RGU_FLASHB_RST, RGU_TIMER0_RST = 32, RGU_TIMER1_RST, RGU_TIMER2_RST, RGU_TIMER3_RST, RGU_RITIMER_RST, RGU_SCT_RST, RGU_MOTOCONPWM_RST, RGU_QEI_RST, RGU_ADC0_RST, RGU_ADC1_RST, RGU_DAC_RST, RGU_UART0_RST = 44, RGU_UART1_RST, RGU_UART2_RST, RGU_UART3_RST, RGU_I2C0_RST, RGU_I2C1_RST, RGU_SSP0_RST, RGU_SSP1_RST, RGU_I2S_RST, RGU_SPIFI_RST, RGU_CAN1_RST, RGU_CAN0_RST, RGU_LAST_RST = 63 }
| RGU reset enumerations. More...

## Functions
void | Chip_RGU_TriggerReset (CHIP_RGU_RST_T ResetNumber)
| Trigger a peripheral reset for the selected peripheral.
bool | Chip_RGU_InReset (CHIP_RGU_RST_T ResetNumber)
| Checks the reset status of a peripheral.
void | Chip_RGU_ClearReset (CHIP_RGU_RST_T ResetNumber)
| Clears reset for the selected peripheral.