| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions | Variables
LPC13xx ADC example
Peripheral examples

## Detailed Description

Example description
The ADC example shows how to use the A/D converter on the LPC13XX. The example is setup to get the ADC values periodically and print it out via UART.

To use this example, build and program it and then run it on the LPCXpresso board with LPCXpresso Base Board rev A. Turn potentiometer on Base board to change ADC signal input.Converted ADC values is displayed periodically via the UART.

Special connection requirements
Connect the Jumper J27 on the LPCXpresso Base Board rev A. Connect the UART to display ADC value on your computer

Build procedures:
LPC13xx example quickstart for Code Red Xpresso
LPC13xx example quickstart for Keil uVision4
LPC13xx example quickstart for IAR EWARM

Supported boards and board setup:
NXP Xpresso LPC1347 board

Submitting LPCOpen issues:
Community support for LPCOpen

## Functions
static void | App_print_ADC_value (uint16_t data)
static void | App_Polling_Test (void)
int | main (void)
| main routine for ADC example

## Variables
static ADC_Clock_Setup_T | ADCSetup

## Function Documentation

static void App_Polling_Test | ( | void |  | ) |
| static

Definition at line 99 of file adc.c.

static void App_print_ADC_value | ( | uint16_t | data | ) |
| static

Definition at line 80 of file adc.c.

int main | ( | void |  | ) |

main routine for ADC example

Main program body.

Returns
  Function should not exit.

defined(CHIP_LPC175X_6X)

Definition at line 126 of file adc.c.

## Variable Documentation

ADC_Clock_Setup_T ADCSetup
| static

Definition at line 69 of file adc.c.