| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Functions | Variables
HAL.h File Reference

Go to the source code of this file.

## Functions
void | HAL_USBInit (uint8_t corenum)
| This function is called by void USB_Init(void) to do the initialization for chip's USB core. Normally, this function will do the following:
void | HAL_USBDeInit (uint8_t corenum, uint8_t mode)
| This function usage is opposite to HAL_USBInit.
void | HAL_EnableUSBInterrupt (uint8_t corenum)
| This function used to enable USB interrupt.
void | HAL_DisableUSBInterrupt (uint8_t corenum)
| This function usage is opposite to HAL_EnableUSBInterrupt.
void | HAL_USBConnect (uint8_t corenum, uint32_t con)
| This function is used in device mode to pull up resistor on USB pin D+ Normally, this function is called when every setup or initial are done.

## Variables
uint8_t | USBPortNum