| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Macros | Typedefs | Enumerations | Functions
can_17xx_40xx.h File Reference

Go to the source code of this file.

## Macros
#define | CAN_SEG1_DEFAULT_VAL 5
#define | CAN_SEG2_DEFAULT_VAL 4
#define | CAN_SJW_DEFAULT_VAL 0

## Typedefs
typedef IP_CAN_AF_LUT_T | CANAF_LUT_T
| CAN structures and definitions.
typedef IP_CAN_STD_ID_Entry_T | CAN_STD_ID_ENTRY_T
typedef IP_CAN_STD_ID_RANGE_Entry_T | CAN_STD_ID_RANGE_ENTRY_T
typedef IP_CAN_EXT_ID_Entry_T | CAN_EXT_ID_ENTRY_T
typedef IP_CAN_EXT_ID_RANGE_Entry_T | CAN_EXT_ID_RANGE_ENTRY_T
typedef IP_CAN_MSG_T | CAN_MSG_T
typedef IP_CAN_BUFFER_ID_T | CAN_BUFFER_ID
typedef IP_CAN_AF_RAM_SECTION_T | CANAF_RAM_SECTION

## Enumerations
enum | CHIP_CAN_MODE_T { CAN_RESET_MODE = CAN_MOD_RM, CAN_SELFTEST_MODE = CAN_MOD_STM, CAN_TEST_MODE = CAN_MOD_TM, CAN_LISTEN_ONLY_MODE = CAN_MOD_LOM, CAN_SLEEP_MODE = CAN_MOD_SM, CAN_OPERATION_MODE = CAN_MOD_OPERATION, CAN_TRANSMIT_PRIORITY_MODE = CAN_MOD_TPM, CAN_RECEIVE_PRIORITY_MODE = CAN_MOD_RPM }
| CAN Mode definition. More...
enum | CHIP_CAN_AF_MODE_T { CAN_AF_NORMAL_MODE = 0, CAN_AF_OFF_MODE = CANAF_AFMR_ACCOFF, CAN_AF_BYBASS_MODE = CANAF_AFMR_ACCBP, CAN_AF_FULL_MODE = CANAF_AFMR_EFCAN }
| CAN AF Mode definition. More...

## Functions
STATIC INLINE uint32_t | Chip_CAN_GetStatus (LPC_CAN_T *pCAN)
| Get the status of the CAN Controller.
STATIC INLINE void | Chip_CAN_IntEnable (LPC_CAN_T *pCAN, uint32_t IntMask)
| Enable the CAN Interrupts.
STATIC INLINE void | Chip_CAN_IntDisable (LPC_CAN_T *pCAN, uint32_t IntMask)
| Disable the CAN Interrupts.
STATIC INLINE uint32_t | Chip_CAN_GetIntStatus (LPC_CAN_T *pCAN)
| Get interrupt status of the given CAN Controller.
STATIC INLINE void | Chip_CAN_FullCANIntConfig (LPC_CANAF_T *pCANAF, FunctionalState NewState)
| Enable/Disable CAN controller FullCAN Interrupts.
STATIC INLINE uint32_t | Chip_CAN_GetFullCANIntStatus (LPC_CANAF_T *pCANAF, uint8_t ObjID)
| Get FullCAN interrupt status of the given object.
STATIC INLINE void | Chip_CAN_SetMode (LPC_CAN_T *pCAN, CHIP_CAN_MODE_T Mode, FunctionalState NewState)
| Set CAN controller enter/exit to a given mode.
STATIC INLINE void | Chip_CAN_SetAFMode (LPC_CANAF_T *pCANAF, CHIP_CAN_AF_MODE_T AfMode)
| Set CAN AF Mode.
STATIC INLINE Status | Chip_CAN_SetAFLUT (LPC_CANAF_T *pCANAF, CANAF_LUT_T *pAFSections)
| Set CAN AF LUT.
STATIC INLINE Status | Chip_CAN_InsertFullCANEntry (LPC_CANAF_T *pCANAF, CAN_STD_ID_ENTRY_T *pEntry)
| Insert a FullCAN Entry into the current LUT.
STATIC INLINE Status | Chip_CAN_InsertIndividualSTDEntry (LPC_CANAF_T *pCANAF, CAN_STD_ID_ENTRY_T *pEntry)
| Insert an individual Standard Entry into the current LUT.
STATIC INLINE Status | Chip_CAN_InsertGroupSTDEntry (LPC_CANAF_T *pCANAF, CAN_STD_ID_RANGE_ENTRY_T *pEntry)
| Insert an Group Standard Entry into the current LUT.
STATIC INLINE Status | Chip_CAN_InsertIndividualEXTEntry (LPC_CANAF_T *pCANAF, CAN_EXT_ID_ENTRY_T *pEntry)
| Insert an individual Extended Entry into the current LUT.
STATIC INLINE Status | Chip_CAN_InsertGroupEXTEntry (LPC_CANAF_T *pCANAF, CAN_EXT_ID_RANGE_ENTRY_T *pEntry)
| Insert an Group Extended Entry into the current LUT.
STATIC INLINE Status | Chip_CAN_RemoveFullCANEntry (LPC_CANAF_T *pCANAF, int16_t Position)
| Remove a FullCAN Entry from the current LUT.
STATIC INLINE Status | Chip_CAN_RemoveIndividualSTDEntry (LPC_CANAF_T *pCANAF, int16_t Position)
| Remove an individual Standard Entry from the current LUT.
STATIC INLINE Status | Chip_CAN_RemoveGroupSTDEntry (LPC_CANAF_T *pCANAF, int16_t Position)
| Remove an Group Standard Entry from the current LUT.
STATIC INLINE Status | Chip_CAN_RemoveIndividualEXTEntry (LPC_CANAF_T *pCANAF, int16_t Position)
| Remove an individual Extended Entry from the current LUT.
STATIC INLINE Status | Chip_CAN_RemoveGroupEXTEntry (LPC_CANAF_T *pCANAF, int16_t Position)
| Remove an Group Extended Entry from the current LUT.
STATIC INLINE uint16_t | Chip_CAN_GetEntriesNum (LPC_CANAF_T *pCANAF, CANAF_RAM_SECTION SectionID)
| Get the number of entries in the given section.
STATIC INLINE Status | Chip_CAN_ReadFullCANEntry (LPC_CANAF_T *pCANAF, uint16_t Position, CAN_STD_ID_ENTRY_T *pEntry)
| Read a FullCAN Entry into from current LUT.
STATIC INLINE Status | Chip_CAN_ReadIndividualSTDEntry (LPC_CANAF_T *pCANAF, uint16_t Position, CAN_STD_ID_ENTRY_T *pEntry)
| Read an individual Standard Entry from the current LUT.
STATIC INLINE Status | Chip_CAN_ReadGroupSTDEntry (LPC_CANAF_T *pCANAF, uint16_t Position, CAN_STD_ID_RANGE_ENTRY_T *pEntry)
| Read an Group Standard Entry from the current LUT.
STATIC INLINE Status | Chip_CAN_ReadIndividualEXTEntry (LPC_CANAF_T *pCANAF, uint16_t Position, CAN_EXT_ID_ENTRY_T *pEntry)
| Read an individual Extended Entry from the current LUT.
STATIC INLINE Status | Chip_CAN_ReadGroupEXTEntry (LPC_CANAF_T *pCANAF, uint16_t Position, CAN_EXT_ID_RANGE_ENTRY_T *pEntry)
| Read an Group Extended Entry from the current LUT.
STATIC INLINE Status | Chip_CAN_Receive (LPC_CAN_T *pCAN, CAN_MSG_T *pMsg)
| Get message received by the CAN Controller.
STATIC INLINE Status | Chip_CAN_FullCANReceive (LPC_CANAF_T *pCANAF, uint8_t ObjID, CAN_MSG_T *pMsg, uint8_t *pSCC)
| Get message received automatically by the AF.
STATIC INLINE Status | Chip_CAN_Send (LPC_CAN_T *pCAN, CAN_BUFFER_ID TxBufID, CAN_MSG_T *pMsg)
| Request the given CAN Controller to send message.
void | Chip_CAN_Init (LPC_CAN_T *pCAN)
| Initialize CAN Interface.
void | Chip_CAN_DeInit (LPC_CAN_T *pCAN)
| De-Initialize CAN Interface.
Status | Chip_CAN_SetBitRate (LPC_CAN_T *pCAN, uint32_t BitRate)
| Set CAN bitrate.
CAN_BUFFER_ID | Chip_CAN_GetFreeTxBuf (LPC_CAN_T *pCAN)
| Get Free TxBuffer.