| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
ritimer_18xx_43xx.h
Go to the documentation of this file.
1 /*
2 * @brief LPC18xx/43xx RITimer chip driver
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __RITIMER_18XX_43XX_H_
33 #define __RITIMER_18XX_43XX_H_
34
35 #ifdef __cplusplus
36 extern "C" {
37 #endif
38
49 void Chip_RIT_Init(LPC_RITIMER_T *pRITimer);
50
56 void Chip_RIT_DeInit(LPC_RITIMER_T *pRITimer);
57
63 STATIC INLINE void Chip_RIT_Enable(LPC_RITIMER_T *pRITimer)
64 {
65 IP_RIT_Enable(pRITimer);
66 }
67
73 STATIC INLINE void Chip_RIT_Disable(LPC_RITIMER_T *pRITimer)
74 {
75 IP_RIT_Disable(pRITimer);
76 }
77
83 STATIC INLINE void Chip_RIT_TimerDebugEnable(LPC_RITIMER_T *pRITimer)
84 {
85 IP_RIT_TimerDebugEnable(pRITimer);
86 }
87
93 STATIC INLINE void Chip_RIT_TimerDebugDisable(LPC_RITIMER_T *pRITimer)
94 {
95 IP_RIT_TimerDebugDisable(pRITimer);
96 }
97
103 STATIC INLINE IntStatus Chip_RIT_GetIntStatus(LPC_RITIMER_T *pRITimer)
104 {
105 return IP_RIT_GetIntStatus(pRITimer);
106 }
107
114 STATIC INLINE void Chip_RIT_SetCOMPVAL(LPC_RITIMER_T *pRITimer, uint32_t val)
115 {
116 IP_RIT_SetCOMPVAL(pRITimer, val);
117 }
118
125 STATIC INLINE void Chip_RIT_EnableCTRL(LPC_RITIMER_T *pRITimer, uint32_t val)
126 {
127 IP_RIT_EnableCTRL(pRITimer, val);
128 }
129
135 STATIC INLINE void Chip_RIT_ClearInt(LPC_RITIMER_T *pRITimer)
136 {
137 IP_RIT_EnableCTRL(pRITimer, RIT_CTRL_INT);
138 }
139
145 STATIC INLINE uint32_t Chip_RIT_GetCounter(LPC_RITIMER_T *pRITimer)
146 {
147 return IP_RIT_GetCounter(pRITimer);
148 }
149
156 void Chip_RIT_SetTimerInterval(LPC_RITIMER_T *pRITimer, uint32_t time_interval);
157
162 #ifdef __cplusplus
163 }
164 #endif
165
166 #endif /* __RITIMER_18XX_43XX_H_ */