| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
usb_001.h
Go to the documentation of this file.
1 /*
2 * @brief USB registers and control functions
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __USB_001_H_
33 #define __USB_001_H_
34
35 #include "sys_config.h"
36 #include "cmsis.h"
37
38 #ifdef __cplusplus
39 extern "C" {
40 #endif
41
52 typedef struct
53 {
54 __I uint32_t Revision; /* USB Host Registers */
55 __IO uint32_t Control;
56 __IO uint32_t CommandStatus;
57 __IO uint32_t InterruptStatus;
58 __IO uint32_t InterruptEnable;
59 __IO uint32_t InterruptDisable;
60 __IO uint32_t HCCA;
61 __I uint32_t PeriodCurrentED;
62 __IO uint32_t ControlHeadED;
63 __IO uint32_t ControlCurrentED;
64 __IO uint32_t BulkHeadED;
65 __IO uint32_t BulkCurrentED;
66 __I uint32_t DoneHead;
67 __IO uint32_t FmInterval;
68 __I uint32_t FmRemaining;
69 __I uint32_t FmNumber;
70 __IO uint32_t PeriodicStart;
71 __IO uint32_t LSTreshold;
72 __IO uint32_t RhDescriptorA;
73 __IO uint32_t RhDescriptorB;
74 __IO uint32_t RhStatus;
75 __IO uint32_t RhPortStatus1;
76 __IO uint32_t RhPortStatus2;
77 uint32_t RESERVED0[40];
78 __I uint32_t Module_ID;
79
80 __I uint32_t IntSt; /* USB On-The-Go Registers */
81 __IO uint32_t IntEn;
82 __O uint32_t IntSet;
83 __O uint32_t IntClr;
84 __IO uint32_t StCtrl;
85 __IO uint32_t Tmr;
86 uint32_t RESERVED1[58];
87
88 __I uint32_t DevIntSt; /* USB Device Interrupt Registers */
89 __IO uint32_t DevIntEn;
90 __O uint32_t DevIntClr;
91 __O uint32_t DevIntSet;
92
93 __O uint32_t CmdCode; /* USB Device SIE Command Registers */
94 __I uint32_t CmdData;
95
96 __I uint32_t RxData; /* USB Device Transfer Registers */
97 __O uint32_t TxData;
98 __I uint32_t RxPLen;
99 __O uint32_t TxPLen;
100 __IO uint32_t Ctrl;
101 __O uint32_t DevIntPri;
102
103 __I uint32_t EpIntSt; /* USB Device Endpoint Interrupt Regs */
104 __IO uint32_t EpIntEn;
105 __O uint32_t EpIntClr;
106 __O uint32_t EpIntSet;
107 __O uint32_t EpIntPri;
108
109 __IO uint32_t ReEp; /* USB Device Endpoint Realization Reg*/
110 __O uint32_t EpInd;
111 __IO uint32_t MaxPSize;
112
113 __I uint32_t DMARSt; /* USB Device DMA Registers */
114 __O uint32_t DMARClr;
115 __O uint32_t DMARSet;
116 uint32_t RESERVED2[9];
117 __IO uint32_t UDCAH;
118 __I uint32_t EpDMASt;
119 __O uint32_t EpDMAEn;
120 __O uint32_t EpDMADis;
121 __I uint32_t DMAIntSt;
122 __IO uint32_t DMAIntEn;
123 uint32_t RESERVED3[2];
124 __I uint32_t EoTIntSt;
125 __O uint32_t EoTIntClr;
126 __O uint32_t EoTIntSet;
127 __I uint32_t NDDRIntSt;
128 __O uint32_t NDDRIntClr;
129 __O uint32_t NDDRIntSet;
130 __I uint32_t SysErrIntSt;
131 __O uint32_t SysErrIntClr;
132 __O uint32_t SysErrIntSet;
133 uint32_t RESERVED4[15];
134
135 union {
136 __I uint32_t I2C_RX; /* USB OTG I2C Registers */
137 __O uint32_t I2C_TX;
138 };
139 __IO uint32_t I2C_STS;
140 __IO uint32_t I2C_CTL;
141 __IO uint32_t I2C_CLKHI;
142 __O uint32_t I2C_CLKLO;
143 uint32_t RESERVED5[824];
144
145 union {
146 __IO uint32_t USBClkCtrl; /* USB Clock Control Registers */
147 __IO uint32_t OTGClkCtrl;
148 };
149 union {
150 __I uint32_t USBClkSt;
151 __I uint32_t OTGClkSt;
152 };
153 } IP_USB_001_T;
158 #ifdef __cplusplus
159 }
160 #endif
161
162 #endif /* __USB_001_H_ */
163