| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Enumerations | Functions
sct_8xx.h File Reference

Go to the source code of this file.

## Enumerations
enum | CHIP_SCT_MATCH_REG_T { SCT_MATCH_0 = 0, SCT_MATCH_1 = 1, SCT_MATCH_2 = 2, SCT_MATCH_3 = 3, SCT_MATCH_4 = 4 }
enum | CHIP_SCT_EVENT_T { SCT_EVT_0 = (1 << 0), SCT_EVT_1 = (1 << 1), SCT_EVT_2 = (1 << 2), SCT_EVT_3 = (1 << 3), SCT_EVT_4 = (1 << 4) }

## Functions
STATIC INLINE void | Chip_SCT_Config (LPC_SCT_T *pSCT, uint32_t value)
| Configures the State Configurable Timer.
STATIC INLINE void | Chip_SCT_SetCount (LPC_SCT_T *pSCT, uint32_t count)
| Set unified count value in State Configurable Timer.
STATIC INLINE void | Chip_SCT_SetCountL (LPC_SCT_T *pSCT, uint16_t count)
| Set lower count value in State Configurable Timer.
STATIC INLINE void | Chip_SCT_SetCountH (LPC_SCT_T *pSCT, uint16_t count)
| Set higher count value in State Configurable Timer.
STATIC INLINE void | Chip_SCT_SetMatchCount (LPC_SCT_T *pSCT, CHIP_SCT_MATCH_REG_T n, uint32_t value)
| Set unified match count value in State Configurable Timer.
STATIC INLINE void | Chip_SCT_SetMatchReload (LPC_SCT_T *pSCT, CHIP_SCT_MATCH_REG_T n, uint32_t value)
| Set unified match reload count value in State Configurable Timer.
STATIC INLINE void | Chip_SCT_EventIntEnable (LPC_SCT_T *pSCT, CHIP_SCT_EVENT_T evt)
| Enable the interrupt for the specified event in State Configurable Timer.
STATIC INLINE void | Chip_SCT_EventIntDisable (LPC_SCT_T *pSCT, CHIP_SCT_EVENT_T evt)
| Disable the interrupt for the specified event in State Configurable Timer.
STATIC INLINE void | Chip_SCT_ClearEventFlag (LPC_SCT_T *pSCT, CHIP_SCT_EVENT_T evt)
| Clear the specified event flag in State Configurable Timer.
void | Chip_SCT_Init (LPC_SCT_T *pSCT)
| Initializes the State Configurable Timer.
void | Chip_SCT_DeInit (LPC_SCT_T *pSCT)
| Deinitializes the State Configurable Timer.