| LPCOpen Platform v1.03 LPCOpen Platform for NXP LPC Microcontrollers

- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
rtc_17xx_40xx.h
Go to the documentation of this file.
1 /*
2 * @brief LPC17xx/40xx RTC driver
3 *
4 * @note
5 * Copyright(C) NXP Semiconductors, 2012
6 * All rights reserved.
7 *
8 * @par
9 * Software that is described herein is for illustrative purposes only
10 * which provides customers with programming information regarding the
11 * LPC products. This software is supplied "AS IS" without any warranties of
12 * any kind, and NXP Semiconductors and its licensor disclaim any and
13 * all warranties, express or implied, including all implied warranties of
14 * merchantability, fitness for a particular purpose and non-infringement of
15 * intellectual property rights. NXP Semiconductors assumes no responsibility
16 * or liability for the use of the software, conveys no license or rights under any
17 * patent, copyright, mask work right, or any other intellectual property rights in
18 * or to any products. NXP Semiconductors reserves the right to make changes
19 * in the software without notification. NXP Semiconductors also makes no
20 * representation or warranty that such application will be suitable for the
21 * specified use without further testing or modification.
22 *
23 * @par
24 * Permission to use, copy, modify, and distribute this software and its
25 * documentation is hereby granted, under NXP Semiconductors' and its
26 * licensor's relevant copyrights in the software, without fee, provided that it
27 * is used in conjunction with NXP Semiconductors microcontrollers. This
28 * copyright, permission, and disclaimer notice must appear in all copies of
29 * this code.
30 */
31
32 #ifndef __RTC_17XX_40XX_H_
33 #define __RTC_17XX_40XX_H_
34
35 #ifdef __cplusplus
36 extern "C" {
37 #endif
38
44 #if RTC_EV_SUPPORT
45
46 typedef IP_RTC_EV_CHANNEL_T RTC_EV_CHANNEL_T;
48 typedef IP_RTC_EV_MODE_T RTC_EV_MODE_T;
50 typedef IP_RTC_EV_TIMESTAMP_T RTC_EV_TIMESTAMP_T;
51 #endif /*RTC_EV_SUPPORT*/
52
58 STATIC INLINE void Chip_RTC_ResetClockTickCounter(LPC_RTC_T *pRTC)
59 {
60 IP_RTC_ResetClockTickCounter(pRTC);
61 }
62
71 STATIC INLINE void Chip_RTC_Enable(LPC_RTC_T *pRTC, FunctionalState NewState)
72 {
73 IP_RTC_Enable(pRTC, NewState);
74 }
75
83 STATIC INLINE void Chip_RTC_CntIncrIntConfig(LPC_RTC_T *pRTC, uint32_t cntrMask, FunctionalState NewState)
84 {
85 IP_RTC_CntIncrIntConfig(pRTC, cntrMask, NewState);
86 }
87
95 STATIC INLINE void Chip_RTC_AlarmIntConfig(LPC_RTC_T *pRTC, uint32_t alarmMask, FunctionalState NewState)
96 {
97 IP_RTC_AlarmIntConfig(pRTC, alarmMask, NewState);
98 }
99
107 STATIC INLINE void Chip_RTC_SetTime(LPC_RTC_T *pRTC, IP_RTC_TIMEINDEX_T Timetype, uint32_t TimeValue)
108 {
109 IP_RTC_SetTime(pRTC, Timetype, TimeValue);
110 }
111
118 STATIC INLINE uint32_t Chip_RTC_GetTime(LPC_RTC_T *pRTC, IP_RTC_TIMEINDEX_T Timetype)
119 {
120 return IP_RTC_GetTime(pRTC, Timetype);
121 }
122
129 STATIC INLINE void Chip_RTC_SetFullTime(LPC_RTC_T *pRTC, IP_RTC_TIME_T *pFullTime)
130 {
131 IP_RTC_SetFullTime(pRTC, pFullTime);
132 }
133
140 STATIC INLINE void Chip_RTC_GetFullTime(LPC_RTC_T *pRTC, IP_RTC_TIME_T *pFullTime)
141 {
142 IP_RTC_GetFullTime(pRTC, pFullTime);
143 }
144
152 STATIC INLINE void Chip_RTC_SetAlarmTime(LPC_RTC_T *pRTC, IP_RTC_TIMEINDEX_T Timetype, uint32_t ALValue)
153 {
154 IP_RTC_SetAlarmTime(pRTC, Timetype, ALValue);
155 }
156
163 STATIC INLINE uint32_t Chip_RTC_GetAlarmTime(LPC_RTC_T *pRTC, IP_RTC_TIMEINDEX_T Timetype)
164 {
165 return IP_RTC_GetAlarmTime(pRTC, Timetype);
166 }
167
174 STATIC INLINE void Chip_RTC_SetFullAlarmTime(LPC_RTC_T *pRTC, IP_RTC_TIME_T *pFullTime)
175 {
176 IP_RTC_SetFullAlarmTime(pRTC, pFullTime);
177 }
178
185 STATIC INLINE void Chip_RTC_GetFullAlarmTime(LPC_RTC_T *pRTC, IP_RTC_TIME_T *pFullTime)
186 {
187 IP_RTC_GetFullAlarmTime(pRTC, pFullTime);
188 }
189
201 STATIC INLINE void Chip_REGFILE_Write(LPC_REGFILE_T *pRegFile, uint8_t index, uint32_t Value)
202 {
203 IP_REGFILE_Write(pRegFile, index, Value);
204 }
205
216 STATIC INLINE uint32_t Chip_REGFILE_Read(LPC_REGFILE_T *pRegFile, uint8_t index)
217 {
218 return IP_REGFILE_Read(pRegFile, index);
219 }
220
229 STATIC INLINE void Chip_RTC_CalibCounterCmd(LPC_RTC_T *pRTC, FunctionalState NewState)
230 {
231 IP_RTC_CalibCounterCmd(pRTC, NewState);
232 }
233
243 STATIC INLINE void Chip_RTC_CalibConfig(LPC_RTC_T *pRTC, uint32_t CalibValue, uint8_t CalibDir)
244 {
245 IP_RTC_CalibConfig(pRTC, CalibValue, CalibDir);
246 }
247
256 STATIC INLINE void Chip_RTC_ClearIntPending(LPC_RTC_T *pRTC, uint32_t IntType)
257 {
258 IP_RTC_ClearIntPending(pRTC, IntType);
259 }
260
269 STATIC INLINE IntStatus Chip_RTC_GetIntPending(LPC_RTC_T *pRTC, uint32_t IntType)
270 {
271 return IP_RTC_GetIntPending(pRTC, IntType);
272 }
273
274 #if RTC_EV_SUPPORT
275
285 STATIC INLINE void Chip_RTC_EV_Config(LPC_RTC_T *pRTC, RTC_EV_CHANNEL_T ch, uint32_t flag)
286 {
287 IP_RTC_EV_Config(pRTC, ch, flag);
288 }
289
296 STATIC INLINE void Chip_RTC_EV_SetMode(LPC_RTC_T *pRTC, RTC_EV_MODE_T mode)
297 {
298 IP_RTC_EV_SetMode(pRTC, mode);
299 }
300
306 STATIC INLINE uint8_t Chip_RTC_EV_GetStatus(LPC_RTC_T *pRTC)
307 {
308 return IP_RTC_EV_GetStatus(pRTC);
309 }
310
317 STATIC INLINE void Chip_RTC_EV_ClearStatus(LPC_RTC_T *pRTC, uint32_t flag)
318 {
319 IP_RTC_EV_ClearStatus(pRTC, flag);
320 }
321
328 STATIC INLINE FlagStatus Chip_RTC_EV_GetChannelStatus(LPC_RTC_T *pRTC, RTC_EV_CHANNEL_T ch)
329 {
330 return IP_RTC_EV_GetChannelStatus(pRTC, ch);
331 }
332
339 STATIC INLINE void Chip_RTC_EV_ClearChannelStatus(LPC_RTC_T *pRTC, RTC_EV_CHANNEL_T ch)
340 {
341 IP_RTC_EV_ClearChannelStatus(pRTC, ch);
342 }
343
350 STATIC INLINE uint8_t Chip_RTC_EV_GetCounter(LPC_RTC_T *pRTC, RTC_EV_CHANNEL_T ch)
351 {
352 return IP_RTC_EV_GetCounter(pRTC, ch);
353 }
354
362 STATIC INLINE void Chip_RTC_EV_GetFirstTimeStamp(LPC_RTC_T *pRTC, RTC_EV_CHANNEL_T ch, RTC_EV_TIMESTAMP_T *pTimeStamp)
363 {
364 IP_RTC_EV_GetFirstTimeStamp(pRTC, ch, pTimeStamp);
365 }
366
374 STATIC INLINE void Chip_RTC_EV_GetLastTimeStamp(LPC_RTC_T *pRTC, RTC_EV_CHANNEL_T ch, RTC_EV_TIMESTAMP_T *pTimeStamp)
375 {
376 IP_RTC_EV_GetLastTimeStamp(pRTC, ch, pTimeStamp);
377 }
378
379 #endif /*RTC_EV_SUPPORT*/
380
386 void Chip_RTC_Init(LPC_RTC_T *pRTC);
387
393 void Chip_RTC_DeInit(LPC_RTC_T *pRTC);
394
399 #ifdef __cplusplus
400 }
401 #endif
402
403 #endif /* __RTC_17XX_40XX_H_ */