Instructions to erase and load Seanav software v1.30 into the SEADeViL System

· The batch file "hadal130.BAT" will erase and load v1.30 into T24 SEADeViL part number K600A377-36

NOTE: The batch file will only work with the Seadevil K600A377-36

DO NOT USE WITH ANY OTHER SYSTEMS. 

Equipment Required:

a. Computer with RS232 port (COM1)

b. Operating software: Win98 or below (DOS 6.22 preferred)

c. Power supply and associated cables

The procedure of loading is as follows:

1. Boot the computer into DOS prompt.

2. Switch to Drive and directory containing the batch file.

3. Connect PC com1 to the SEADeViL J3 as follows:  


4. With the SEADeViL power off, Type desired batch file at the dos prompt             and depress the ENTER key.

5. Follow onscreen instructions and power up the SEADeViL when prompted to "Reset target system now ..."

6. The software will burn the new files and then exit the program by displaying the following on the screen:


7. Power off the SEADeViL.

8. Using PCDAS (or equivalent), verify that the OCP Version is 17010130 and the OCP Checksum is “7BB0EB6C”  (This information is transmitted in System Status message (ID 27, subID 6, Data bytes D5-D8 & D9-D12)

Tx    J3-6  to COM1-2 (Pc_in)


Rx    J3-2  to COM1-3 (pc_out)


GND   J3-8  to COM1-5 (Sig GND)





or Connect the RS232/Rs422 converter to J2. (Ref. Diagram Below)








Rx (pc_in)  __   Tx (-)            


	 COM1-2  --------------|  |---------------- J2-6


       		Tx (pc_out)|  |  Tx (+)            


	 COM1-3  --------------|  |---------------- J2-2


	            Sig GND    |  |  Rx (-)            


	 COM1-5  --------------|  |---------------- J2-7


	                       |  |  Rx (+)            


	                       |__|---------------- J2-3


	                                            


	                     232 / 422


	                     Converter








          BOOT232            V105 R4                  		090617





          Terminated








Power off the system





The batch file has successfully completed the software load.
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