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1. OUTLINE
These specifications define the PC mode as the situation in which the digital camera D700 (hereinafter referred to as the camera) and the PC are connected by the USB and the USB communication has been established.

Although the USB connector of the camera is also used for the connection with the wireless transmitter or the printer that supports PictBridge, this situation is not included in the PC mode.

The PC mode has the following connection mode.

· MTP (PTP) connection (camera control function from the PC)

In addition, the PC mode has the following modes depending on the usage condition.

· PC camera mode

· PC host mode

2. SPECIFICATIONS FOR EACH CONNECTION MODE
For the operation and the detailed specifications in the PC mode, refer to the specifications below.

· MTP (PTP):  
D700 USB Still Capture Device Media Transfer Protocol (MTP) Specifications

3. PROCESS FLOW IN CONNECTING USB
This chapter describes the behavior of the camera when it is connected with the PC using USB cable.

3.1. USB Signal Lines
USB has four signal lines.
1) V BUS

2) D+

3) D-

4) GND

- The condition for the camera to detect USB connection

   5V current is supplied on V BUS line of the camera.

- The condition for the PC to detect USB connection

   D+ line is pulled up.

3.2. Connection with the PC and the Camera
In this section, the flowchart of the process on the camera is described when connecting with the PC by using USB.


[image: image1.emf]
Figure 1. Flowchart of the process on the camera when connecting with the PC

3.3. Setup USB between the PC and the Camera
The camera sends the information of USB to the PC after getting the specific command from the PC.


[image: image2.emf]
Figure 2. Setup USB between the PC and the camera in the PTP mode
4. SHIFTING TO THE PC MODE
When the USB cable that is connected to the PC is connected to the USB connector in the camera, the camera automatically enters the PC mode and the PC mode is always set during the connection.  When the USB connection is released, the PC mode is also released.

The timing when shifting to the PC mode changes depending on the processing status of the camera.

Shifts to the PC mode after the processing is completed

· During shooting (AF operation, release operation)

· During the preview operation
· During access to the card

Aborts the processing and then shifts to the PC mode

· During the self-timer operation
· Mirror-up shooting waiting status (during the mirror-up)
· Preset release waiting status

· Dust reference release waiting status
· During multi-exposure operation

· During Live view
· During the TFT display (menu display, playback display)

· Formatting waiting status
However, the camera does not shift to the PC mode in the cases below.

· While the cleaning mode is being set or executed

· While the interval-timer shooting is being set or executed

· During the firmware updating

· Battery level “Operation disabled status”
· During the power interruption (during the power SW-OFF operation in the camera)

5. PC HOST MODE AND PC CAMERA MODE
The camera has the following modes depending on the connection setting and the processing status of the camera.

· PC camera mode

· PC host mode

5.1. PC Host Mode

When the host mode switching request from the PC is made or the command processing from the PC is executed, the mode is switched to the PC host mode automatically.  For the automatic switching by the command processing, the mode is switched to the PC camera mode automatically after the processing is completed.

In the PC host mode, the operation of the buttons/dials of the camera becomes invalid and the operation from the PC becomes valid.  However, the operation of the power switch is excluded.

The operation section status immediately after changing to the PC host mode becomes the status that is set on the camera.

Because the operation of the buttons/dials is prohibited in the PC host mode, the setting of the menu items is also performed by operating the PC.

5.2. PC Camera Mode

The PC camera mode is set by the PC camera mode switching request from the PC in the PC host mode.

The operation on the camera becomes valid and shooting by the shutter-release button of the camera is enabled (whether the captured image data is recorded to the card or transferred to the PC is described later).  Only the acquisition of the operation section status is possible on the PC.

The control other than the operation section of the camera (such as the menu items) can be operated by the PC as well.

When the operation section is controlled by the PC in the PC host mode and the PC host mode is switched to the PC camera mode, the control status by the PC is canceled and the information of the buttons/dials on the camera is used.

5.3. Display Section of the Camera in the PC Mode

The display conditions of the display in the finder/the top display panel/the back display panel change depending on the connection mode and the recording destination setting in the PC mode.

Each display condition is shown below.

	PC mode
	Recording destination
	In the finder
	Top display
	Back display

	PC host mode
	Card
	PC display only
	PC display only
	PC display only

	
	PC
	PC display only
	PC display only
	PC display only

	PC camera mode
	Card
	Normal display
	Normal display
	Normal display

	
	PC
	Normal display
	The number of images that can be captured: PC display

Other: Normal display
	Normal display


6. OPERATION AND SETTING DEPENDING ON THE PC MODE STATUS
The camera operation and its setting method differ depending on the PC mode state (camera as a single unit, in the PC camera mode, or in the PC host mode).  The differences are shown below.

6.1. Validity of Operation of Buttons/Dials

Whether the operation of the buttons/dials in the PC mode is valid or not is shown below.

	Name of the operation section
	PC camera mode
	PC host mode

	Power switch
	Valid
	Valid

	Shutter-release button
	Valid
	Invalid

	Main command dial
	Valid
	Invalid

	Sub-command dial
	Valid
	Invalid

	AF actuation button
	Valid
	Invalid

	Exposure mode button
	Valid
	Invalid

	Exposure compensation button
	Valid
	Invalid

	Metering selector
	Valid
	Invalid

	Release mode dial
	Valid
	Invalid

	Sync mode button
	Valid
	Invalid

	Function button
	Valid
	Invalid

	Preview button
	Valid
	Invalid

	AE-L/AF-L button
	Valid
	Invalid

	Focus-mode selector
	Valid
	Invalid

	Multi-selector
	Valid
	Invalid

	Multi-selector center button
	Valid
	Invalid

	Focus area lock lever
	Valid
	Invalid

	AF area mode selection dial
	Valid
	Invalid

	Playback button
	Valid
	Invalid

	Delete button
	Valid
	Invalid

	Menu button
	Valid
	Invalid

	Protect button/Help button
	Valid
	Invalid

	Reduce button/Thumbnail button
	Valid
	Invalid

	Enlarge button
	Valid
	Invalid

	ISO sensitivity button
	Valid
	Invalid

	Image quality mode button
	Valid
	Invalid

	White balance button
	Valid
	Invalid

	Info button
	Valid
	Invalid

	Format (Exposure button + Delete button)
	Invalid
	Invalid


6.2. Possibility of Menu Item Setting

Whether the menu item can be set from the camera in the PC mode is described below.

When the item is changed from the PC while the menu item is being changed in the camera, the light of the nemu screen is turned off and the set item from the PC is reflected.

6.2.1. Playback menu

(Yes: Operation is enabled.  C: Some limitation exists.  No: Operation is disabled.)

	Menu item
	PC camera mode
	PC host mode

	Playback nemu (all items) (*1)
	No
	No


*1. The selection of the playback menu from the menu itself is disabled.

6.2.2. Shooting menu

(Yes: Operation is enabled.  C: Some limitation exists.  No: Operation is disabled.)

	Menu item
	PC camera mode
	PC host mode

	Shooting menu change
	Yes
	No

	Shooting menu reset
	Yes
	No

	Recording folder setting
	No
	No

	File name setting
	Yes
	No

	Image quality mode
	Yes
	No

	Image size
	Yes
	No

	Capturing range
	Yes
	No

	JPEG compression
	Yes
	No

	RAW recording
	Yes
	No

	White balance
	Yes
	No

	Picture Control
	Yes
	No

	Custom Picture Control
	Yes
	No

	Color space
	Yes
	No

	Active D-Lighting
	Yes
	No

	Vignette Control
	Yes
	No

	Long-time noise reduction
	Yes
	No

	High-sensitivity noise reduction
	Yes
	No

	ISO sensitivity setting
	Yes
	No

	Live view
	Yes
	No

	Multi-exposure
	No
	No

	Interval-timer shooting
	No
	No


6.2.3. Custom menu

(Yes: Operation is enabled.  C: Some limitation exists.  No: Operation is disabled.)

	Menu item
	PC camera mode
	PC host mode

	Custom menu (all items)
	Yes
	No


6.2.4. Setup menu

(Yes: Operation is enabled.  C: Some limitation exists.  No: Operation is disabled.)

	Menu item
	PC camera mode
	PC host mode

	Formatting the card (Format)
	No
	No

	Brightness of the liquid crystal monitor
	Yes
	No

	Image sensor cleaning
	Yes
	No

	Cleaning mirror-up
	No
	No

	Video output
	Yes
	No

	HDMI
	Yes
	No

	World time
	Yes
	No

	Language
	Yes
	No

	Image comment
	Yes
	No

	Recording the lengthwise/widthwise position information
	Yes
	No

	Image dust off data acquisition
	Yes
	No

	Battery check
	Yes
	No

	Wireless transmitter
	No
	No

	Image reliability detection function
	Yes
	No

	Copyright information
	Yes
	No

	Saving/Loading camera setting
	Yes
	No

	GPS
	Yes
	No

	Level display
	Yes
	No

	Manual setting for lens information
	Yes
	No

	AF fine adjustment
	Yes
	No

	Firmware version
	C (*1)
	No


*1. The firmware version upgrade is disabled.
6.2.5. Image editing menu

(Yes: Operation is enabled.  C: Some limitation exists.  No: Operation is disabled.)

	Menu item
	PC camera mode
	PC host mode

	Image editing menu (all items) (*1)
	No
	No


*1. The selection of the image editing menu from the menu itself is disabled.

6.2.6. My menu

This is consistent with the contents of sections 6.2.1 to 6.2.5.

7. DIFFERENCES FROM THE OPERATIONS ON THE CAMERA
Available operations on the camera in the PC mode are shown below.
(Yes: Conforms to the camera.  No: Operation is disabled.)

	Action by operating the camera
	PC camera mode
	PC host mode

	One-frame shooting
	Yes
	No

	Continuous shooting
	Yes
	No

	Self-timer shooting
	Yes
	No

	Moirror-up shooting
	Yes
	No

	Bulb shooting
	Yes
	No

	Interval-timer shooting
	Yes
	No

	Preset WB measurement
	Yes
	No

	Image dust off data acquisition
	Yes
	No

	AF operation
	Yes
	No

	Live view
	No
	No

	Two-button reset
	Yes
	No

	Image playback/Image deletion
	No
	No

	Formatting
	No
	No


The differences from the operations on the camera when operating from the PC in the PC mode are shown below.

(Yes: Conforms to the camera. C: There is some difference. No: Operation is disabled.)
	Action by operating the camera
	PC camera mode
	PC host mode

	One-frame shooting
	Yes (*1)
	Yes

	Continuous shooting
	Yes (*1, *2)
	Yes (*2)

	Self-timer shooting
	No
	No

	Moirror-up shooting
	No
	No

	Bulb shooting
	No
	No

	Interval-timer shooting
	No
	No

	Preset WB measurement
	C (*1)
	C

	Image dust off data acquisition
	C (*1)
	C

	AF operation
	C (*1)
	C

	Shutter speed setting
	C (*1)
	C

	Live view
	No
	C

	Image playback/Image deletion
	Yes (*3)
	Yes (*3)

	Formatting
	No
	No


*1. When the operation from the PC is performed, the mode is changed to the PC host mode temporarily.

*2. When the number of images that can be captured continuously is not set from the PC, the number of images for continuous shot is 1.

*3. The data can be played back and deleted on the PC, while it cannot be played back and deleted on the camera TFT.

7.1. Shooting Operation

The differences in the shooting operation are shown below.

7.1.1. Image data recording

For the image data captured by the shooting operation in the PC mode, the recording destination is changed by “Recording destination setting” and the “Release command” from the PC.

The recording destination setting can be changed by the MTP (PTP) command.

There are two kinds of release commands; MTP (PTP) standard command and vendor-defined command.

While shooting operation by the release command is being performed (from the release command notification to the image recording), the operation is performed in the PC host mode.

The recording destination setting and the recording destination of the image data by the release command are shown below.

	Recording destination
	Shutter release button
	MTP (PTP) standard
	Vendor definition

	Card
	Records on the card
	Records on the card
	Transfers to the PC

	PC
	Transfers to the PC
	Records on the card
	Transfers to the PC


For the image data transfer to the PC, the camera notifies the PC by the event that the image data has been created and the image data is acquired by the image acquisition request from the PC that detects the event generation.  The operation is performed in the PC host mode between the release command issue and the image data acquisition completion.

7.1.2. The number of captured images depending on the release mode

The number of images that can be captured by the release mode dial of the camera or the release mode setting from the PC according to the shooting request from the PC is shown below.

	Release mode
	The number of images that can be captured
	Description

	One-frame shooting
	1
	-

	Continuous shooting
	1 to 46
	The default in the PC connection mode is 1.

The number of images that can be captured continuously is changed by the PC operation.

	Self-timer shooting
	1
	The self-timer function does not operate.

The shooting operation is treated as one-frame shooting.

	Mirror-up shooting
	-
	Shooting from the PC is disabled.


7.1.3. Bulb shooting
The bulb shooting is disabled because the “keep pressing the shutter-release button” situation cannot be reproduced by the command operation from the PC.

However, because the shutter-release button of the camera is valid in the camera mode, the bulb setting is also possible for the shutter speed setting.

7.1.4. Interval-timer shooting
The interval-timer shooting is disabled.

7.1.5. Preset WB measurement

The preset WB measurement in the camera continues if the measurement fails depending on the exposure condition or the like.  However, if the measurement fails when the measurement is performed by operating the PC, the measurement failure is notified to the PC and the operation is terminated.

In addition, the measurement is possible even if the WB is other than the preset.
The operation is performed in the PC host mode during the operation by the preset WB measurement command.

7.1.6. Image dust off data acquisition

The image dust off data acquisition in the camera continues if the acquisition fails depending on the exposure condition or the like.  However, if the acquisition fails when the data is acquired by operating the PC, the acquisition failure is notified to the PC and the operation is terminated.

When the data acquisition succeeds, the data is treated thereafter in the same manner as that of the image data captured normally.

The operation is performed in the PC host mode during the operation by the image dust off data acquisition command.

7.2. AF Operation

For the AF driving, the operation conforms to that of the camera as a single unit.

The operation is performed in the PC host mode during shooting operation by the AF driving command.

However, when the release mode is set to the continuous shooting, there should be the following limitations depending on the auto focus setting of the custom menu.

	Focus mode
	Priority mode
	Description

	MF
	-
	(No AF operation)

	AF-S
	Focus priority
	Conforms to the camera operation.

	
	Release priority
	Conforms to the camera operation.

	AF-C
	Release priority
	Conforms to the camera operation.

	
	Focus priority
	Operates only when the first image is captured.  For the second and later images, the operation is the same as that of the release priority.


7.3. Shutter Speed Setting

In the PC, the normal shutter speed and the synchronization speed (for x speed) are treated as identical.

The synchronization speed cannot be set from the PC.  If the shutter speed that is the same as the synchronization speed is set from the PC when the synchronization speed is set in the camera, the synchronization speed setting is released and it is treated as the normal shutter speed.

7.4. Live View
In the PC mode, Live view from the camera is prohibited.

In the PC host mode, Live view is enabled by the MTP (PTP) command.

At this time, the Live view display is performed on the PC.

7.5. Card Operation

The differences in the card operation are described below.

7.5.1. Image playback/Image deletion

Image data playback and deletion in the camera is disabled in order to coordinate the image data information of the camera with that of the PC.

7.5.2. Formatting

In the PC mode, formatting from the camera is prohibited both by using the nemu and by using the two buttons.

For the formatting from the PC, the card formatting by the format command is enabled.

7.6. Auto Meter-off Delay
The Auto meter-off delay is set to “No limit”.

If the images are captured and the USB cable is disconnected while the image data is being transferred when the recording destination is the PC, the remaining image data is transferred by connecting the USB again.  Therefore, if there is any image data that has not been transferred to the PC yet in the camera, the Auto meter-off delay is left unlimited even if the PC mode is released.

8. SUPPLEMENTARY MATTERS
The supplementary matters are described below.

8.1. Battery Voltage Drop during Continuous Shooting
When the camera is operated by using the battery, there is a possibility that the battery voltage may drop and become on the shooting prohibition level during continuous shooting.  In this case, shooting is terminated when the voltage drop is detected even if the number of captured images does not reach the number of images that can be captured continuously.  When the recording destination is the PC, the image data is transferred to the PC without a break.

However, the connection with the USB may not be established depending on the battery voltage drop level.  In this case, the image data is not transferred normally because the PC recognizes that the camera is disconnected.
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