Link Controller Unit FPGA revision register bits
	Bits
	Description

	15:12
	Revision Number

	11
	1 = dual MPA, 0 = non dual MPA

	10
	1 = RS232 IOP wet downlink, 0 = 80 Mb LVDS IOP wet downlink

	9
	1 = BITE enabled, 0 = BITE disabled

	8
	Reserved

	7 
	1 = 125 MHz beam former bus base clock, 0 = 80 MHz beam former bus base clock

	6:4
	Beam former bus clock (for bit 7 = 1) 100 = 62.5 MHz, (for bit 7 = 0) 001 = 10MHz, 010 = 20MHz, 100 = 40 MHz

	3
	1 = RX dual uplink, 0 = RX single uplink

	2
	1 = PHY uplink and downlink, 0 = PHY disabled

	1
	1 = AUV (bf connected), 0 = ROV (bf unconnected)

	0
	1 = 80Mb coax uplink, 0 = coax disabled


