Release code for Link Module for GDC YS2000 
Rev 8250
Add destination address modification from broadcast (E0 hex) to IOPW (25 hex) for time stamp packets (type 80 hex) headed for the LCU

Condition LNKLOCKn led with slow speed bit to prevent chatter
Following were in Rev 8240 already

Added uplink data capture for DSP with read register at 3

Bit15:10 is opposite polarity of valid

Bit 9 is valid (1 is valid)

Bit 8 is first byte of packet

Bit 7:0 are the data bytes

Pushed PHY interface signals to IOB

